*********************************************

Avago Technologies MegaRAID Firmware Release 

*********************************************



**************************************************************************************************************************
***********PLEASE READ IF USING CACHEVAULT OPTION ON ANY OF THESE MEGARAID CONTROLLERS ***********************************
**************************************************************************************************************************
If using Cachevault option on your MegaRAID Controller, the Gas Gauge component on your controller should also be updated.
Please refer to the "S11253_Gas_Gauge_FW_Update_Instructions_SAS3108_SEN_v1.0" pdf included in this package.
If there are any questions regarding Gas Gauge upgrade, please contact Technical Support or your Field Support.
**************************************************************************************************************************
**************************************************************************************************************************



**************************************************************************************************************************
***********PLEASE READ BEFORE DOWNGRADING FROM THIS FIRMWARE VERSION TO ANY PRIOR FIRMWARE VERSION************************
**************************************************************************************************************************
Online Firmware Update should not be performed when downgrading from this release to a release prior to the first MR 6.6 
release: Firmware Package:24.7.0-0026 (MR 6.6), Firmware 4.270.00-3972.  
Please refer to the 240_VD_Feature_Limitations_Known_Issues_Addendum_v1.0.pdf document included with this package for 
additional details.
**************************************************************************************************************************
**************************************************************************************************************************




Release date: 12/30/15

====================== 
Supported Controllers:
======================

MegaRAID SAS 9361-8i
MegaRAID SAS 9361-4i
MegaRAID SAS 9380-8e
MegaRAID SAS 9380-4i4e

Component:
=========
SAS MegaRAID Firmware Release for MegaRAID Controllers
Release date: 12/30/15


Version Numbers:	
===============
Current Package Details:
Firmware Package:24.12.0-0020 (MR 6.10)
Firmware 4.620.00-5026
ROMENV 1.09
BootBlock 3.07.00.00-0003
NVDATA  3.1511.00-0004
UEFI_Driver 0x06130200(signed)
Hii 03.19.07.00(signed)
FCODE 4.17.08.00
BIOS 6.30.03.0
Ctrl-R 5.15-0700
PCLI 1.07.05

Previous Package Details:
Firmware Package:24.10.0-0020 (MR 6.9 P1)
Firmware 4.600.00-4907
ROMENV 1.09
BootBlock 3.07.00.00-0003
NVDATA  3.1508.00-0009
UEFI_Driver 0x06110200(signed)
Hii 03.17.14.01(signed)
FCODE 4.17.08.00
BIOS 6.28.04.0
Ctrl-R 5.13-1101
PCLI 1.07.05


Bug Fixes and Enhancements:
===========================
Firmware:
SCGCQ00856175 - (Closed) - MSM does not have PD locate option if you are connected in Multipath mode with DES300SAS enclosure to Intruder controller.
SCGCQ00860613 - (Closed) - Dirty Cache LED not behaving as expected
SCGCQ00870476 - (Closed) - Intruder(Armstrong)_MR6.9-Pre-Alpha_AmberLED Not Working
SCGCQ00873336 - (Closed) - VD's do not switch back to Write Back mode after the successful completion of learn cycle.
SCGCQ00878232 - (Closed) - Not able to inject ECC L2 errors(call L2InjectEccErrors 400000) with latest Intruder firmware but OK with old release FW 4467
SCGCQ00881128 - (Closed) - MonTask: line 245 in file ../../raid/1078int.c when run heavy I/O with different RAID level + CC and trigger controller reset
SCGCQ00883007 - (Closed) - System does not wait for cache off load to complete during BBU relearn, VDs in WT, not expected per test case
SCGCQ00887019 - (Closed) - MonTask: line 2735 in file ../../ssd/ssd_cache_fw.c when inject error in a loop
SCGCQ00889794 - (Closed) - ONFI already armed message is seen at initialization
SCGCQ00890342 - (Closed) - Read Eye failure messages are seen during reset
SCGCQ00894344 - (Closed) - Patrol read doesn't resume after power cycle.
SCGCQ00894610 - (Closed) - Montask observed while trying to create a CCVD using SLT : MonTask: line 1413 in file ../../raid/config.c
SCGCQ00895577 - (Closed) - Firmware does not log controller property change event for enabling/disabling 240VD feature
SCGCQ00895689 - (Closed) - After reboot imported 4K drive R0 is not visible
SCGCQ00897147 - (Closed) - Updating intruder firmware package to 8 disables cachecade functionality.
SCGCQ00897406 - (Closed) - Sanity check for handling the cases where event length comes up as zero/ rPtr goes beyond iptr
SCGCQ00897700 - (Closed) - Intruder: The firmware retires the timed out IOs for three times instead of the reduced count to two tries.
SCGCQ00898631 - (Closed) - SCGCQ00475165 PR is not proted to 6.9 Intruder stream.
SCGCQ00898652 - (Closed) - DMA completion interrupt incorrectly coded as EH
SCGCQ00898686 - (Closed) - Intruder - Severe performance issue with Write workloads - SATA HDD RAID modes
SCGCQ00898690 - (Closed) - FW messages corrupt while restore dram contents from flash.
SCGCQ00899911 - (Closed) - Drive negotiated link rate didn't response the correct status after hotplug test
SCGCQ00903988 - (Closed) - Hit Continue Error Message ' ER DECREMENTER exception: sf=MER DECREMENTER exception: ' and System Hang during I/O and
SCGCQ00904103 - (Closed) - Pull the chain frame for SYSTEM PDs in MptHostCmdPreProcess()
SCGCQ00904982 - (Closed) - iMR Fatal firmware error: Line 245 in ../../raid/1078int.c
SCGCQ00905416 - (Closed) - on creating 240VD and rebooting the server, FW breaks into montask.
SCGCQ00905628 - (Closed) - Pinned cache is not getting discarded correctly.
SCGCQ00905864 - (Closed) - MR6.10: Hibernating the Windows 10 machine leads to iMR FW crash at line 229 in file ../../raid/mtask.c
SCGCQ00906949 - (Closed) - Firmware Updrade/Downgrade issue due to incorrect flash offset for seondary Image in FW
SCGCQ00907430 - (Closed) - Intruder Armstrong : MonTask: line 1286 in file ../../raid/1078dma.c when run testIO
SCGCQ00910124 - (Closed) - as been observed that the firmware retires the FPIO timed out IOs for 3 times instead of the reduced count to
SCGCQ00910723 - (Closed) - Fixing compilation issues for Intruder 6.9 Int stream.
SCGCQ00912235 - (Closed) - Locate and Fault LED do not work on remote LED boards for drives connected to ports 4-15
SCGCQ00914274 - (Closed) - MR_6.10 : On removing a redundant path with IO on JBOD's , result to "LMID HS-FIFO Error 0x8"
SCGCQ00914343 - (Closed) - MR 6.10 : Storcli shows improper ScapBatVersionNO through /c0/cv show all
SCGCQ00914723 - (Closed) - Defect to check in code for AIs from code review
SCGCQ00915073 - (Closed) - OFU fails while upgrading iMR FW from MR 6.9 to MR 6.10
SCGCQ00915081 - (Closed) - MR 6.10: iMR FW: Chainmid handling for Failed JBOD IO's in iMR
SCGCQ00921714 - (Closed) - Clearing NVRAM results in ONFI picking up offload image from default location (block 0)
SCGCQ00922858 - (Closed) - SRAM_FIXED changes after Rebase from 6.10_Int
SCGCQ00924986 - (Closed) - Controller became unresponsive after hitting OCM error
SCGCQ00925887 - (Closed) - Pinned cache is lost with reboot with no further dirty cache lines
SCGCQ00926277 - (Closed) - Difference of Code between the Defect Fix and Cset - Code Review AI
SCGCQ00927173 - (Closed) - unnecessary update of PD map in DM_ProcessDevWaitQueue()
SCGCQ00928150 - (Closed) - On performing a stop drive erase operation from application results to FW hang
SCGCQ00930044 - (Closed) - MR: on enabling cachecade and setting ldlimit to max,cachecade vd creation fails with improper error message
SCGCQ00930569 - (Closed) - Defect to fix AIs from group code review
SCGCQ00936693 - (Closed) - Queue depth throttling changes to support OFU with OCR
SCGCQ00937487 - (Closed) - Avalon:Powering ON the Workstation from S3 Sleep leads to iMR FW crash
SCGCQ00937572 - (Closed) - iMR-6.10 alpha: Observing prints "C0:Index 0098 allocated from pool 3 " continuously with 12G Encl and SATA drives
SCGCQ00941531 - (Closed) - MR6.10Beta:MonTaskline 1281 in file /raid/1078dma.c on running enclosure cable pull push with Source VD's associated to CC VD
SCGCQ00941536 - (Closed) - MR 6.10:Remove code due to merge issue
SCGCQ00942547 - (Closed) - Disabling SATA HOQ for iMR controllers
SCGCQ00948257 - (Closed) - SVT: MR6.10: Driver panic and firmware locks up during Medium Error testing
SCGCQ00948466 - (Closed) - VDs don't revert back to WB state once the Controller Pinned Cache is destaged
SCGCQ00952627 - (Closed) - FW crashes while running full initialization on VDs with LDBBM entries created on running consistency check
SCGCQ00976741 - (Closed) - SES Error observed when Dell13G BP is connected
SCGCQ00869639 - (Closed) - Misleading message because of missing return statement
SCGCQ00869653 - (Closed) - Re-order the check for ongoing offload during power restore while offload in progress.
SCGCQ00871785 - (Closed) - Intruder PA - Numerous performance regressions with 8 SAS HDDs in WB
SCGCQ00875231 - (Closed) - Intruder 6.9 code compile fails for Ring buffer.
SCGCQ00878251 - (Closed) - Breakout led is not getting on.
SCGCQ00885589 - (Closed) - Addressing code inconsistency caused after merging Intruder and Invader code.
SCGCQ00887068 - (Closed) - Controller hang and restart multiple times when running IO and start OCR - Only when SSC enabled on the VD's
SCGCQ00890729 - (Closed) - MonTask: line 2056 in file ../../raid/flex.c when reboot server with multiple background operation: CC/Rebuild/Copyback/Recon
SCGCQ00894124 - (Closed) - MR_6.9_Intruder: Locate LED functionlaity is not proper on a PD in power save mode.
SCGCQ00895142 - (Closed) - Warm reset sequence with Intruder A1 results in intermittent ONFI bringup failure
SCGCQ00898799 - (Closed) - Firmware crashed while running I/Os on fast path volumes with SSD caching
SCGCQ00899907 - (Closed) - Running PCIECV Application causes system to halt and bluescreen
SCGCQ00900601 - (Closed) - MR6.10:Importing 240 VD foreign configuration leads to FW Crash
SCGCQ00904899 - (Closed) - Storcli throws error while performing /c0/vx show all after full Init on R1 VD created by SSD drives.
SCGCQ00905119 - (Closed) - Defect to check in code changes for static analysis tool reported bugs.
SCGCQ00905578 - (Closed) - Addressing group code review issues.
SCGCQ00905633 - (Closed) - Firmware is breaking when pinned cache is present and supercap is absent.
SCGCQ00914736 - (Closed) - As been observed that the firmware retires the FPIO timed out IOs for 3 times instead of the reduced co
SCGCQ00915343 - (Waiting_Info) - MSM Show Port Connector Nullx0 When Connect to Port 4-7 & Port 5-8 On iMR/Cutlass Intruder
SCGCQ00917307 - (Closed) - MR6.10_FW : Configuration creation on Controller fails after creation of a CC VD followed by JBOD creation.
SCGCQ00918195 - (Closed) - Pinned cache during OCR results in an offload operation without subsequent dirty cache.
SCGCQ00922239 - (Closed) - Enable read and write cache of ONFI operations
SCGCQ00922776 - (Closed) - Clearing of link equalization from trap isr is not required for Intruder.
SCGCQ00923289 - (Closed) - Cable pull from controller during target reset on JBOD resulted into data TLB error
SCGCQ00928333 - (Closed) - Controller heart beat disappeared after performing a cable pull
SCGCQ00930846 - (Closed) - Dev Defect : vSAN iMR Queue Depth change to 928(Long term) - Part 3
SCGCQ00931262 - (Resolved) - Compilation Broken after Rebase of 6.10_Intruder_Int from Sas3_Int
SCGCQ00934196 - (Closed) - MR-Intruder: MegaRAID controller hangs/crashes while importing the drive back to the RAID-0 CacheCade VD
SCGCQ00934856 - (Closed) - Instruction TLB Error in iMR.
SCGCQ00866272 - (Closed) - Not able to import secure config from Invader iMR/MR to Intruder controller
SCGCQ00869681 - (Closed) - MR6.9 Invader : PD locate LED goes off after second ESM is plugged in a multipath cable breaker test
SCGCQ00883636 - (Closed) - Locate VD ( across enclosure ) LED is not continue blinking on first casacading enclosure but OK on second enclosure
SCGCQ00886992 - (Closed) - add code to ensure that (SCGCQ00885631) changes doesn;t effect invader.
SCGCQ00896497 - (Closed) - Dev Defect : vSAN iMR Queue Depth change to 928(Long term) - Part 2
SCGCQ00897457 - (Closed) - Development defect to find the difference in behaviour between nmake and make builds.
SCGCQ00902938 - (Closed) - MR6.10 Montask when loading Intel Cutlass drivers
SCGCQ00905085 - (Closed) - ONFI debug message to be masked.
SCGCQ00906846 - (Closed) - CacheCade disassociation progress status missing for some source VDs
SCGCQ00910006 - (Closed) - MR6.10: Assert at line 1181 mpthostcmd.c issueFlag == TRUE),"MptProcessHostIO: Caller does not exepect this IO to be queued
SCGCQ00911849 - (Closed) - Option ROM would not post when cache offload in interrupted by applying power to the system
SCGCQ00914751 - (Closed) - Applications show incorrect value for Max Parallel Commands filed of controller information with iMR controllers
SCGCQ00915088 - (Closed) - Issue ABORT TASK and ABORT TASK SET to SATA device instead of failing them as unsupported
SCGCQ00917523 - (Closed) - FW binray built with PLDEBUG enabled FW results in program exception
SCGCQ00919229 - (Closed) - In drive/multipath removal scenario, update PD map and RAID map appropriately
SCGCQ00924335 - (Closed) - Mask PEPPQLockUp Error from PCI engine
SCGCQ00930862 - (Closed) - Error "Bad symbol name was entered or symbol table is not available" on MegaMon command "ei SCapWBThreshold 0xffff"
SCGCQ00930917 - (Closed) - Invader 6.10 : OFU fails during downgrade from 240 VD stream to non 240 VD stream
SCGCQ00936617 - (Closed) - FW keep on printing "DM_EnableFastPathOnDevice :: FP enabled on devhandle" , even though FP is enabled
SCGCQ00937617 - (Closed) - ONFI good blocks are falsely marked as bad, resulting in FW prematurely rejecting ONFI module.
SCGCQ00887428 - (Closed) - Cannot start rebuild for degrade cachecade VDs after an overnight heavy IO run
SCGCQ00891316 - (Closed) - Fix compilation issue
SCGCQ00893564 - (Closed) - Boot message missing in case bad blocks exceed limit
SCGCQ00900689 - (Closed) - Issue was caused by ECC checks on unscrubbed areas of DRAM.
SCGCQ00907658 - (Closed) - LUID gets changed during foreing import from non-240VD FW to 240VD FW
SCGCQ00915078 - (Closed) - iMR - Lmid Queueing in checkFwIoDescList() needs to be added
SCGCQ00915092 - (Closed) - iMR 6.10 Alpha:MonTask: line 1279 in file ../../raid/1078dma.c on IMR card while booting with R0 DIFF VD on Ubuntu 14.10.
SCGCQ00915398 - (Closed) - Adapter reset occured with 240VDs configured and Ios
SCGCQ00915454 - (Closed) - MR 6.10: iMR_FW Add support to Enable Disable iMR Dual QD for avoiding OFU issues.
SCGCQ00921993 - (Closed) - Data TLB error found while reconstruction operation is running with target reset on JBOD
SCGCQ00870412 - (Closed) - Implemented the TiimerH changes as per requirement from the chip team
SCGCQ00915409 - (Closed) - MR 6.10: Handling LD I/Os on R0/R1 FP capable volume in presence of R5/R6 WT volume and running sequential write stream
SCGCQ00919945 - (Closed) - MR6.10_FW : CRC mismatch and invalid log event found while querying for Controller properties and learn cycle in parallel.
SCGCQ00925628 - (Closed) - fw hit 2108vI2o.c when doing the cable pull a few times.
SCGCQ00931895 - (Closed) - Disable region lock bypass for R1 volumes
SCGCQ00908982 - (Closed) - MR_6.10:iMR FW printing a message "MsgAlloc: No free messages, poolIndex=4" , while running IO on JB
SCGCQ00835036 - (Closed) - Intruder reference platform requires breakout connection for discrete LED
SCGCQ00942215 - (Closed) - MR 6.10: Integrating PL 10.25.03.00 to MR 6.10
SCGCQ00904581 - (Closed) - DDR Cache Line Reduction for Successful Cache Offload
SCGCQ00897917 - (Closed) - Dynamic Detection of Controller SAS Cores Phase-II
SCGCQ00895757 - (Closed) - Firmware Changes to bring up Shannon Controllers which has only one Channel between flash device and the Chip.
SCGCQ00892244 - (Closed) - Update to PL library 250.36
SCGCQ00888894 - (Implemented) - 3216 IMR: Add Support for OEM IMR Board
SCGCQ00883176 - (Closed) - Restart Patrol Read when interrupted by a consistency check for Invader
SCGCQ00881820 - (Closed) - Check in Intruder DDR3 library version 7
SCGCQ00879207 - (Closed) - Check in Intruder DDR3 library version 6
SCGCQ00871641 - (Closed) - Add support for new mem ref clock frequency on Armstrong evt2 boards.
SCGCQ00870867 - (Closed) - Update and Implement changes with regards to new ExtManPage42 and 43 introduced by PL to manage I2C devices handled;FW change
SCGCQ00869643 - (Closed) - Onfi debug command implemented to add blocks to the bad blocks table
SCGCQ00869640 - (Closed) - Implemented the new onfi debug commands and functionality
SCGCQ00686666 - (Closed) - MPI 2.6: Extend Task Management - Target Reset Method to include PCIe devices
SCGCQ00827088 - (Closed) - MPI 2.6: BootDeviceSelect and Host Boot changes for Ventura
SCGCQ00852827 - (Closed) - MPI 2.6: SRIOV support for PCIe devices
SCGCQ00852831 - (Closed) - MPI 2.6: Update Flash Signature.
SCGCQ00872169 - (Closed) - MPI 2.6: add new feature to control NVMe SGL format
SCGCQ00884740 - (Closed) - MPI 2.6: Additional PCIe Enumeration Event EnumerationStatus bit
SCGCQ00908248 - (Closed) - enabling the supportMoreThan16Phys bit in Ctrl Info
SCGCQ00896400 - (Closed) - Update to PL library 250.39
SCGCQ00894170 - (Closed) - Firmware changes required for ONFI bringup on Shannon Boards
SCGCQ00891675 - (Implemented) - Clamp the size of dram to 4GB and correct size for NAND limitaion
SCGCQ00890623 - (Implemented) - Dynamic detection of Number of SAS cores present in Intruder/Cutlass controller
SCGCQ00890192 - (Closed) - Integrate 09.250.05.00 MR PL with MR 6.10
SCGCQ00878767 - (Closed) - CPLD gpio changes
SCGCQ00890158 - (Closed) - MR build fails with out of memory for FW code when PLDEBUG enabled
SCGCQ00928293 - (Implemented) - Integrate Phase 10 MR PL (version 10.0.0.0) with MR 6.10
SCGCQ00885631 - (Closed) - A1 chip support added(A0 support retained.).
SCGCQ00931266 - (Implemented) - Support for making MR 6.10 Invader and Intruder releases from MR_6.10_Int Stream
SCGCQ00896536 - (Closed) - Change the flash clock speed to generation 5
SCGCQ00934167 - (Closed) - MR 6.10: Integrating PL(SCGCQ00933984) 10.00.02.00 to MR 
SCGCQ00888862 - (Port_Complete) - Increase iMR Queue Depth to 928(Long term)
SCGCQ00889209 - (Port_Complete) - Foreign config is not allowed to be cleared if there is preserved cach
SCGCQ00895265 - (Active) - System hung after abort running CC continuously overnight.
SCGCQ00896169 - (Port_Complete) - Cannot start rebuild for degrade cachecade VDs after an overnight heavy IO run
SCGCQ00898395 - (Active) - Patrol read doesn't resume after power cycle.
SCGCQ00908149 - (Port_Complete) - Storcli throws error while performing /c0/vx show all after full Init on R1 VD created by SSD drives.
SCGCQ00910570 - (Port_Complete) - After reboot imported 4K drive R0 is not visible
SCGCQ00923279 - (Port_Complete) - Cleanup device wait queue if drive is no longer online
SCGCQ00927938 - (Port_Complete) - MR6.9_FW : sasPortNumberValid bit does not get updated in CtrlR
SCGCQ00931370 - (Port_Complete) - During overnight multipath break/restore test, FW began printing "Found invalid event at fc4966ec" every 5 seconds
SCGCQ00942380 - (Port_Complete) - Unable to detect All VD degrade status for Partial VDs created on same PDs 
SCGCQ00990093 - (Port_Complete) - Data miscompare found with WB R1 cachecade when IOs run overnight
SCGCQ00883311 - (Port_Complete) - WT and WB cached policies can be changed via Windows Logical Disk Properties.
SCGCQ00896166 - (Port_Complete) - Montask observed while trying to create a CCVD using SLT : MonTask: line 1413 in file ../../raid/config.c
SCGCQ00896171 - (Port_Complete) - MonTask: line 2735 in file ../../ssd/ssd_cache_fw.c when inject error in a loop
SCGCQ00900027 - (Port_Complete) - Alert repeated twice for cancel check consistency on VDs
SCGCQ00905603 - (Port_Complete) - Controller encountered fatal error and was reset under heavy IOs and background operations.
SCGCQ00905809 - (Port_Complete) - CLCA defect: cachecade related 240VD checks needs to account for controller property settings.
SCGCQ00908237 - (Port_Complete) - OOB SLT not displaying Show Configuration Summary for 240 VDs created
SCGCQ00924743 - (Port_Complete) - iMR 6.10 Alpha:MonTask: line 1279 in file ../../raid/1078dma.c on IMR card while booting with R0 DIFF VD on Ubuntu 14.10.
SCGCQ00997546 - (Port_Complete) - MR_6.11_FW: Data corruption seen on IMR controller on JBOD with raw IO using smash tool- sles OS
SCGCQ00894455 - (Port_Complete) - Add Event Reporting for SuperCap Health After Learn Cycles
SCGCQ00898398 - (Port_Complete) - Firmware does not log controller property change event for enabling/disabling 240VD feature
SCGCQ00910741 - (Port_Complete) - wave4scrum pdisk state remains as ready even after creating a vdisk on that
SCGCQ00924740 - (Port_Complete) - Issue ABORT TASK and ABORT TASK SET to SATA device instead of failing them as unsupported
SCGCQ00926791 - (Port_Complete) - Difference of Code between the Defect Fix and Cset - Code Review AI
SCGCQ00936647 - (Port_Complete) - RAID 10 PI error message "SAS core detected EEDP error in application tag".
SCGCQ00883356 - (Port_Complete) - Enabling fault LED behavior for a specific customer
SCGCQ00908238 - (Port_Complete) - Firmware logs event MR_EVT_CTRL_PR_PROP_CHANGED twice.
SCGCQ00922677 - (Port_Not_Required) - Recon VD made "degraded" when the recon pd is pulled out allowing for rebuild once the drive is plugged back in.
SCGCQ00824712 - (Port_Complete) - PERC 9.2: Auto Configured RAID0 DGs is disordered in H83


NVDATA:
Numerous changes for specific customers

HII:
SCGCQ00921982 - (Closed) - handle coverity defects
SCGCQ00892931 - (Closed) - Not able to set Controller properties
SCGCQ00893936 - (Closed) - Add missing MFI STATS and corresponding strings
SCGCQ00896827 - (Closed) - Cannot convert the state of drive from JBOD to UG if the drive is not 16byte CDB
SCGCQ00927163 - (Closed) - MR_6.10_HII: Inconsistency across apps for retention time in HII.
SCGCQ00891345 - (Closed) - Add new logic to find valid PD device ID in multipath
SCGCQ00936369 - (Closed) - HII: Multipath logic change in enclosure management
SCGCQ00894460 - (Closed) - Controller status inconsistency between Dashboard and Controller management in HII
SCGCQ00907693 - (Closed) - Code Cleanup in HII for JBOD case
SCGCQ00915093 - (Closed) - HII: Updating LargeIOSupport as per the new API changes
SCGCQ00928664 - (Closed) - MR_6.10_HII: With pinned cache HII hangs while trying to enter "cache and memory" tab under advanced controller properties
SCGCQ00903490 - (Closed) - HII RLM for only R0 available when 18 or more drives are present
SCGCQ00898506 - (Closed) - OS doesn't boot after installing OS on the 100th VD , while having 240 VDs created in EFI mode
SCGCQ00893928 - (Closed) - HII: Address review comments
SCGCQ00901060 - (Closed) - Display NVRAM Size only if hwpresent.nvram is present
SCGCQ00922002 - (Closed) - DATA TLB Error(MonTask: line 245 in file) on enabling JBOD from HII while running patrol rea
SCGCQ00897580 - (Opened) - Add Support for OEM iMR Board
SCGCQ00890588 - (Implemented) - Support for RAID00 RAID-Level in HII Utility
SCGCQ00877539 - (Implemented) - Profile Based Virtual Drive creation menu doesn't describe what it expects.
SCGCQ00893152 - (Closed) - HII: Add support to enable/Disable of Large IO Support
SCGCQ00897578 - (Closed) - Add Support for OEM iMR Boa

UEFI Driver:
SCGCQ00898506 - (Closed) - OS doesn't boot after installing OS on the 100th VD , while having 240 VDs created in EFI m
SCGCQ00897578 - (Closed) - Add Support for OEM iMR Boa
SCGCQ00900968 - (Port_Complete) - OS doesn't boot after installing OS on the 100th VD , while having 240 VDs created in EFI 

BIOS:
SCGCQ00900948 - (Closed) - Remove \n from the bios binary
SCGCQ00877528 - (Implemented) - Add "(boot)" next to boot VD/PD in Legacy OpROM P

CTRL-R
SCGCQ00907063 - (Closed) - CTRL+R allows to choose R00 RAID level during CC VD creation and which leads to FW exception
SCGCQ00892129 - (Closed) - Most of the commands fail with "Invalid argument" error.
SCGCQ00892967 - (Closed) - Intruder: The size of the foreign config shown does not match with that after an import.
SCGCQ00893032 - (Closed) - With Liberator the Physical sector size of 512E drive is shown wrong
SCGCQ00936370 - (Closed) - Ctrl-H: Multipath logic change in PD Management
SCGCQ00914908 - (Closed) - Expand size link is enabled eventhough available size is 0 in Cachecade diskgroup
SCGCQ00906848 - (Closed) - Configure Hot spare is enabled for R00 VD during the VD cretion in CTRL+R
SCGCQ00819233 - (Closed) - StorCli EFI : Displaying string error message in JSON validation for show init (storcli) command
SCGCQ00891323 - (Closed) - Add new logic to find valid PD device ID in multipath
SCGCQ00940643 - (Closed) - Getting option to import foreign config after pinned cache in Ctrl-R when BIOS mode is in "safe mode"
SCGCQ00921914 - (Closed) - CTRL-H:handle coverity defects
SCGCQ00880534 - (Closed) - Invader 6.9 : Efi cli - Command fails with a hang when multiple controllers connected .
SCGCQ00911319 - (Closed) - Intruder: In Max link speed we will display only 8 phys information.
SCGCQ00916740 - (Closed) - LibMod: Display connector and Enclosure information for backplane drives
SCGCQ00902996 - (Resolved) - Intruder: Ctrl-R causes Firmware Montask when user clicks on Manage Link Speed option
SCGCQ00915525 - (Closed) - Resource leaks while getting drive phy error counters
SCGCQ00905925 - (Closed) - Apply button is active in Ctrl Mgnt when traversed from Rebuild rate to BGI rate
SCGCQ00914876 - (Closed) - Manage dedicated hotspare is available for Cachecade DG and assign hotspare fails at the end
SCGCQ00899384 - (Closed) - Buffer is not incremented when reading sector of the drive
SCGCQ00915518 - (Closed) - Checking in the changes for multipath logic as part of architechts review comments.
SCGCQ00916410 - (Closed) - Ctrl-H: Display connector and Enclosure information for backplane drives
SCGCQ00915164 - (Closed) - CTRL-H: Updating LargeIOSupport as per the new API changes
SCGCQ00934146 - (Closed) - Hotspares are shown as transport ready even it is excluded from transpor
SCGCQ00900104 - (Closed) - Added the iMR cutlass PNP id's(0x1000/0052h, 0x1000/0x0053h) to EFI controller explorer class.
SCGCQ00930245 - (Implemented) - Added the support to set and clear the transport on a DG either by including/excluding hotspares.
SCGCQ00893498 - (Closed) - LibMods: Add support to enable/Disable of Large IO Support - 1 MB IO
SCGCQ00893153 - (Closed) - CTRL-H: Add support to enable/Disable of Large IO Support
SCGCQ00933319 - (Implemented) - Added the support to swtich the large queue depth ctrl property in storcli
SCGCQ00894986 - (Implemented) - System x: Rebranding effort: Add new PCI VENDOR ID 0x1D49 for lenovo system x
SCGCQ00867891 - (Closed) - StorCLI Feature Request: Request a way to link MegaRAID virtual disk to Linux kerbel /dev/sdX]
SCGCQ00890587 - (Implemented) - Support for RAID00 RAID-Level in Ctrl+R Utility
SCGCQ00897714 - (Implemented) - 3216 IMR: CtrlH Add Support for OEM iMR Board
SCGCQ00889858 - (Closed) - Support for RAID00 RAID-Level in Ctrl+R Utili
SCGCQ00894633 - (Port_Complete) - LibMods: Add support to enable/Disable of Large IO Support - 1 MB IO
SCGCQ00904852 - (Port_Complete) - Checking-in changes for defect-SCGCQ00904794
SCGCQ00907053 - (Port_Complete) - Apply button is active in Ctrl Mgnt when traversed from Rebuild rate to BGI rate
SCGCQ00916359 - (Port_Complete) - Manage dedicated hotspare is available for Cachecade DG and assign hotspare fails at the end
SCGCQ00925305 - (Active) - MR6.8_StorCLI : GetCtrlInfo : ProcessLibCommand failed; retCode = 0x8017 seen when 1 out of 2 controller is in fault state.
SCGCQ00925306 - (Active) - MR6.8_StorCLI : GetCtrlInfo : ProcessLibCommand failed; retCode = 0x8017 seen when 1 out of 2 controller is in fault state.
SCGCQ00911728 - (Port_Complete) - With Liberator the Physical sector size of 512E drive is shown wrong
SCGCQ00928642 - (Port_Complete) - Ctrl-H: Handle return value when updating controller property
SCGCQ00900172 - (Port_Complete) - Added the iMR cutlass PNP id's(0x1000/0052h, 0x1000/0x0053h) to EFI controller explorer class.
SCGCQ00901264 - (Port_Complete) - MR 6.8: storcli reports legacy driver version when native driver is loaded for a Fury controller in ESXi 6.0
SCGCQ00901598 - (Port_Complete) - CTRL_H showing on-board memory size when memory is not present
SCGCQ00905068 - (Port_Complete) - CTRL-H: 'Next Learn Cycle Time' & 'Learn Period' not displayed when battery supports transparent learn.
SCGCQ00912802 - (Active) - Mis-alignment of error messages display for hide operation
SCGCQ00914212 - (Port_Complete) - EPMR8:Ctrl-R: Error code "Unknown" for setting hidden VD as boot VD in Ctrl-R
SCGCQ00916352 - (Port_Complete) - Expand size link is enabled eventhough available size is 0 in Cachecade diskgroup
SCGCQ00894489 - (Port_Complete) - Inconsistency in showing controller status between MSM and StorCLI for Fake Flash errors
SCGCQ00896676 - (Port_Complete) - CTRL-H: Add support to enable/Disable of Large IO Support
SCGCQ00901284 - (Active) - MR 6.8: storcli reports legacy driver version when native driver is loaded for a Fury controller in ESXi 6.0
SCGCQ00914214 - (Port_Complete) - EPMR8:Ctrl-R: Error code "Unknown" for setting hidden VD as boot VD in Ctrl-R
SCGCQ00895070 - (Active) - Invader 6.9 : Efi cli - Command fails with a hang when multiple controllers connected .
SCGCQ00931904 - (Port_Complete) - storcli command shows Failure on SWR for command "storcli /c0 show all"
SCGCQ00942778 - (Port_Complete) - Ctrl-R is allowing to enable and disable JBOD on the controller in SDS Mode
SCGCQ00893015 - (Port_Complete) - Inconsistency in showing controller status between MSM and Ctrl-R for Fake Flash errors
SCGCQ00907133 - (Port_Complete) - Intruder: The size of the foreign config shown does not match with that after an import.
SCGCQ00914218 - (Port_Complete) - No error message for failure of Disable SSD Caching of an offline VD
SCGCQ00915728 - (Port_Complete) - CTRL-H: Updating LargeIOSupport as per the new API changes
SCGCQ00931889 - (Port_Complete) - CTRL_H showing on-board memory size when memory is not present
SCGCQ00932144 - (Port_Complete) - storcli command shows Failure on SWR for command "storcli /c0 show all"
SCGCQ00894487 - (Port_Complete) - Inconsistency in showing controller status between MSM and StorCLI for Fake Flash errors
SCGCQ00899415 - (Port_Complete) - Buffer is not incremented when reading sector of the drive
SCGCQ00902429 - (Port_Complete) - LibMod:Missing WB Option
SCGCQ00904856 - (Port_Complete) - Most of the commands fail with "Invalid argument" error.
SCGCQ00914215 - (Port_Complete) - No error message for failure of Disable SSD Caching of an offline VD
SCGCQ00915469 - (Port_Complete) - Checking-in Libmod changes for defect-SCGCQ0091483
SCGCQ00942788 - (Port_Complete) -  LibMod Ctrl-R is allowing to enable and disable JBOD on the controller in SDS Mode
SCGCQ00893255 - (Port_Complete) - Inconsistency in showing controller status between MSM and Ctrl-R for Fake Flash errors
SCGCQ00932043 - (Port_Complete) - CTRL-H: 'Next Learn Cycle Time' & 'Learn Period' not displayed when battery supports transparent lear


Installation:
=============
Use StorCLI to flash the SAS controllers.  These tools can be downloaded from the support and download
section of www.avagotech.com

Command syntax:  
StorCLI /c0 download file=mr3108fw.rom



=================================
=================================
Previous Releases
=================================
=================================
Component:
=========
SAS MegaRAID Firmware Release for MegaRAID Controllers
Release date: 11/18/15


Version Numbers:	
===============
Current Package Details:
Firmware Package:24.10.0-0020 (MR 6.9 P1)
Firmware 4.600.00-4907
ROMENV 1.09
BootBlock 3.07.00.00-0003
NVDATA  3.1508.00-0009
UEFI_Driver 0x06110200(signed)
Hii 03.17.14.01(signed)
FCODE 4.17.08.00
BIOS 6.28.04.0
Ctrl-R 5.13-1101
PCLI 1.07.05

Previous Package Details:
Firmware Package:24.10.0-0017 (MR 6.9)
Firmware 4.290.00-4536
ROMENV 1.09
BootBlock 3.07.00.00-0003
NVDATA  3.1508.00-0007
UEFI_Driver 0x06110200(signed)
Hii 03.17.14.00(signed)
FCODE 4.17.08.00
BIOS 6.28.04.0
Ctrl-R 5.13-1100
PCLI 1.07.05


Bug Fixes and Enhancements:
===========================
Firmware:
SCGCQ00864348 - (Closed) - Unexpcted AEN of aborting Init During Firmware Down/upgrade
SCGCQ00894719 - (Closed) - Reconstruction error message "invalid arguments"
SCGCQ00898140 - (Closed) - Code changes to be made under specific macro for a feature
SCGCQ00898564 - (Closed) - MSM shows "null x0" to describe port connection to enclosure when multipath is broken
SCGCQ00900237 - (Closed) - Created VD configuration with PDs released from previous VD erased will lost after next reboot
SCGCQ00901889 - (Closed) - A hidden VD can be configured as bootdrive
SCGCQ00901919 - (Closed) - hot remove then hot add of drive in array causes BSOD
SCGCQ00906997 - (Closed) - forceCacheFlush check was added inappropriately in flush_cache() function
SCGCQ00907673 - (Closed) - Handling the DIF errors identified by BLADE DMA.
SCGCQ00908165 - (Closed) - Firmware logs event MR_EVT_CTRL_PR_PROP_CHANGED twice.
SCGCQ00908885 - (Closed) - Random Write perf drop up to %30 in 2R1 WB RA DCD 
SCGCQ00910433 - (Closed) - HDD LED state indicating Ready-To-Remove is affected by Locate LED on/off
SCGCQ00913426 - (Closed) - Controller hits MonTask: line 1278 in file ../../raid/1078dma.c after importing PD's with pinned cache
SCGCQ00914515 - (Closed) - Make sure boot target ID is in valid range
SCGCQ00916037 - (Closed) - Controller encountered fatal error and was reset during IO and Drive Pull
SCGCQ00919487 - (Closed) - Handle recon allowed Operation in Firmware
SCGCQ00925394 - (Closed) - Native config come up as foreing during FW upgrade from non-240 VD FW to 240VD FW.
SCGCQ00925640 - (Closed) - Set factory default does not reset the modified phy link speed
SCGCQ00927792 - (Closed) - Particular Drive not discovered in MR6.8, but MR6.7 works fine.
SCGCQ00928506 - (Closed) - StorCLI show all command triggers datastore disconnect on 3 R5 VD VMware ESXi
SCGCQ00928699 - (Closed) - Unexpected AEN "Warning Error during boot - Configuration command was not committed, please retry"
SCGCQ00930593 - Wrong MFI_STAT was returned in PdDcmdSysPdMapAbort()
SCGCQ00945033 - (Closed) - Add Flush in LdInitPdDone
SCGCQ00880907 - (Closed) - MR Controller reported fatal error and reset while creating 240 VD
SCGCQ00883996 - (Closed) - StorCLI/StorCLIO allows to Hide boot drive which is already in Hidden State.
SCGCQ00890968 - (Closed) - R6 Stays Enabled on TFM
SCGCQ00904616 - (Closed) - Fails to downgrade hba fw
SCGCQ00904833 - (Closed) - OOB SLT not displaying Show Configuration Summary for 240 VDs created
SCGCQ00907123 - (Closed) - CtrlH will halt(no responding) at the end of erase When perform VD erase and delete VD on the 2 VDs simultaneous
SCGCQ00923103 - (Closed) - Remove environment string for large IO support
SCGCQ00889734 - (Closed) - StorCLI/StorCLIO allows to Hide drive which is already in Hidden State
SCGCQ00893368 - (Closed) - Cachecade related 240VD checks needs to account for controller property settings.
SCGCQ00904466 - (Closed) - MSM shows messages with Error code 240 and no description
SCGCQ00883612 - (Closed) - Enable sgpioSmpPresenceDetect for all Invader based OEM controllers.
SCGCQ00935706 - (Closed) - Support Single Write for 4GB 3108 ROMB Design using 8GB Ptolemy for an OEM (MR FW)
SCGCQ00917409 - (Closed) - MR 6.8: Integrating PL 08.00.09.00 to MR 6.8
SCGCQ00916738 - (Closed) - MR 6.7: Integrating PL 07.00.10.00 to MR 6.7
SCGCQ00915869 - (Closed) - Block upgrade and downgrade Firmware when reconstruction is in progress
SCGCQ00903649 - (Closed) - Support locate bit for locate LED on/off on JBOD PD
SCGCQ00886938 - (Closed) - when multiple VDs are present VD reconstruction fails, but throws the error message "invalid arguments" in storCLI
SCGCQ00833849 - (Port_Complete) - FW hung at LogInit: Flushing events from previous boot while running policy change script of Vd and learn cycles.
SCGCQ00833850 - (Port_Complete) - FW hung at LogInit: Flushing events from previous boot while running policy change script of Vd and learn cycles.
SCGCQ00833852 - (Port_Complete) - FW hung at LogInit: Flushing events from previous boot while running policy change script of Vd and learn cycles.
SCGCQ00849554 - (Port_Complete) - Unexpected controller reset during test run
SCGCQ00876061 - (Port_Complete) - FW hits to MonTask: line 4946 in file ../../raid/ld.c while multipath push pull with patrol read
SCGCQ00876102 - (Active) - 'Watchdog Timer Exception' followed by FW crash after initiating PD Erase on UG PD, with BG operation & IO's on 64 VD's
SCGCQ00877435 - (Port_Complete) - Recon VD made "degraded" when the recon pd is pulled out allowing for rebuild once the drive is plugged back in.
SCGCQ00880776 - (Port_Complete) - Foreign config is not allowed to be cleared if there is preserved cache
SCGCQ00880870 - (Port_Complete) - MR 6.6.3 "storcli /c0 show all" shows lot of bad block messages in the log
SCGCQ00880875 - (Port_Complete) - Do not automatically assign boot VD by default
SCGCQ00880877 - (Port_Complete) - Support Zone Out functionality for OEM expanders
SCGCQ00880878 - (Port_Complete) - Megaraid Thunderbolt controller reports cache memory size as 0 when no logical drives are present.
SCGCQ00880880 - (Port_Complete) - StorCli to Message Hide Boot VD User Operation Status correctly
SCGCQ00882931 - (Port_Complete) - Fault LED behavior in OEM Blades
SCGCQ00883500 - (Port_Complete) - MonTask after Initiating a Raid Level migration
SCGCQ00885571 - (Port_Complete) - Windows BSOD when upgrade FW 24.6.0-0040 to 24.8.0-0026 with driver 6.707.08.00
SCGCQ00885733 - (Port_Complete) - StorCLI/StorCLIO allows to Hide boot drive which is already in Hidden State.
SCGCQ00885734 - (Port_Complete) - StorCLI/StorCLIO allows to Hide boot drive which is already in Hidden State.
SCGCQ00886910 - (Port_Complete) - Data TLB error found while running the target reset script with multipath cable pull-push operation
SCGCQ00889826 - (Port_Complete) - Add support for show SBR command
SCGCQ00889922 - (Port_Complete) - FW hung at LogInit: Flushing events from previous boot while running policy change script of Vd and learn cycles.
SCGCQ00893924 - (Port_Complete) - IO halts on JBODs with read/write error when the target drives are reset via MFI or MPT path on Linux distro
SCGCQ00895476 - (Port_Complete) - FW breaks MonTask: line 245 in file ../../raid/1078int.c with IOs on max VD configured and BGOps
SCGCQ00898359 - (Port_Complete) - 'Watchdog Timer Exception' followed by FW crash after initiating PD Erase on UG PD, with BG operation & IO's on 64 VD's
SCGCQ00898397 - (Port_Complete) - Firmware does not log controller property change event for enabling/disabling 240VD feature
SCGCQ00898473 - (Port_Complete) - Firmware breaks to montask while importing the Foreign Config.
SCGCQ00898730 - (Port_Complete) - Core 0 exception seen while trying to import foreign configuration with pinned cache present.
SCGCQ00898752 - (Port_Complete) - FW downgrade fails with IOs and BGops .
SCGCQ00898758 - (Port_Complete) - Controller killed on issuing OCR from StorCLI after disabling it from OS.
SCGCQ00898762 - (Port_Complete) - TTY log dump is not persistent for multiple boots.
SCGCQ00898773 - (Port_Complete) - Add sanity check for iPtr and rPtr after restore is completed.
SCGCQ00898780 - (Port_Complete) - One deletion of CCVD FW displays incorrect CCVD target id and remaining CacheCade size on the system
SCGCQ00898790 - (Port_Complete) - sasPortNumberValid bit does not get updated in CtrlR
SCGCQ00898808 - (Port_Not_Required) - Remove checkSysPwrStatus() and processSysPwrReturn() functions.
SCGCQ00898880 - (Port_Complete) - Kill adapter during test run
SCGCQ00899333 - (Port_Complete) - Controller discovery failed due to pending Boot messages, adapter at baseport not responding.
SCGCQ00899474 - (Port_Complete) - On receiving CACHE_FLUSH_DCMD, set forceCacheflush flag to 1 to flush the cache
SCGCQ00904475 - (Port_Complete) - Unexpcted AEN of aborting Init During Firmware Down/upgrade
SCGCQ00905418 - (Port_Complete) - Controller encountered fatal error and was reset under heavy IOs and background operations.
SCGCQ00905782 - (Port_Complete) - FW breaks MonTask: line 245 in file ../../raid/1078int.c with IOs on max VD configured and BGOps
SCGCQ00907679 - (Port_Complete) - on creating 240VD and rebooting the server, FW breaks into montask.
SCGCQ00907680 - (Port_Complete) - on creating 240VD and rebooting the server, FW breaks into montask.
SCGCQ00907682 - (Port_Complete) - LUID gets changed during foreing import from non-240VD FW to 240VD FW
SCGCQ00908903 - (Port_Complete) - LUID gets changed during foreing import from non-240VD FW to 240VD FW
SCGCQ00909037 - (Port_Complete) - fails to downgrade hba fw
SCGCQ00910375 - (Port_Complete) - OOB SLT not displaying Show Configuration Summary for 240 VDs created
SCGCQ00910389 - (Port_Complete) - Firmware logs event MR_EVT_CTRL_PR_PROP_CHANGED twice.
SCGCQ00910569 - (Port_Complete) - After reboot imported 4K drive R0 is not visible
SCGCQ00911211 - (Port_Complete) - Created VD configuration with PDs released from previous VD erased will lost after next reboot
SCGCQ00911213 - (Port_Complete) - Created VD configuration with PDs released from previous VD erased will lost after next reboot
SCGCQ00911215 - (Port_Complete) - Created VD configuration with PDs released from previous VD erased will lost after next reboot
SCGCQ00911773 - (Port_Complete) - Handling Functional Level Reset (FLR) .
SCGCQ00911790 - (Active) - Reduce Command Block Latency during Background Operations
SCGCQ00922541 - (Port_Complete) - Importing 240 VD foreign configuration leads to FW Crash
SCGCQ00922542 - (Port_Complete) - as been observed that the firmware retires the FPIO timed out IOs for 3 times instead of the reduced count to
SCGCQ00922716 - (Port_Complete) - Controller encountered fatal error and was reset under heavy IOs and background operations.
SCGCQ00923113 - (Port_Complete) - hot remove then hot add of drive in array causes BSOD
SCGCQ00923405 - (Port_Complete) - Configuration creation on Controller fails after creation of a CC VD followed by JBOD creation.
SCGCQ00929473 - (Port_Complete) - Handling the DIF errors identified by BLADE DMA.
SCGCQ00934617 - (Port_Complete) - RAID 10 PI error message "SAS core detected EEDP error in application tag".
SCGCQ00934619 - (Port_Complete) - CRC mismatch and invalid log event found while querying for Controller properties and learn cycle in parallel.
SCGCQ00934711 - (Port_Complete) - CtrlH will halt(no responding) at the end of erase When perform VD erase and delete VD on the 2 VDs simultaneous
SCGCQ00873095 - (Port_Complete) - FW allows CCVD deletion with pinned windows
SCGCQ00873096 - (Port_Complete) - FW allows CCVD deletion with pinned windows
SCGCQ00880876 - (Port_Complete) - Support Zone In functionality for OEM expanders
SCGCQ00883175 - (Port_Complete) - Consistency Check running under high I/O load causing VMWare DataStore disconnect on RAID 5 VDs
SCGCQ00898761 - (Port_Complete) - FW breaks MonTask: line 245 in file ../../raid/1078int.c with IOs on max VD configured and BGOps
SCGCQ00899818 - (Port_Complete) - MonTask: line 1280 in file ../../raid/1078dma.c. DCDB cmd timed out
SCGCQ00905494 - (Port_Complete) - fails to downgrade hba fw
SCGCQ00906991 - (Port_Complete) - On receiving CACHE_FLUSH_DCMD, set forceCacheflush flag to 1 to flush the cache
SCGCQ00908347 - (Port_Complete) - Copyback fails to start and causes a FW fault
SCGCQ00908894 - (Port_Complete) - LUID gets changed during foreing import from non-240VD FW to 240VD FW
SCGCQ00908904 - (Port_Complete) - on creating 240VD and rebooting the server, FW breaks into montask.
SCGCQ00914742 - (Port_Complete) - Medium error correction events were not reported
SCGCQ00917202 - (Active) - During long run reboot test, FW eventually reports "Disabling writes to flash due to a critical error"
SCGCQ00922595 - (Port_Complete) - Cachecade related 240VD checks needs to account for controller property settings.
SCGCQ00923292 - (Port_Complete) - Remove environment string for large IO support
SCGCQ00929474 - (Port_Complete) - Controller encountered fatal error and was reset during IO and Drive Pull
SCGCQ00880864 - (Port_Complete) - StorCLI reports success on 4MB MR flash on iMR which fails after reset - (SCGCQ00870439)
SCGCQ00880872 - (Port_Complete) - Disable FLR support in MR FW to address VMware guest VM abrupt shutdown issue
SCGCQ00881276 - (Port_Complete) - Megaraid_sas driver fails to communicate with the FW and fails to discover any disks attached
SCGCQ00885732 - (Port_Complete) - StorCLI/StorCLIO allows to Hide boot drive which is already in Hidden State.
SCGCQ00911685 - (Active) - wave4scrum pdisk state remains as ready even after creating a vdisk on that
SCGCQ00942794 - (Port_Complete) - Chaos report DC after rebuild complete on R6 with SAS SSD
SCGCQ00880866 - (Port_Complete) - Handling NVRAM migration for Patrol Read
SCGCQ00833851 - (Port_Complete) - FW hung at LogInit: Flushing events from previous boot while running policy change script of Vd and learn cycles.
SCGCQ00922681 - (Port_Complete) - Sanity check for handling the cases where event length comes up as zero/ rPtr goes beyond iptr

NVDATA:
Numerous changes for specific customers

HII:
SCGCQ00932071 - (Port_Complete) - Inconsistency across apps for retention time in HII.
SCGCQ00914259 - (Port_Complete) - HII Dashboard doesn't refresh enclosure and drive counter when an enclosure with foreign config is disconnected
SCGCQ00897835 - (Port_Complete) - HII Missing WB Option
SCGCQ00905879 - (Port_Complete) - MegaRAID Firmware Information not Displayed Under IMM
SCGCQ00932045 - (Port_Complete) - With pinned cache HII hangs while trying to enter "cache and memory" tab under advanced controller properties
SCGCQ00932117 - (Port_Complete) - DATA TLB Error(MonTask: line 245 in file) on enabling JBOD from HII while running patrol read.
SCGCQ00931887 - (Port_Complete) - In-correct associated drive group number showing for DHS drive
SCGCQ00931890 - (Port_Complete) - 'Next Learn Cycle Time' & 'Learn Period' not displayed when battery supports transparent learn.
SCGCQ00911105 - (Port_Complete) - HII Firmware Update Option
SCGCQ00931921 - (Port_Complete) - Display NVRAM Size only if hwpresent.nvram is present

CTRL-R
SCGCQ00907053 - (Port_Complete) - Apply button is active in Ctrl Mgnt when traversed from Rebuild rate to BGI rate
SCGCQ00916359 - (Port_Complete) - Manage dedicated hotspare is available for Cachecade DG and assign hotspare fails at the end
SCGCQ00916352 - (Port_Complete) - Expand size link is enabled eventhough available size is 0 in Cachecade diskgroup
SCGCQ00914214 - (Port_Complete) - Error code "Unknown" for setting hidden VD as boot VD in Ctrl-R
SCGCQ00933861 - (Port_Complete) - CTRL-H Missing WB Option
SCGCQ00897838 - (Port_Complete) - CTRL-H Missing WB Option
SCGCQ00914218 - (Port_Complete) - No error message for failure of Disable SSD Caching of an offline VD
SCGCQ00931889 - (Port_Complete) - CTRL_H showing on-board memory size when memory is not present
SCGCQ00932144 - (Port_Complete) - storcli command shows Failure on SWR for command "storcli /c0 show all"
SCGCQ00932043 - (Port_Complete) - 'Next Learn Cycle Time' & 'Learn Period' not displayed when battery supports transparent learn.

Installation:
=============
Use StorCLI to flash the SAS controllers.  These tools can be downloaded from the support and download
section of www.avagotech.com

Command syntax:  
StorCLI /c0 download file=mr3108fw.rom



Component:
=========
SAS MegaRAID Firmware Release for MegaRAID Controllers
Release date: 10/05/15


Version Numbers:	
===============
Current Package Details:
Firmware Package:24.10.0-0017 (MR 6.9)
Firmware 4.290.00-4536
ROMENV 1.09
BootBlock 3.07.00.00-0002
NVDATA  3.1507.00-0006
UEFI_Driver 0x06110200(signed)
Hii 03.17.14.00(signed)
FCODE 4.17.08.00
BIOS 6.28.04.0
Ctrl-R 5.13-1100
PCLI 1.07.05

Previous Package Details:
Current Package Details:
Firmware Package:24.9.0-0022 (MR 6.8)
Firmware 4.600.00-4747
ROMENV 1.09
BootBlock 3.07.00.00-0002
NVDATA  3.1507.00-0006
UEFI_Driver 0x060E0300 (SIGNED)
Hii v03.14.09.00 (SIGNED)
FCODE 4.17.08.00
BIOS 6.25.03.0
Ctrl-R 5.10-0700
PCLI 1.07.05


Bug Fixes and Enhancements:
===========================
Firmware:
SCGCQ00718801 - (Closed) - FW breaks to MonTask: line 1168 in file ../../raid/raid.c during RAID Operations
SCGCQ00724451 - (Closed) - FW breaks to MonTask: line 889 in file ../../raid/bladeDMA.c while creating a filesystem on R5 VD.
SCGCQ00725844 - (Closed) - Intruder pre alpha 2 : On a R1 to R5 reconstructing Virtual Drive, IO failed with data miscompare
SCGCQ00729599 - (Closed) - Intruder pre alpha 2 : "MonTask: line 396 in file ../../ssd/ssd_cache_fw.c" with IO on R5 VD with a CacheCade VD in WB
SCGCQ00747258 - (Closed) - .10 PL cause DataTLB error with MR FW.
SCGCQ00751361 - (Closed) - 512e support needs to be enabled in MR FW
SCGCQ00788071 - (Closed) - Code review items were fixed
SCGCQ00788072 - (Closed) - Code Review fixes for review Review #38871 -Integrate 6.5 Changes with Intruder Code stream
SCGCQ00791766 - (Closed) - Rebase Dev stream with Integration 6.5 manual changes
SCGCQ00794871 - (Closed) - FW breaks to MonTask: line 257 in file ../../dm/src/dmDrvPrep.c when booting FPGA
SCGCQ00807498 - (Closed) - Data corruption detected with offload and restore operation
SCGCQ00812867 - (Closed) - Data corruption reported with Intruder ONFI2 offload and restore operation
SCGCQ00819772 - (Closed) - Flash wrongly discovered as transported across back to back offload and restore cycles
SCGCQ00822311 - (Closed) - ONFI unable to offload to controllers with multiple chipselects
SCGCQ00823817 - (Closed) - FPGA stream missing .4 release stream content
SCGCQ00831595 - (Closed) - FW hanging with 0.6 release while bootup.
SCGCQ00832908 - (Closed) - MSM displays error message if 'Schedule Consistency Check' is selected.
SCGCQ00843098 - (Closed) - Un-correctable ECC error on Armstong board during cold boot
SCGCQ00844777 - (Closed) - Modifying SBR PnP IDs offset
SCGCQ00845435 - (Closed) - Data Corruption on WB VDs
SCGCQ00846621 - (Closed) - Medium error correction events were not reported
SCGCQ00848339 - (Closed) - FW hangs during cache flush after restore cache from flash.
SCGCQ00850401 - (Closed) - ONFI: FC0 CS0 offload meta length not valid:0, expected:7c00 causing restore to not start after offload.
SCGCQ00850839 - (Closed) - FW hangs after re-inserting SATA drive in direct connect topology during I/O.
SCGCQ00856977 - (Closed) - Unable to update drive firmware on customer specific FDE SATA SSDs
SCGCQ00858697 - (Closed) - For Sugon Romb dont Initialize the port activity LED's GPIO.
SCGCQ00863880 - (Closed) - MR_6.9_FW : Core 0 exception seen while trying to import foreign configuration with pinned cache present.
SCGCQ00864054 - (Closed) - Perform the PCI release retry while performing BISR on the second CPU.
SCGCQ00865116 - (Closed) - ROC Temp GPIO action item
SCGCQ00866261 - (Closed) - Invader firmware (4.280.00-4331 in MR 6.7) with write-verify has abnormal behavior/performance.
SCGCQ00867065 - (Closed) - Increase CACHE HEADER version, since new member was added to PinnedCacheDataStructure(Persistent DRAM)
SCGCQ00872875 - (Closed) - MR_6.9: MonTask: line 1280 in file ../../raid/1078dma.c. DCDB cmd timed out
SCGCQ00872889 - (Closed) - MR6.9_FW : Kill adapter seen while issuing Task Management in loop on 240 JBODs with IOs.
SCGCQ00873991 - (Closed) - Data TLB error occured after issuing task abort from host
SCGCQ00878414 - (Closed) - 6.9 : Write perf drops in 16R5 WT NoRA DCD SS64 1MB IO at QD128/256
SCGCQ00878432 - (Closed) - Blade DMA errors observed while running IOs
SCGCQ00878587 - (Closed) - MonTask: line 245 in file ../../raid/1078int.c while running I/Os with 64VDs and pull out drives belonging to CacheCade VD
SCGCQ00879193 - (Closed) - Restricting the VD deletion optimization to reduce IO freeze to least latency mode.
SCGCQ00881001 - (Closed) - StorCLI Reports Incorrect TFM Manufacturing Date
SCGCQ00881901 - (Closed) - FW hang, even-after Task Abort is successful on a drive in Linux OS
SCGCQ00882125 - (Closed) - On receiving CACHE_FLUSH_DCMD, set forceCacheflush flag to 1 to flush the cache
SCGCQ00882897 - (Closed) - Need to set perfTunerMode appropriately on controller reset.
SCGCQ00884589 - (Closed) - Windows BSOD when upgrade FW 24.6.0-0040 to 24.8.0-0026 with driver 6.707.08.00
SCGCQ00890133 - (Closed) - Invader 6.9: FW breaks MonTask: line 245 in file ../../raid/1078int.c with IOs on max VD configured and BGOps
SCGCQ00891924 - (Closed) -  Buffer Size is set to 1M and number of BSB per BB is set to 1.
SCGCQ00893588 - (Closed) - MR6.9_FW : IO halts on JBODs with read/write error when the target drives are reset via MFI or MPT path on Linux distro
SCGCQ00895554 - (Closed) - MR_6.9_FW: Kill adapter during test run
SCGCQ00904905 - (Resolved) - Copyback fails to start and causes a FW fault
SCGCQ00717238 - (Closed) - MR Intruder Fault x6101 - FW breaks to Montask: line 1557 in file ../../dm/pl2/pliopi.c
SCGCQ00738085 - (Closed) - Change flags for each sge in the sglist.
SCGCQ00750804 - (Closed) - FW breaks to MonTask: line 299 in file ../../raid/1078int.c when try to run IO on 32 drive R0 16 VD configuration.
SCGCQ00771238 - (Closed) - remove Cache split related changes from Int stream
SCGCQ00788087 - (Closed) - Multi- SAS Core - Code reivew defect fixes.
SCGCQ00788526 - (Closed) - Defect to check in code changes reported by static analysis tool for intruder
SCGCQ00803219 - (Closed) - Data corruption when destaging pinned cache after foreign config import.
SCGCQ00812295 - (Closed) - Back to back restore happen because flash region not toggled after a restore operation
SCGCQ00819786 - (Closed) - FW should prepare and arm HW for second offload before starting cache flush
SCGCQ00836031 - (Closed) - NVDATA and Controller Properties all zero
SCGCQ00845921 - (Closed) - Development defect for Cache Offload work around.
SCGCQ00846655 - (Closed) - Battery relearn timed out on Supercap on Armstrong board
SCGCQ00847001 - (Closed) - MR6.6 Controller is not accessible through OOB before OS is up and running
SCGCQ00848264 - (Closed) - Development defect for flash chip M83C workaround in Intruder
SCGCQ00850368 - (Closed) - Firmware Faults with error code 0x22 after an OCR
SCGCQ00855837 - (Closed) - A race condition exists while creating the flash filesystem and making the corresponding entries in NVRAM
SCGCQ00855845 - (Closed) - Disable pause for memory offload control 1.
SCGCQ00857181 - (Closed) - On performing back to back target reset on the same JBOD results into online controller reset(OCR)
SCGCQ00857680 - (Closed) - MR 6.7 Point : Few test cases fail when PCIeCV tool is executed
SCGCQ00857692 - (Closed) - MR 6.9 : Firmware allows to perform Reconstruction when Pinned Cache is present.
SCGCQ00859850 - (Closed) - Pinned Cache lost after trigger few OCR and reboot server as result data got corrupt
SCGCQ00860066 - (Closed) - Firmware breaks to montask while importing the Foreign Config.
SCGCQ00860503 - (Closed) - MR 6.9 : Controller boots to OS Even when Pinned Cache is present and Boot Error handling is set to Stop on Error.
SCGCQ00860635 - (Closed) - Firmware hang is observed when Cache Offload is interrupted by power restore.
SCGCQ00860716 - (Closed) - Firmware allows to create more than 64 logical drives in legacy mode.
SCGCQ00861819 - (Closed) - Address code review defects for ER SCGCQ008554
SCGCQ00871973 - (Closed) - FW allows CCVD deletion with pinned windows
SCGCQ00873239 - (Closed) - FW downgrade fails with IOs and BGops .
SCGCQ00874200 - (Closed) - Re-eanbling 1MB IO support.
SCGCQ00878554 - (Closed) - Core 0 exception in line 245 in ../../raid/1078int.c while Target reset on PDs and BG Operations in parallel
SCGCQ00879198 - (Closed) - MR6.9_FW : Assertion failure in ../../dm/src/dmDrvPrep.c at line 836: while Cable pull push on secondary enclosure.
SCGCQ00882742 - (Closed) - Fix coverity defects
SCGCQ00886685 - (Closed) - Add sanity check for iPtr and rPtr after restore is completed.
SCGCQ00894472 - (Closed) - Adjust cache thresholds appropriately after the pinned cache is generated and volumes are retained in WB mode.
SCGCQ00894608 - (Closed) - OS become unresponsive after creating multiple sliced VD's
SCGCQ00899762 - (Closed) - SKINNY compilation was broken after fixing SCGCQ00882125
SCGCQ00906129 - (Closed) - Intruder : Data Corruption issue seen while running cable breaker with CCVD associated
SCGCQ00908325 - (Closed) - Undoing the changes of CSET activity SCGCQ00803718
SCGCQ00914740 - (Closed) - 6.9: Default values does not get picked up for un-changed controller property sharing same byte.
SCGCQ00764924 - (Closed) - FW breaks to Montask: line 891 in file ../../raid/bladeDMA.c while creating file system on VDs.
SCGCQ00788106 - (Closed) - Code review fixes for 33080
SCGCQ00819441 - (Closed) - Port ONFI changes to Intruder .5 stream.
SCGCQ00823465 - (Closed) - Reconstruction from R1 to R5 causing FW hang.
SCGCQ00844839 - (Closed) - Armstrong board causing HP server to hang during bootup.
SCGCQ00845436 - (Closed) - Limit the Memory size to 1GB as temp workaround to DC issue.
SCGCQ00850220 - (Closed) - Check in OCR work around
SCGCQ00850441 - (Closed) - iMR 6.1.1 : Exception seen during OS Reboot heat run test
SCGCQ00850818 - (Closed) - Controller hangs during post if you have dirty cache that needs to be flushed to the VD.
SCGCQ00851267 - (Closed) - Firmware halted after trigger OCR with I/O
SCGCQ00852327 - (Closed) - When no drives connected tlb error is seen
SCGCQ00853020 - (Closed) - Firmware Test API returns incorrectly that hardware is armed for offload, when supercap is bad.
SCGCQ00855322 - (Closed) - !!! Firmware initialization failed. Fault code = 0x4 !!!
SCGCQ00857528 - (Closed) - MR_6.8:FW hits to MonTask: line 4946 in file ../../raid/ld.c while multipath push pull with patrol read
SCGCQ00859961 - (Closed) - Cannot disable patrol read on an Armstrong controller.
SCGCQ00865963 - (Closed) - Too many event in firmware log : onfiHwIsOffloadSustainableStateSet onfi_status 0
SCGCQ00872140 - (Closed) - MR6.9:'Watchdog Timer Exception' followed by FW crash after initiating PD Erase on UG PD, with BG operation & IO's on 64 VD's
SCGCQ00873201 - (Closed) - Avoid cache FLUSH during VD Deletion to reduce IO Freeze time on other VDs
SCGCQ00874332 - (Closed) - MR6.9_FW : FW hits montask due to a non-spinning up FDE drive, issue seen on repeated reboots.
SCGCQ00880919 - (Closed) - MR6.9_FW : Controller discovery failed due to pending Boot messages, adapter at baseport not responding.
SCGCQ00886351 - (Closed) - MR 6.8 : Few test cases fail when PCIeCV tool is executed
SCGCQ00900250 - (Closed) - Send appropritate MFI status for the command which needs to be aborted
SCGCQ00827430 - (Closed) - Loss of smart recovery blocks in a small window when switching regions
SCGCQ00832205 - (Closed) - Development defect to fix Code Coverity issues found in Intruder 0.6 Stream.
SCGCQ00845707 - (Closed) - MSM reports 4MB and 8MB FW image is corrupt and does not allow flashing Armstrong board.
SCGCQ00846582 - (Closed) - SATA drives not detected in direct connect topology -MR
SCGCQ00846657 - (Closed) - ONFI offload descriptors are not set to offload all valid DATA cache
SCGCQ00859720 - (Closed) - On OCR or reboot, retain volumes in WB if the number of pinned buffers is less than 50% of available buffers.
SCGCQ00859975 - (Closed) - Code review defect with 6.9 merge with Inv team
SCGCQ00860140 - (Closed) - Coverity: fix Coverity defect 16729
SCGCQ00874357 - (Closed) - Data TLB error occured while tring dereference invalid command ID
SCGCQ00877673 - (Closed) - Kill adapter while running IO with Task Reset on JBODs
SCGCQ00878923 - (Closed) - Remove PinnedCacheDataStructure totalPinnedBbs and totalPinnedBsbs update in PinCacheForLd()
SCGCQ00881919 - (Closed) - Data TLB error found while running the target reset script with multipath cable pull-push operation
SCGCQ00848368 - (Closed) - Armstrong Controller hangs when make JBOD from powersave PD.
SCGCQ00848372 - (Closed) - API calls to corrupt and verify DIS on ONFI NAND flash are not available in Intruder code release
SCGCQ00856566 - (Closed) - Code review defect with 6.9 merge with Inv team
SCGCQ00866487 - (Closed) - MR6.9_FW : sasPortNumberValid bit does not get updated in CtrlR
SCGCQ00867120 - (Closed) - MR6.8_FW : DISM stuck at device discovery on enclosure power cycle, Devices present with DM but not reflected in upper layers
SCGCQ00869626 - (Closed) - Compilation Error in Invader with Intruder merged code
SCGCQ00878097 - (Closed) - MR6.9:Assertion failure in ../../raid/cache.c at line 774, after pulling out the enclosure cable
SCGCQ00864019 - (Closed) - One deletion of CCVD FW displays incorrect CCVD target id and remaining CacheCade size on the system
SCGCQ00878150 - (Closed) - Controller killed on issuing OCR from StorCLI after disabling it from OS.
SCGCQ00881005 - (Closed) - Code cleanup issues.
SCGCQ00848321 - (Closed) - Offload starting with residual power, which corrupts metadata
SCGCQ00849733 - (Closed) - Development defect to remove the hardcoded TFM VPD values in firmware for Intruder.
SCGCQ00863348 - (Closed) - Remove checkSysPwrStatus() and processSysPwrReturn() functions.
SCGCQ00866206 - (Closed) - Modify app.ld to address iopath and dramCode region overflow - MR 6.9Intruder
SCGCQ00869060 - (Closed) - Intruder6.9 code review changes
SCGCQ00877100 - (Closed) - TTY log dump is not persistent for multiple boots.
SCGCQ00848328 - (Closed) - L2 Cache Error was NOT detected at POST after inject ECC error
SCGCQ00859968 - (Resolved) - Deleting duplicate/unwanted files from source contr
SCGCQ00679021 - (Closed) - Bringup MR Intruder fpga with Init bit stream.
SCGCQ00681940 - (Closed) - Following FW interfaces are implemented
SCGCQ00696857 - (Closed) - Invader 6.3 GCA code ported to Invader stream
SCGCQ00713577 - (Closed) - 2.1b Bitstream related MR Fw changes for Dallas FPGA Validation.
SCGCQ00760455 - (Closed) - Integrate .12 PL into MR code
SCGCQ00772420 - (Closed) - Merge 6.5 Changes with Intruder Code stream
SCGCQ00791733 - (Closed) - New PL integrated.
SCGCQ00804452 - (Closed) - Integrate Latest PL .19 with MR stack
SCGCQ00813852 - (Closed) - PL 0.85 release check-in
SCGCQ00813853 - (Closed) - Flash header changes for Intruder
SCGCQ00814430 - (Closed) - Code bring up on 3108 controller
SCGCQ00817806 - (Closed) - Updating release script for Intruder code base
SCGCQ00827051 - (Closed) - Integrate .22 PL and Invader 6.7 code.
SCGCQ00827085 - (Closed) - Adding Support in Firmware for a new Flash Controller for Intruder.
SCGCQ00834328 - (Closed) - Enable Synchronous mode of communication between Intruder and Flash Chip.
SCGCQ00840256 - (Closed) - Code changes for A0 silicon & Eval board.
SCGCQ00842347 - (Closed) - Creation and productization of new product SKU for 9361-8i board with 2GB of memory
SCGCQ00844787 - (Closed) - support for dual rank ddr memory in Intruder, new pl library, and DMA workaround
SCGCQ00846939 - (Closed) - Re-branding effort for customer.
SCGCQ00850707 - (Closed) - Fault LED support for predictive failure drives for SGPIO
SCGCQ00855889 - (Closed) - OEM wants controller VPD reporting should be disable
SCGCQ00856088 - (Closed) - GPIO Settings for a customer
SCGCQ00861994 - (Closed) - Check-in 6.9 Intruder code changes to use same MEM_FIXED for Inruder and Invader
SCGCQ00864357 - (Closed) - Check-in PL 250.34 to Inruder A0.
SCGCQ00865372 - (Implemented) - Reduce Command Block Latency during Background Operations
SCGCQ00882016 - (Closed) - Integrating PL 06.00.05.00 with 6.6 FW stream.
SCGCQ00884951 - (Closed) - Integrate 08.00.05.00 MR PL with MR 6.8
SCGCQ00893029 - (Closed) - Add support to enable/Disable of Large IO Support - 1 MB IO
SCGCQ00908329 - (Closed) - SCSI Inquiry string should not change in current generation HBA
SCGCQ00681943 - (Closed) - ONFI debug functionality implemented to test software based offload and restore operations
SCGCQ00687251 - (Closed) - Implement Cache-split feature
SCGCQ00710266 - (Closed) - Intruder Dual SAS core changes.
SCGCQ00721312 - (Closed) - Add support for TM and Error handling with dual sas core to MR.
SCGCQ00772441 - (Closed) - Intergrate PL 0.13 to Intruder fpga
SCGCQ00772443 - (Closed) - Put Infrastructure to compile Intruder and Invader on same code base.
SCGCQ00792619 - (Closed) - Implemented as part of Intruder FPGA bringup.
SCGCQ00837210 - (Closed) - For the new flash chip in Intruder, additional DDR Regions is memset to 0 after cache restore is complete.
SCGCQ00841116 - (Closed) - Add Manual BISR to bring up secondary core for Intruder
SCGCQ00862035 - (Closed) - New LED to indicate Over Temperature in Intruder.
SCGCQ00809693 - (Closed) - Invader 6.6 Code stream merge to Intuder.
SCGCQ00852052 - (Closed) - Add pl 0.250.27 to Intruder code.
SCGCQ00853299 - (Closed) - Incorporate Memory Port difference for xor base address for Intruder
SCGCQ00853423 - (Closed) - Implement the HW workaround in Intruder to recover from warm reset
SCGCQ00855457 - (Implemented) - Task management support for JBOD/sysPD to Windows and Linux drivers (follow-on to PR SCGCQ00687438)
SCGCQ00860586 - (Closed) - Add 5/15 6.9 action item changes
SCGCQ00861695 - (Closed) - Add support for Micron M83C flash part for Intruder generation products.
SCGCQ00880731 - (Closed) - Integrate Phase 9 PL 9.0.0.0 with MR 6.9
SCGCQ00781019 - (Closed) - Retain Configuration btw boots on FPGA environment
SCGCQ00846602 - (Closed) - New GPIO definitions for Intruder
SCGCQ00868957 - (Closed) - Integrate Phase 9 PL (version 9.0.0.0) with MR 6.9
SCGCQ00841181 - (Closed) - A0 Intruder bring activities Part 2
SCGCQ00856859 - (Closed) - Check in new pl 250.32
SCGCQ00860624 - (Closed) - Update ManPage12 and ManPage13 as per new structures defined for Intruder
SCGCQ00852061 - (Closed) - MPIC configuration table changes
SCGCQ00852502 - (Implemented) - Avoid Moving WB volumes to WT on pinned cache genera
SCGCQ00805369 - (Port_Complete) - Bad physical drive caused controller error recovery go in loop
SCGCQ00833943 - (Port_Complete) - MR6.7-Beta:FW hits to MonTask: line 1272 in file ../../raid/1078dma.c after Injecting media error in loop on CCVD metadata
SCGCQ00833944 - (Port_Complete) - MR6.7-Beta:FW hits to MonTask: line 1272 in file ../../raid/1078dma.c after Injecting media error in loop on CCVD metadata
SCGCQ00833945 - (Port_Complete) - MR6.7-Beta:FW hits to MonTask: line 1272 in file ../../raid/1078dma.c after Injecting media error in loop on CCVD metadata
SCGCQ00833946 - (Port_Complete) - MR6.7-Beta:FW hits to MonTask: line 1272 in file ../../raid/1078dma.c after Injecting media error in loop on CCVD metadata
SCGCQ00837206 - (Port_Complete) - Setting the Learn Cycle property of iBBU09 gives an I2C error
SCGCQ00838545 - (Port_Complete) - MR_6.8_FW: Fw hits to MonTask: line 1272 in file ../../raid/1078dma.c while running IO in VM
SCGCQ00841545 - (Port_Complete) - Performing a cable pull/push with array property change resulting into FW hang.
SCGCQ00844445 - (Port_Complete) - Commands to the fde drives are not responding within 500ms.
SCGCQ00845203 - (Port_Complete) - MR_6.8_FW:Firmware halted and restarted while doing flash erase on the onfi flash
SCGCQ00848415 - (Port_Not_Required) - flush cache with write_verify on R0 volume and sata drive
SCGCQ00849553 - (Port_Complete) - Unexpected controller reset during test run
SCGCQ00849614 - (Port_Complete) - chain element for non RW commands were not pulled in the FW
SCGCQ00849620 - (Port_Complete) - Deleting a Cachecade VD (CC VD) results in a firmware hang situation.
SCGCQ00850990 - (Port_Complete) - Rebuild Performance for RAID 1 arrays is slower.
SCGCQ00851993 - (Port_Complete) - Patrol Read Properties window does not pop up on MSM
SCGCQ00853534 - (Port_Complete) - L2 unrecoverable cache error was seen during Patrol read properties modification in certain conditions.
SCGCQ00854160 - (Port_Complete) - Controller Reboots after doing an OCR with IOs running in the background
SCGCQ00854164 - (Port_Complete) - Controller cache fails to destage when multiple SVDs are present
SCGCQ00854165 - (Port_Complete) - Controller cache fails to destage when multiple SVDs are present
SCGCQ00854168 - (Port_Complete) - Controller cache fails to destage when multiple SVDs are present
SCGCQ00854169 - (Port_Complete) - Controller cache fails to destage when multiple SVDs are present
SCGCQ00854170 - (Port_Complete) - Controller cache fails to destage when multiple SVDs are present
SCGCQ00869785 - (Port_Complete) - Fault LED support for predictive failure drives for SGPIO
SCGCQ00873092 - (Port_Complete) - FW allows CCVD deletion with pinned windows
SCGCQ00873093 - (Port_Complete) - FW allows CCVD deletion with pinned windows
SCGCQ00873094 - (Port_Complete) - FW allows CCVD deletion with pinned windows
SCGCQ00878362 - (Port_Complete) - Code collab fixes delivered
SCGCQ00878401 - (Port_Complete) - Cleanup device wait queue if drive is no longer online
SCGCQ00882474 - (Port_Complete) - Disable FLR support in MR FW to address VMware guest VM abrupt shutdown issue
SCGCQ00886272 - (Port_Complete) - Windows BSOD when upgrade FW 24.6.0-0040 to 24.8.0-0026 with driver 6.707.08.00
SCGCQ00886665 - (Port_Complete) - disableImmediateIO is not reflected in FW
SCGCQ00886666 - (Port_Complete) - disableImmediateIO is not reflected in FW
SCGCQ00886826 - (Port_Complete) - Need to set perfTunerMode appropriately on controller reset.
SCGCQ00889407 - (Port_Complete) - MonTask: line 245 in file ../../raid/1078int.c while running I/Os with 64VDs and pull out drives belonging to CacheCade VD
SCGCQ00889884 - (Port_Complete) - MonTask: line 245 in file ../../raid/1078int.c while running I/Os with 64VDs and pull out drives belonging to CacheCade VD
SCGCQ00891282 - (Port_Complete) - Recon VD made "degraded" when the recon pd is pulled out allowing for rebuild once the drive is plugged back in.
SCGCQ00891288 - (Port_Complete) - Cisco - Colusa1 MonTask after Initiating a Raid Level migration
SCGCQ00908121 - (Port_Complete) - on creating 240VD and rebooting the server, FW breaks into montask.
SCGCQ00908153 - (Port_Complete) - LUID gets changed during foreing import from non-240VD FW to 240VD FW
SCGCQ00914823 - (Port_Complete) - Created VD configuration with PDs released from previous VD erased will lost after next reboot
SCGCQ00803718 - (Port_Complete) - Ctrl-r and HII does not show proper message when you try to import the 65th VD.
SCGCQ00838560 - (Port_Complete) - MR6.8_FW : Unable to Convert a JBOD PD to UG in Solaris
SCGCQ00843936 - (Port_Complete) - Handling Functional Level Reset (FLR) .
SCGCQ00844446 - (Port_Complete) - Enable I2C clock frequency of 100kHz for specific OEM is not working accurately
SCGCQ00844447 - (Port_Complete) - Handle enabling disk "write" cache setting from OS for OEM
SCGCQ00846479 - (Port_Complete) - Secure Erase on SATA SSD via CtrR or HII leads to unresponsive application, Secure erase failing intermittently
SCGCQ00849580 - (Port_Complete) - Failed to import iMR RAID configuration to 12G MR
SCGCQ00850924 - (Port_Complete) - MR & iMR FW Work-around is required for 3x08 chip Errata ID - 2012-RC714 for PCIE 3.0 compliance
SCGCQ00853537 - (Port_Not_Required) - L2 unrecoverable cache error was seen during Patrol read properties modification in certain conditions.
SCGCQ00854177 - (Port_Complete) - Vd erase does not resume after reboot in the presence of CCVD
SCGCQ00871400 - (Port_Complete) - Fault LED support for predictive failure drives for SGPIO
SCGCQ00886271 - (Port_Complete) - Windows BSOD when upgrade FW 24.6.0-0040 to 24.8.0-0026 with driver 6.707.0
SCGCQ00887602 - (Port_Complete) - MR 6.8 : Few test cases fail when Intel PCIeCV tool is executed
SCGCQ00895459 - (Port_Complete) - Removal of "LdDcmd ***** return pinned list 0" spam in FW logs.
SCGCQ00844068 - (Port_Complete) - iMR:6.5-Exception in core 0 is seen when drives are spun down and an ocr is triggered
SCGCQ00844152 - (Port_Complete) - FW doesn't poll all temp sensor channels every 5 seconds
SCGCQ00853147 - (Port_Complete) - Continuous "TASK_ABORT_INTERNAL" prints observed in FW, after running heavy IO's on JBOD configured using 12Gig SAS SSD
SCGCQ00868527 - (Port_Complete) - MR 6.9 : Controller boots to OS Even when Pinned Cache is present and Boot Error handling is set to Stop on Error.
SCGCQ00870846 - (Port_Complete) - FW unable to detect the inserted drives
SCGCQ00876154 - (Port_Complete) - SAS and SATA HDD R0 and R10 1M performance regressions (-15% to -35%) at QD16 to QD256
SCGCQ00882149 - (Port_Complete) - StorCLI reports success on 4MB MR FW package flashing on iMR only controller.
SCGCQ00884719 - (Port_Complete) - 'Fw initializing devices' hangs on controller with specific failed drives on backplane
SCGCQ00891273 - (Port_Complete) - Megaraid Thunderbolt controller reports cache memory size as 0 when no logical drives are present.
SCGCQ00841533 - (Port_Complete) - Instruction TLB error seen when auto configuration command exectued from CLI application
SCGCQ00843390 - (Port_Complete) - Megaraid-sas driver hang with Falcon card
SCGCQ00851886 - (Port_Complete) - MSM displays error message if 'Schedule Consistency Check' is selected.
SCGCQ00892136 - (Port_Complete) - MR 6.6.3 "storcli /c0 show all" shows lot of bad block messages in the log
SCGCQ00835227 - (Port_Complete) - STASH firmware entered fault state with SSD drive
SCGCQ00872263 - (Port_Complete) - Fw crash and BIOS RSODs when VD1 deleted with recon on a PI VD(VD2) and Slow init on VD3.
SCGCQ00841772 - (Port_Complete) - MR firmware reports no smart error when attaching a PFA drive
SCGCQ00876142 - (Port_Complete) - FW unable to detect the inserted dr

BIOS:
SCGCQ00879731 - (Closed) - Legacy OpROM: Handle the conditions for battery failed state as per the Battery design do
SCGCQ00882729 - (Closed) - Legacy OpROM: Controller POST shows JBOD found on host adapter, when number of INT13 device is > deviceExposure
SCGCQ00866982 - (Closed) - Legacy OpROM: Overlapping seen in POST in presence of two controllers and foreign config during CTRL-H laun
SCGCQ00834718 - (Closed) - PNPs and support for 16 port 12G designs

NVDATA:
Numerous changes for specific customers

UEFI Driver:
SCGCQ00898506 - (Closed) - OS doesn't boot after installing OS on the 100th VD , while having 240 VDs created in EFI mod
SCGCQ00834720 - (Closed) - PNPs and support for 16 port 12G designs

HII:
SCGCQ00844774 - (Closed) - Handle coverity defects
SCGCQ00880737 - (Closed) - Handled the coverity defects.
SCGCQ00892931 - (Closed) - Not able to set Controller properties
SCGCQ00896827 - (Closed) - Cannot convert the state of drive from JBOD to UG if the drive is not 16byte CDB
SCGCQ00825741 - (Closed) - UEFI Driver: Compilation error when debug Flags are enabled
SCGCQ00852480 - (Closed) - "Question value mismatch type!Press Enter" message is displayed while entering create virtual drive page
SCGCQ00878350 - (Closed) - HII Enclosure Management form multiple time navigation results in hang/multiple entries of enclosure seen
SCGCQ00879673 - (Closed) - HII: Add GUID check for bootable drive
SCGCQ00894460 - (Closed) - Controller status inconsistency between Dashboard and Controller management in HII
SCGCQ00915093 - (Closed) - HII: Updating LargeIOSupport as per the new API changes
SCGCQ00870398 - (Closed) - Incomplete Port enumeration i.e connector information is displayed for ESM and PD's in HII
SCGCQ00873973 - (Closed) - Profile Based DHS creation grayed out
SCGCQ00879726 - (Closed) - HII: Handle the conditions for battery failed state as per the Battery design doc
SCGCQ00889780 - (Closed) - HII: Address review comments
SCGCQ00903490 - (Closed) - HII RLM for only R0 available when 18 or more drives are present
SCGCQ00860564 - (Closed) - In Make UG warning message OS JBOD drives are not listed
SCGCQ00898506 - (Closed) - OS doesn't boot after installing OS on the 100th VD , while having 240 VDs created in EFI mode
SCGCQ00881426 - (Closed) - VD properties does not display Emulation type.
SCGCQ00893928 - (Closed) - HII: Address review comment
SCGCQ00834719 - (Implemented) - PNPs and support for 16 port 12G designs
SCGCQ00834720 - (Closed) - PNPs and support for 16 port 12G designs
SCGCQ00844917 - (Implemented) - OEM requesting to do a WRITE VERIFY prior to flushing cache. This needs to be managed via CLI
SCGCQ00893152 - (Closed) - HII: Add support to enable/Disable of Large IO Support
SCGCQ00828031 - (Implemented) - Add support to detect that an OS is installed on a JBOD
SCGCQ00854621 - (Closed) - Provide a more descriptive port enumerati
SCGCQ00888846 - (Port_Complete) - HII: Spelling mistakes in strings
SCGCQ00893220 - (Port_Complete) - Inconsistency in showing controller status between MSM and HII for Fake Flash errors
SCGCQ00865978 - (Port_Complete) - Pause for Password at boot time Enable/Disbale based on Boot Mode
SCGCQ00878512 - (Port_Complete) - HII-VD renaming truncates 15th character & allows for 16 characters,though only 15 supported
SCGCQ00882762 - (Port_Complete) - "Question value mismatch type!Press Enter" message is displayed while entering create virtual drive page
SCGCQ00884560 - (Port_Complete) - 13G Exception Screen thrown in uEFI environm

CTRL-R
SCGCQ00873155 - (Closed) - Ctrl-R:Not able to lauch ctrl-R if 2 controllers, one with huawei and another with generic PnP ID is present.
SCGCQ00871350 - (Closed) - Handled the coverity defects.
SCGCQ00837424 - (Closed) - Storcli reports cache type as 'RW' instead of 'R' after R1 CC VD is degraded
SCGCQ00855701 - (Closed) - StorCLI does not find enclosures in multipath environment
SCGCQ00869436 - (Closed) - Include Partition table and GPT GUID check to detect OS/FS
SCGCQ00892967 - (Resolved) - Intruder: The size of the foreign config shown does not match with that after an import.
SCGCQ00893032 - (Closed) - With Liberator the Physical sector size of 512E drive is shown wrong
SCGCQ00853268 - (Resolved) - In EFI, Storcli displaying Bus Number ,Device Number and Function Number = 0 for all the controllers.
SCGCQ00868215 - (Closed) - Connector name field is displayed as & port 4-7 when a single ESM is connected in Multipath
SCGCQ00864200 - (Closed) - Checking in fix for resource leak
SCGCQ00867569 - (Closed) - storcli /c0 vall show is not listing CaC column when CC is not supported and displaying sCC with wrong value.
SCGCQ00870485 - (Closed) - EFI storcli is not working with intruder
SCGCQ00880534 - (Closed) - Invader 6.9 : Efi cli - Command fails with a hang when multiple controllers connected .
SCGCQ00860461 - (Closed) - In JBOD warning message all the drives are getting listed
SCGCQ00881720 - (Closed) - Foreign Config pop up scrollup/down does not respond
SCGCQ00860056 - (Closed) - "storcli show" shows wrong count for aso.
SCGCQ00868198 - (Closed) - Removing Phy information from Enclosure PD details.
SCGCQ00874381 - (Closed) - StorCLI: Memory Leak in function _available_memory_calc1.
SCGCQ00876796 - (Closed) - null pointer dereference
SCGCQ00892129 - (Resolved) - Most of the commands fail with "Invalid argument" error.
SCGCQ00884910 - (Closed) - StorCli Libmods 6.9 coverity fixes
SCGCQ00865108 - (Closed) - Ventura: storcli add vd fails with NVMe
SCGCQ00883409 - (Closed) - Storcli shows the wrong position of enclosures when they are connected in daisy chain with controller
SCGCQ00899384 - (Closed) - Buffer is not incremented when reading sector of the drive
SCGCQ00915164 - (Closed) - CTRL-H: Updating LargeIOSupport as per the new API changes
SCGCQ00889924 - (Closed) - Intruder Port2 and Port3 display are not handled in PD Mngt
SCGCQ00889771 - (Closed) - CTRL-H:Address Review comments
SCGCQ00881936 - (Closed) - Ctrl-R doesnot show the controller name above the menu 
SCGCQ00850607 - (Closed) - added new command /c0 show swalilog equivalent to adpalilog
SCGCQ00834721 - (Implemented) - PNPs and support for 16 port 12G designs
SCGCQ00854633 - (Implemented) - Add details of pending FW images to StorCLI/sho adpinfo
SCGCQ00859740 - (Implemented) - RRB 88: Provide a more descriptive port enumeration (Libmods changes)
SCGCQ00893498 - (Closed) - LibMods: Add support to enable/Disable of Large IO Support - 1 MB IO
SCGCQ00893153 - (Closed) - CTRL-H: Add support to enable/Disable of Large IO Support
SCGCQ00854622 - (Closed) - Provide a more descriptive port enumeration
SCGCQ00850636 - (Closed) - Added support for flashing the FW on intruder and new Dev-ID's of Invader are added for EFI.
SCGCQ00828032 - (Implemented) - Add support to detect that an OS is installed on a JBOD
SCGCQ00853218 - (Implemented) - Add support to detect that an OS is installed on a JBOD
SCGCQ00844918 - (Implemented) - OEM requesting to do a WRITE VERIFY prior to flushing cache. This needs to be managed via CLI
SCGCQ00854626 - (Closed) - Provide a more descriptive port enumera
SCGCQ00904852 - (Port_Complete) - Checking-in changes for defect-SCGCQ00904794
SCGCQ00857695 - (Port_Complete) - Consistent Sorting of Controllers for End Users in Customer Facing Tools (EFI storcli)
SCGCQ00873795 - (Port_Complete) - CTRL-H: MonTask - line 243 in file ../../raid/1078int.c during rebuild
SCGCQ00854296 - (Port_Complete) - Add Pause For Password feature in CTRLH
SCGCQ00853654 - (Port_Complete) - Libmods implementation for WRITE VERIFY prior to flushing cache.
SCGCQ00878517 - (Port_Complete) - CTLR_R: PI-DG : After break mirror, data protection shown as "NA"
SCGCQ00900172 - (Port_Complete) - Added the iMR cutlass PNP id's(0x1000/0052h, 0x1000/0x0053h) to EFI controller explorer class.
SCGCQ00901264 - (Port_Complete) - MR 6.8: storcli reports legacy driver version when native driver is loaded for a Fury controller in ESXi 6.0
SCGCQ00853586 - (Port_Complete) - Get and Set Factory settings Failure
SCGCQ00850019 - (Port_Complete) - storcli /c0/eall/sall show smart command gives all zeros in the output
SCGCQ00849728 - (Port_Complete) - LibMOD:OEM requesting to do a WRITE VERIFY prior to flushing cache.
SCGCQ00878555 - (Port_Complete) - Ctrl-R is creating a smaller VD than specified when selecting a VD size in TB
SCGCQ00867486 - (Port_Complete) - Changed the Message for Hiding Boot VD Operation Status as per FW return error status.
SCGCQ00854279 - (Port_Complete) - Add Pause For Password feature in CTRLH
SCGCQ00893015 - (Port_Complete) - Inconsistency in showing controller status between MSM and Ctrl-R for Fake Flash errors
SCGCQ00874679 - (Port_Complete) - storcli doesnt display E252/E253 enclosure info on an 84016
SCGCQ00894487 - (Port_Complete) - Inconsistency in showing controller status between MSM and StorCLI for Fake Flash errors
SCGCQ00841286 - (Port_Complete) - Storcli : The bus error message is displaying for storcli /c0/eall/sall show smart comm


Installation:
=============
Use StorCLI to flash the SAS controllers.  These tools can be downloaded from the support and download
section of www.lsi.com.

Command syntax:  
StorCLI /c0 download file=mr3108fw.rom







SAS MegaRAID Firmware Release for MegaRAID Controllers
Release date: 07/13/15


Version Numbers:	
===============
Current Package Details:
Firmware Package:24.9.0-0022 (MR 6.8)
Firmware 4.290.00-4536
ROMENV 1.09
BootBlock 3.07.00.00-0002
NVDATA  3.1507.00-0006
UEFI_Driver 0x060E0300 (SIGNED)
Hii v03.14.09.00 (SIGNED)
FCODE 4.17.08.00
BIOS 6.25.03.0
Ctrl-R 5.10-0700
PCLI 1.07.05

Previous Package Details:
Firmware Package:24.8.0-0020 (MR 6.7)
Firmware 4.280.00-4226
ROMENV 1.09
BootBlock 3.07.00.00-0002
NVDATA  3.1503.00-0005
UEFI_Driver 0x060D0200 (SIGNED)
Hii v03.13.09.00(SIGNED)
FCODE 4.17.08.00
BIOS 6.24.05.0
Ctrl-R 5.08-0006
PCLI 1.07.05


Bug Fixes and Enhancements:
===========================
Firmware:
SCGCQ00781736 - (Closed) - Customer ROMB design GPIO/SGPIO drive LED question
SCGCQ00808221 - (Closed) - Correctable ECC errors are not getting detected.
SCGCQ00819314 - (Closed) - SSDs getting data with bad PI CRC.
SCGCQ00819811 - (Closed) - When consistency check is aborted/suspended, HBA resets
SCGCQ00825126 - (Closed) - Unexpected controller reset during test run
SCGCQ00825568 - (Closed) - Montask at Line 108 in ../../raid/span.c while configuring PR11/R0 CCVD using 1.4 TB SSD's
SCGCQ00825602 - (Closed) - Function isCcvdOkToImport was failing the import
SCGCQ00826884 - (Closed) - During one MB IO’s along with background flush causing the chainframe(MID) getting leaked leads to Montask.
SCGCQ00828327 - (Closed) - OEM check for SCGCQ00762968 fix as it is only for OEM.
SCGCQ00829214 - (Closed) - MR firmware exposes more than 240 VD's to the host, even when the host driver doesn't support more than 64VD's.
SCGCQ00829218 - (Closed) - With 6.7MR driver and 6.8MR fw a kill adapter is observed while IO in progress and importing of degraded VD.
SCGCQ00830847 - (Closed) - Block CCVD creation if the number of CCVd’s > 1 and CCVD’s are associated with SVD
SCGCQ00835586 - (Closed) - Instruction TLB error seen when auto configuration command exectued from CLI application
SCGCQ00835725 - (Closed) - Source VD of Config2 [2G-CTRL] fails to imports in Config1 [1G-CTRL]
SCGCQ00837878 - (Closed) - Firmware halted and restarted while doing flash erase on the onfi flash
SCGCQ00837937 - (Closed) - Fail to set read and write command timer for multiple SATA drives.
SCGCQ00839323 - (Resolved) - Authentication Raid key Failed! err:1 error while issuing OCR with IOs on multiple VDs
SCGCQ00841359 - (Closed) - Rebuild Performance for RAID 1 arrays is slower.
SCGCQ00841512 - (Closed) - Multi CCVD import fails after FW downgrade from MR 6.8 to 6.7
SCGCQ00842625 - (Closed) - Controller cache fails to destage when multiple SVDs are present
SCGCQ00842804 - (Closed) - CacheCade allows the user to create a as small as 32-MB
SCGCQ00844101 - (Closed) - Reverting Simplified Buffer Manager Code Changes
SCGCQ00844102 - (Closed) - Mismatch in the CCVD size after importing the CCVD configuration from MR 6.7 to MR 6.8
SCGCQ00844698 - (Closed) - Deleting a Cachecade VD (CC VD) results in a firmware hang situation.
SCGCQ00844838 - (Closed) - Pd counters are reset to zero on every iteration.
SCGCQ00845569 - (Closed) - Observed drops around 15-25 % across all RAID levels in many areas for 1MB stripe size
SCGCQ00845695 - (Closed) - FW gives wrong warning message"Warning!!! no free slot in nvram" in the logs
SCGCQ00851230 - (Closed) - MR6.8 Alpha SSD Random Read/Write performance regressions (15-45%) vs MR6.7GCA
SCGCQ00852739 - (Closed) - MR6.8 Alpha SAS HDD Random Write performance regressions (15-35%) vs MR6.7GCA
SCGCQ00855258 - (Closed) - Compilation warning occurring due to usage of inline boolean macro
SCGCQ00856313 - (Closed) - Undo the changes made for defect SCGCQ00837917 [DISM stuck at device discovery on enclosure power cycle]
SCGCQ00860270 - (Closed) - FW unable to detect the inserted drives
SCGCQ00867117 - (Closed) - OFU fails when FW downgraded from 6.8 to 6.7(GCA)
SCGCQ00869551 - (Closed) - SAS and SATA HDD R0 and R10 1M performance regressions (-15% to -35%) at QD16 to QD256
SCGCQ00879124 - (Closed) - Cache bypass algorithm bypasses sequential writes even when there are no sufficient writes to bypass cache
SCGCQ00820519 - (Closed) - Performance drop seen with 1MB + SBM compared against SBM as base code.
SCGCQ00821359 - (Closed) - With IO in progress a Data TLB error is seen on performing background operations.
SCGCQ00824415 - (Closed) - Missed to memset the datastructure used to populate the devhandle
SCGCQ00825797 - (Closed) - Performing a cable pull/push result to Data TLB Error at "RaidIoWriteOver+684".
SCGCQ00827713 - (Closed) - Certian CCVDs created using older FW cannot be properly import on to MR6.8
SCGCQ00831369 - (Closed) - FW doesn't allow auto/foreign import of CCVDs created on MR6.7 or earlier systems
SCGCQ00831398 - (Closed) - Deleting a Cachecade VD (CC VD) results in a firmware hang situation.
SCGCQ00834552 - (Closed) - Unable to Convert a JBOD PD to UG in Solaris
SCGCQ00836496 - (Closed) - Performing a cable pull/push with array property change resulting into FW hang.
SCGCQ00837917 - (Resolved) - DISM stuck at device discovery on enclosure power cycle, Devices present with DM but not reflected in upper layers
SCGCQ00838222 - (Closed) - DATA TLB seen when trying to offline a drive from R1 virtual drive
SCGCQ00838953 - (Closed) - Deleting a Cachecade VD (CC VD) results in a firmware hang situation.
SCGCQ00839635 - (Closed) - chain element for non RW commands were not pulled in the FW
SCGCQ00839936 - (Closed) - FW crash observed, when trying to destage the Pinned Cache
SCGCQ00841317 - (Closed) - Secure Erase on SATA SSD via CtrR or HII leads to unresponsive application, Secure erase failing intermittently
SCGCQ00845245 - (Closed) - Reverting code changes done in SSD Metadata
SCGCQ00853558 - (Closed) - On performing a SATA drive pull/push operation less than 4sec, result to Read/write command timer set to drive default value.
SCGCQ00854856 - (Closed) - Assertion failure while restoring Pinned data with least latency mode switch
SCGCQ00857115 - (Closed) - Pd counter "last 8hour ago" is not propagating/copying to "16hour ago" after reboot.
SCGCQ00862519 - (Closed) - Disabling 1MB IO support
SCGCQ00864181 - (Closed) - CID 16728, Uninitialized pointer read results in DATA TLB error
SCGCQ00763934 - (Closed) - Storcli show device link speed is confused for SATA/SAS drive when connected expander have buffer feature enable
SCGCQ00797643 - (Closed) - FW hung at LogInit: Flushing events from previous boot while running policy change script of Vd and learn cycles.
SCGCQ00800589 - (Closed) - Unexpected all device insert event causes logical state change and VD deletion
SCGCQ00812842 - (Closed) - Firmware will POST bios message when there is a romId mismatch and no features present on the controller
SCGCQ00832774 - (Closed) - Sgl frames crunch observed with Random larger IO's
SCGCQ00833765 - (Closed) - Failed to import iMR RAID configuration to 12G MR
SCGCQ00835377 - (Closed) - With MR6.8 firmware, A phantom LD is being created when LD 0 is created.
SCGCQ00836103 - (Closed) - Incorrect error returned by FW when when PDs with different block size are mixed.
SCGCQ00840587 - (Closed) - Introduce macro and inline function to distinguish between OEM Rack Server and OEM Blade Server
SCGCQ00845703 - (Closed) - FW is setting wrong recovery time Limit in SAS/SATA drives, when detection type is 3 and recoveryTimeLimit is 0 in Nvdata
SCGCQ00863066 - (Closed) - CCVD size inconsistency across FW upgrade to 6.8 and downgrade to lower FW version
SCGCQ00798701 - (Closed) - 4K virtual drive missing across power cyle on iMR controller
SCGCQ00818560 - (Closed) - FW should not block manual check consisteny operation on excluded VDs
SCGCQ00820037 - (Closed) - PL Fault hit while performing Reconstruction.
SCGCQ00828174 - (Closed) - firmware will get Kill Adapter at reboot or power on.
SCGCQ00828305 - (Closed) - Missing/offline PDs in a R0 CCVD to be marked as offline
SCGCQ00830541 - (Closed) - DATA TLB error while unblocking SVD
SCGCQ00830918 - (Closed) - EFI driver health fails when more than 64VDs configured
SCGCQ00836500 - (Closed) - Release buffers appropriately on volume deletion
SCGCQ00850961 - (Closed) - Tuning the Debug Infrastructure for testing Predictive Failure PR
SCGCQ00853249 - (Closed) - FW hangs on changing the Write policy of CCVD
SCGCQ00856310 - (Closed) - Fw hits to MonTask: line 325 in file ../../raid/mem.c while spin up drive.
SCGCQ00822403 - (Closed) - Fw hits to MonTask: line 1272 in file ../../raid/1078dma.c while running IO in VM
SCGCQ00823876 - (Closed) - Fix group code review issues.
SCGCQ00825725 - (Closed) - FW upgrade from non 240VD FW to 240VD FW when OS is behind the controller results in BSOD
SCGCQ00832596 - (Closed) - R10 performance with large block IOs has a large drop while scaling QD with 12Gb/s SAS HDDs
SCGCQ00851810 - (Closed) - Vd erase does not resume after reboot in the presence of CCVD
SCGCQ00852019 - (Closed) - Handling of ONFI Transport case with different Performance Tuner Modes.
SCGCQ00822356 - (Closed) - Fixed build issues from merge.
SCGCQ00828781 - (Closed) - Controller goes into a deadlock when a Logical Drive (LD) is deleted during foreground initialization
SCGCQ00835359 - (Closed) - Controller Reboots after doing an OCR with IOs running in the background
SCGCQ00836381 - (Closed) - ssdDebug to be disbled by default
SCGCQ00843579 - (Closed) - Unexpected behaviour in VD erase after FW upgrade
SCGCQ00845506 - (Closed) - FW is setting Recovery time limit, read and write command timer for SSD drives.
SCGCQ00829098 - (Closed) - added condition check avoid calling the ssdModifyMagicBlock() in case of missing VD’s across reboot/ocr
SCGCQ00837454 - (Closed) - User can create CCVDs whose size can exceed maximum configurable CacheCade size
SCGCQ00846735 - (Closed) - Host TM active flag is not cleared once the target reset completes on JBOD
SCGCQ00850943 - (Closed) - Unable to delete CCVD after foreign import
SCGCQ00827732 - (Closed) - FW hits to MonTask: line 4538 in file ../../raid/cache.c on discarding Preserved Cache
SCGCQ00831819 - (Closed) - Add the forward compatibility bit in DDF to avoid importing CCVD on legacy firmware.
SCGCQ00728066 - (Closed) - update copyright info
SCGCQ00846677 - (Closed) - port latency improvements from development stream
SCGCQ00842239 - (Closed) - Modified SSD Metadata to store number of cache windows generated
SCGCQ00823759 - (Closed) - Increase maximum cache size for Cachecade to 2048GB.
SCGCQ00820593 - (Closed) - Program CVFM(Cache Vault Flash Module) VPD without Supercap connected.
SCGCQ00816361 - (Closed) - Task management support for JBOD/sysPD
SCGCQ00812722 - (Closed) - Single write COL with FBU03 for OEM
SCGCQ00806537 - (Implemented) - Use config sequence number to SYSTEM PD fastpath IOs
SCGCQ00770194 - (Closed) - Include learn cycle failure debug command in FW.
SCGCQ00823470 - (Closed) - Monitoring Drive Performance
SCGCQ00820067 - (Closed) - Request to remove the repeated ROC temperature warnings in ttylog when above 104 deg C.
SCGCQ00817914 - (Implemented) - Refactor Buffer Manager to avoid overheads with various lists
SCGCQ00812724 - (Closed) - FW change for single write to be fully supported for 2:4.
SCGCQ00792582 - (Closed) - Event for LED locate start and stop
SCGCQ00758184 - (Closed) - GG update to include concatenated GG/VPD data for Invader product generation.
SCGCQ00758178 - (Closed) - MegaRAID CPLD update improvements
SCGCQ00824803 - (Closed) - CCVD size parameters have to be handled properly and stored in the DDF
SCGCQ00820055 - (Closed) - CacheCade changes for SBM
SCGCQ00816316 - (Implemented) - Large I/O Suport - suport 1MB transfer size
SCGCQ00839643 - (Closed) - Add strict sequentiality check in cache bypass algorithm
SCGCQ00825197 - (Implemented) - Add Log Latency Framework
SCGCQ00823063 - (Implemented) - Create build environment for MR 6.8 stream
SCGCQ00820329 - (Implemented) - Decouple MR_FW_RAID_MAP update from Command block
SCGCQ00816307 - (Implemented) - Reduce retries for timed-out FastPath I/O’s ( enable CTIO and FP)
SCGCQ00806517 - (Closed) - Add set "Fail PD on SMARTer" property feature to StorCLI
SCGCQ00784955 - (Port_Complete) - Virtual Disk GUID field changes when a VD is moved. The LUID is supposed to be unique and invariant.
SCGCQ00790037 - (Port_Complete) - Firmware logs are not dumped to flash during device discovery phase
SCGCQ00791671 - (Port_Complete) - Command timeout happens though the response returns in 130ms.
SCGCQ00791672 - (Port_Complete) - Command timeout happens though the response returns in 130ms.
SCGCQ00804284 - (Port_Complete) - Calculation for minimum blocks required to offload is wrong for single image configuration.
SCGCQ00806806 - (Port_Complete) - HII hangs for several minutes when entering the security key in for a locked PD
SCGCQ00813167 - (Port_Complete) - Offload timed out for single image configuration
SCGCQ00813744 - (Port_Complete) - Offload timed out for single image configuration
SCGCQ00814987 - (Port_Complete) - GG update to include concatenated GG/VPD data for Invader product generation.
SCGCQ00814997 - (Port_Complete) - Correctable ECC errors are not getting detected.
SCGCQ00821670 - (Port_Complete) - Reduce the clean up time of all the IOs from a host that is powered off.
SCGCQ00822131 - (Port_Complete) - Immediate IO failed in write back cache recovery code 
SCGCQ00822235 - (Port_Complete) - Reduce PD time out value from 12 seconds to 8 Seconds
SCGCQ00822481 - (Port_Complete) - Feature to retrieve the TTY logs compressed
SCGCQ00822642 - (Port_Complete) - Virtual Disk GUID field changes when a VD is moved. The LUID is supposed to be unique and invariant.
SCGCQ00823448 - (Port_Complete) - Fix for crash with Raid 5 write through
SCGCQ00824818 - (Port_Complete) - Megaraid_sas driver fails to communicate with the FW and fails to discover any disks attached
SCGCQ00825773 - (Port_Complete) - OS (CentOS 7.0) crash observed while doing online FW update on IMR Fury controller
SCGCQ00825774 - (Port_Complete) - Background IO's on 235 R0 VD's and abrupt enclosure power cable pull resulting into Fatal FW error
SCGCQ00839018 - (Port_Complete) - After successful reconstruction of VDs, they are not getting reflected in MSM unless the user reboots the system
SCGCQ00839974 - (Port_Complete) - To support secondary key on baseboard to enable fearures for iMR cards
SCGCQ00840631 - (Port_Complete) - MegaRAID CPLD update improvements
SCGCQ00787362 - (Port_Complete) - Firmware logs are not dumped to flash during device discovery phase
SCGCQ00789739 - (Port_Complete) - Virtual Disk GUID field changes when a VD is moved. The LUID is supposed to be unique and invariant.
SCGCQ00791673 - (Port_Complete) - Command timeout happens though the response returns in 130ms.
SCGCQ00813062 - (Port_Complete) - Offload timed out for single image configuration
SCGCQ00820086 - (Port_Not_Required) - SVD's are getting 'Access Blocked' after OCR followed by System Reboot
SCGCQ00820917 - (Port_Complete) - 95% longer boot time compared to shipping stream
SCGCQ00821672 - (Port_Complete) - Host IO may get an error - code review defect
SCGCQ00821693 - (Port_Complete) - Controller commands are getting failed resulting in application hang when Logical Drive (LD) is deleted during reconstruction
SCGCQ00822182 - (Port_Complete) - IO completion may not happen because of earlier aborts
SCGCQ00822184 - (Port_Complete) - Crash when completing Abort.
SCGCQ00822315 - (Port_Complete) - Remove unnecessary debug prints to console (during dma failure)
SCGCQ00822739 - (Port_Complete) - Incorrect SGL from driver crashes FW (expected) but does not let driver do OCR
SCGCQ00825765 - (Port_Complete) - Command timeouts with cdb=ff ff ff ff
SCGCQ00826083 - (Port_Complete) - Invader MR does not update Expander Information dynamically
SCGCQ00839970 - (Port_Complete) - New event when patrol read is aborted due to conflict with other background operation
SCGCQ00844697 - (Port_Complete) - Deleting a Cachecade VD (CC VD) results in a firmware hang situation.
SCGCQ00844801 - (Port_Complete) - Behavior change when FW hit fault code 0x81 (uncorrectable ECC error)
SCGCQ00797554 - (Port_Complete) - Flash of incorrect GG on controller, does not restore VDs back to WB
SCGCQ00814991 - (Port_Complete) - Include learn cycle failure debug command in FW.
SCGCQ00815618 - (Port_Complete) - FW pkg 23.22.0-0017 and later initialize drives ~50% slower
SCGCQ00820922 - (Port_Complete) - Auto Configure RAID0 DG set to READ AHEAD policy instead of NO READ AHEAD
SCGCQ00821671 - (Port_Complete) - IO may not do error recovery (code review fix)
SCGCQ00821674 - (Port_Complete) - Bad physical drive caused controller error recovery go in loop
SCGCQ00825775 - (Port_Complete) - FW breaks into montask while making VDs offline when rebuild is going on with IOs
SCGCQ00826980 - (Port_Complete) - Single OEM card reporting SDRAM Unrecoverable Error
SCGCQ00829706 - (Port_Complete) - SSDs fall offline after reset under heavy IO.
SCGCQ00829929 - (Port_Complete) - Storcli show device link speed is confused for SATA/SAS drive when connected expander have buffer feature enable
SCGCQ00832121 - (Port_Not_Required) - Controller goes into a deadlock when a Logical Drive (LD) is deleted during foreground initialization
SCGCQ00838186 - (Port_Complete) - Makefile Changes to include the macro by default
SCGCQ00840009 - (Port_Complete) - IO freeze on R5 while running host IO with BGI
SCGCQ00853535 - (Port_Complete) - L2 unrecoverable cache error was seen during Patrol read properties modification in certain conditions.
SCGCQ00818815 - (Port_Complete) - Battery Failure observed when upgrading FW from previous versions to latest one.
SCGCQ00821002 - (Port_Complete) - Handling DMA Errors and Write Back Cache Recovery for new program
SCGCQ00821667 - (Port_Complete) - Support in Device module to handle DMA errors
SCGCQ00822081 - (Port_Complete) - This ER is to support DMA failure from SysDma
SCGCQ00822227 - (Port_Complete) - Crash in FW because of two commands having same SMID.
SCGCQ00822321 - (Port_Complete) - Host IO did not complete
SCGCQ00839973 - (Port_Complete) - Invalid event "Consistency Check done on VD:255" coming when CC is running on a VD and VD is deleted
SCGCQ00840019 - (Port_Complete) - Observing I/O stalls for longer duration in firmware version with throttling changes introduced
SCGCQ00844704 - (Port_Complete) - Deleting a Cachecade VD (CC VD) results in a firmware hang situation.
SCGCQ00814989 - (Port_Complete) - MegaRAID CPLD update improvements
SCGCQ00821694 - (Port_Not_Required) - Host abort Command Implementation
SCGCQ00822140 - (Port_Complete) - Hitting Assert in flush logic while doing write back cache recovery in code
SCGCQ00861251 - (Port_Complete) - Observing I/O stalls for longer duration in firmware version with throttling changes introduced
SCGCQ00824799 - (Port_Complete) - Patrol Read Properties window does not pop up on MSM
SCGCQ00835242 - (Port_Complete) - Failed to import iMR RAID configuration to 12G MR
SCGCQ00844085 - (Port_Complete) - Report controller flash device health status
SCGCQ00818816 - (Port_Complete) - Removing OV workound for superCaps
SCGCQ00822166 - (Port_Complete) - Improper handling of Redirtied bit pattern during write back cache recovery
SCGCQ00829961 - (Port_Complete) - Firmware will POST bios message when there is a romId mismatch and no features present on the controller
SCGCQ00845690 - (Port_Complete) - MSM displays error message if 'Schedule Consistency Check' is selected.

BIOS:
SCGCQ00826174 - (Closed) - 64VDs found on Host adapter eventhough more than 64 VDs are present
SCGCQ00845247 - (Closed) - Overlap of controller boot messages with the footage message.
SCGCQ00826176 - (Port_Complete) - 64VDs found on Host adapter eventhough more than 64 VDs are present

NVDATA:
Numerous changes for specific customers

UEFI Driver:
Defects (2)
SCGCQ00844774 - (Closed) - Handle coverity defects
SCGCQ00825741 - (Closed) - Compilation error when debug Flags are enabled
SCGCQ00813457 - (Closed) - Rebranding effort for OEM

HII:
SCGCQ00820006 - (Closed) - Address review comments
SCGCQ00825573 - (Closed) - Create Cache Cade VD option still available even after MaxConfgiureSSCSize is crossed.
SCGCQ00852480 - (Closed) - "Question value mismatch type!Press Enter" message is displayed while entering create virtual drive page
SCGCQ00816666 - (Closed) - Handle CCVD Changes Based on new MR.h bit supportExtendedSSCSize
SCGCQ00830577 - (Closed) - on doing manage SSD caching, the landing page takes to VD management page
SCGCQ00832946 - (Closed) - In the Reconfigure VD, suppress the Add Drives operation based on the UG drives available.
SCGCQ00844160 - (Closed) - Allow CCVD Creation only if we have more than 1 GB space.
SCGCQ00828425 - (Closed) - The help string for maintain PD fail history is not appropriate
SCGCQ00828433 - (Closed) - No description or help for vd status field in HII
SCGCQ00829216 - (Closed) - HII doesn't allow to reconfigure a RAID 6 partically degraded virtual drive to RAID 0
SCGCQ00811352 - (Closed) - Handle Code Collaborator Defect and comments.
SCGCQ00830579 - (Closed) - Raid level gets changed on trying to add a drive to the VD while performing Reconfigure virtual drive.
SCGCQ00844784 - (Closed) - Handle coverity defects
SCGCQ00845541 - (Closed) - Max SSC configurable size not shown
SCGCQ00827376 - (Closed) - the default write policy doesn't change from WB to WT while creating a vd when there is a battery failure.
SCGCQ00828427 - (Closed) - The help string for cache flush interval is not appropriate
SCGCQ00828751 - (Closed) - Manage ssd caching comes under vd property instead of controller property
SCGCQ00838756 - (Closed) - Manage SSD Caching: Empty string seen in warning message
SCGCQ00811295 - (Reworked) - Generic RAID1 Profile based VD creation option is not grayed out after creating 64VD's.
SCGCQ00829208 - (Closed) - In the Reconfigure VD page the help string for the 'New RAID level' is not appropriate
SCGCQ00834097 - (Closed) - Option to migrate from r6 to r0 comes in HII when the VD is in degraded state.
SCGCQ00827315 - (Closed) - Increase maximum cache size for Cachecade to 2048GB. This will be named CC 2.5
SCGCQ00818001 - (Implemented) - Rebranding effort for OEM - Changes outside PNP ID addition
SCGCQ00816310 - (Implemented) - HII & MSM Mismatch on write-back options - UI Inconsistancy issue
SCGCQ00738144 - (Closed) - Code Redundancy in firing MR_DCMD_CTRL_GET_INFO
SCGCQ00789492 - (Closed) - Support decimal fraction for PD/VD size in HII
SCGCQ00804071 - (Closed) - Code refactor: Check return code of HiiGetString()
SCGCQ00816305 - (Implemented) - Add "Remove Drives" option during Raid Level Migration
SCGCQ00813457 - (Closed) - UEFI Driver: Rebranding effort for OEM
SCGCQ00818583 - (Implemented) - Provide richer enclosure related information in the MegaRAID HII Enclosure Management pages.
SCGCQ00805041 - (Port_Complete) - how error message when user clicks on Apply Change wihout choosing drive group
SCGCQ00817320 - (Port_Complete) - PD Remove option is not available for offline drive
SCGCQ00819329 - (Port_Complete) - Show error message when user clicks on Apply Change wihout choosing drive group
SCGCQ00816978 - (Port_Complete) - Prepare For Removal" on PD does not work w/pending PD operations (HII)
SCGCQ00816998 - (Port_Complete) - HII drive menu does not show 0MB drives
SCGCQ00817317 - (Port_Complete) - HII does not provide assigned group array info for dedicated HSP
SCGCQ00817323 - (Port_Complete) - Question value mismatch while Replacing Drive and while view assocaiated Drive Gorup
SCGCQ00817869 - (Active) - Handle CCVD Changes Based on new MR.h bit supportExtendedSSCSize
SCGCQ00817947 - (Port_Complete) - Enclosure properties are not accurate in HII
SCGCQ00817018 - (Port_Complete) - Enclosure properties are not accurate in HII
SCGCQ00817316 - (Port_Complete) - HII drive menu does not show 0MB drives
SCGCQ00826109 - (Port_Complete) - Create Cache Cade VD option still available even after MaxConfgiureSSCSize is crossed.

CTRL-R
SCGCQ00786895 - (Closed) - The warning message is not shown when user tries to create CCVD greater than max configurable SSC size.
SCGCQ00844775 - (Closed) - Handled the coverity defects.
SCGCQ00843395 - (Closed) - Not able to enter ctrl-R when two controllers are connected with one having subOEM=1
SCGCQ00828788 - (Closed) - CTRL_R PD Page display is not proper, when set up is configured in Multipath mode
SCGCQ00817003 - (Closed) - Handle CCVD Changes Based on new API change
SCGCQ00827049 - (Closed) - Storcli cannot create R10 in iMR with 6 or 8 drives per span.
SCGCQ00827299 - (Closed) - Storcli crashes instead of showing error message on enabling caching on Source VDs and C
SCGCQ00839186 - (Closed) - While toggling previous tab at random midst sequence of forward tab, MonTask is hit
SCGCQ00837197 - (Closed) - Cachevault flash size shows differently for different commands in storcli under RHEL6.6 PPC64
SCGCQ00837342 - (Closed) - New PD_Degraded media events are not logging correctly in PPC
SCGCQ00837219 - (Closed) - Change EnclIndex with EnclosureDevice ID.
SCGCQ00840372 - (Closed) - Read policy should be 'NORA' for IMR controller instead of 'none'
SCGCQ00846882 - (Closed) - Handled the memory corruption.
SCGCQ00820392 - (Closed) - Segmentation fault while querying for GHSP/DHSP while drive is going in shield-HSP state.
SCGCQ00830435 - (Closed) - LDViewMirror is giving segmentation fault
SCGCQ00839321 - (Closed) - Storcli gives wrong error code with respect to FW state while converting JBOD to UG
SCGCQ00845545 - (Closed) - CTRL_R pops up wrong message, when trying to import CCVD configuration after downgrading the FW from 6.8 to 6.7
SCGCQ00844167 - (Closed) - Allow CCVD Creation only if we have more than 1 GB space.
SCGCQ00830269 - (Closed) - storcli /call show all fails with "command invalid"
SCGCQ00835758 - (Closed) - Storcli shows caching is enabled on Source VD when CCVD is in offline state
SCGCQ00839919 - (Closed) - Passphrase fails during post with 2 cards in system if we try to launch CTRL+R in between the cards initilization
SCGCQ00828415 - (Closed) - Make semicolumn is sync with other Rates.
SCGCQ00825003 - (Closed) - CTR_R providing the option to create CCVD, when full size CCVD[512GB] is already configured
SCGCQ00819046 - (Closed) - Wrong PD/VD Size value in CtrlR
SCGCQ00836472 - (Closed) - DATA TLB Error observed when trying to create 2nd sliced VD in Degraded R1 DG using CTRL_R
SCGCQ00818101 - (Implemented) - Add set "Fail PD on SMARTer" property feature to StorCLI
SCGCQ00829204 - (Implemented) - Increase maximum cache size for Cachecade to 2048GB. This will be named CC 2.5
SCGCQ00816303 - (Implemented) - Improve the View of Controller Selection Menu
SCGCQ00818987 - (Closed) - LimMod changes related to CtrlH & MSM Mismatch on write-back options - UI Inconsistancy issue
SCGCQ00828476 - (Closed) - Storcli Should display SAS Address N/A if its invalid and change Host interface type names from PCIX, PCIE to PCI-X, PCI-E
SCGCQ00789493 - (Closed) - Support decimal fraction for PD/VD size in HII
SCGCQ00827665 - (Closed) - Implemented the VD-VF mapping related commands in factory tool
SCGCQ00816311 - (Implemented) - CtrlH & MSM Mismatch on write-back options - UI Inconsistancy issue
SCGCQ00817977 - (Closed) - Monitoring Drive performance and predictive failure
SCGCQ00827316 - (Closed) - Increase maximum cache size for Cachecade to 2048GB. This will be named CC 2.5
SCGCQ00833194 - (Port_Complete) - Command /cx/ex show phyerrorcounters gives bus error in Orcale Enterprise Linux
SCGCQ00824446 - (Port_Complete) - StorCLI when ran on HBA that does not support battery, displays “Missing Battery”. (SCGCQ00820005)
SCGCQ00822503 - (Port_Complete) - Segmentation fault while querying for GHSP/DHSP while drive is going in shield-HSP state.
SCGCQ00832852 - (Port_Complete) - Consistent Sorting of Controllers for End Users in Customer Facing Tools (EFI storcli)
SCGCQ00834687 - (Port_Complete) - Personality mode not present in storclif show all command
SCGCQ00819317 - (Port_Complete) - Wrong PD/VD Size value in CtrlR
SCGCQ00817885 - (Port_Complete) - Handle CCVD Changes Based on new API change
SCGCQ00832372 - (Port_Complete) - Libmods changes for defect SCGCQ00823772: StorCLI version 1.14.14 does not allow access to both expanders
SCGCQ00839833 - (Port_Complete) - StorCli show drive FW command not working correctly


Installation:
=============
Use StorCLI to flash the SAS controllers.  These tools can be downloaded from the support and download
section of www.lsi.com.

Command syntax:  
StorCLI /c0 download file=mr3108fw.rom


Component:
=========
SAS MegaRAID Firmware Release for MegaRAID Controllers
Release date: 04/16/15


Version Numbers:	
===============
Current Package Details:
Firmware Package:24.8.0-0020 (MR 6.7)
Firmware 4.280.00-4226
ROMENV 1.09
BootBlock 3.07.00.00-0002
NVDATA  3.1503.00-0005
UEFI_Driver 0x060D0200 (SIGNED)
Hii v03.13.09.00(SIGNED)
FCODE 4.17.08.00
BIOS 6.24.05.0
Ctrl-R 5.08-0006
PCLI 1.07.05

Previous Package Details:
Firmware Package:24.7.0-0042 (MR 6.6 P1)
Firmware 4.270.00-4183
ROMENV 1.09
BootBlock 3.06.00.00-0001
NVDATA  3.1411.00-0016
UEFI_Driver 0x060B0201 (SIGNED)
Hii v03.11.08.01(SIGNED)
FCODE 4.16.08.00
BIOS 6.22.03.1
Ctrl-R 5.08-0006
PCLI 1.07.05


Bug Fixes and Enhancements:
===========================

Firmware:
SCGCQ00774946 - (Closed) - MCTP over PCI-E: Asseration failure while flashing a FW through PCI-E path.
SCGCQ00783365 - (Closed) - Dev defect to support for Dynamic Discovery
SCGCQ00783813 - (Closed) - Dev defect with Dynamic discovery after OCR all commands from SL are timing out
SCGCQ00785425 - (Closed) - MCTP over PCI-E: GetOobStatus command fails when OOB in resume state.
SCGCQ00785435 - (Closed) - MCTP over PCI-E : Set OOB poll parameters are not reflecting in Get OOB poll
SCGCQ00785564 - (Closed) - MCTP over PCI-E: FW hang is observed, when we fire any MCTP command during OCR
SCGCQ00787768 - (Closed) - Dev defect: datalength calculation for eventing is not same as in i2c
SCGCQ00793028 - (Closed) - Flash of incorrect GG on controller, does not restore VDs back to WB
SCGCQ00793616 - (Closed) - MR 6.7::FW breaks to montask on line /ssd/ssd_cache_fw.c
SCGCQ00794102 - (Closed) - In controller safe mode, still can access existing data and run IO on JBODs (Normal JBOD, Secure JBOD and PI JBOD)
SCGCQ00795015 - (Closed) - In certain conditions foreign import of CacheCade VDs may result in catastrophic failure in FW, incorrect CacheCade VD size display
SCGCQ00798606 - (Closed) - FOREIGN secure JBOD should not be exposed to OS.
SCGCQ00798960 - (Closed) - Change the string "pass phrase" to "password" in all applicable Firmware Boot Messages
SCGCQ00801724 - (Closed) - Automatically Controller Security is getting enabled after OCR
SCGCQ00805295 - (Closed) - During CCVD creation applications may send unaligned size to the FW.
SCGCQ00805661 - (Closed) - MR_6.7: Fw hits MonTask: line 245 in file ../../raid/1078int.c while upgrading the FW
SCGCQ00807500 - (Closed) - Firmware fails to import PRL 11 VD in certain scenarios.
SCGCQ00807514 - (Waiting_Info) - R10 8x HDDs have a large variance in performance with 32K SW 64QD workload
SCGCQ00809660 - (Closed) - 240VD mode SLT displays the Write Cache Capable as YES
SCGCQ00810211 - (Closed) - After successful reconstruction of VDs, they are not getting reflected in MSM unless the user reboots the system
SCGCQ00812608 - (Closed) - Background IO's on 235 R0 VD's and abrupt enclosure power cable pull resulting into Fatal FW error
SCGCQ00812661 - (Closed) - Remove the code changes added as part of CSET SCGCQ00791478
SCGCQ00813616 - (Closed) - 240VD - LD Sync fails while installing Linux OS with inbox driver
SCGCQ00814777 - (Closed) - Command block not getting granted on completing a diverted fast path I/O due to divert lock
SCGCQ00814937 - (Closed) - Users can't change default access policy of SVD when it blocked by SSC removal
SCGCQ00815077 - (Closed) - Secure JBODs are not exposed to the OS if the drive were pushed out and inserted back.
SCGCQ00815569 - (Closed) - MCTPoverPCIE :Firmware part for the defect SCGCQ00797846 :SL throws error 0x7009
SCGCQ00816137 - (Closed) - HII: Generic RAID1 Profile based VD creation option is not grayed out after creating 64VD's.
SCGCQ00817045 - (Closed) - ssdModifyMagicBlock() Copying the VDGUID into wrong buffer.
SCGCQ00820121 - (Closed) - OS (CentOS 7.0) crash observed while doing online FW update on IMR Fury controller
SCGCQ00822477 - (Closed) - MR6.7-Beta:FW hits to MonTask: line 1272 in file ../../raid/1078dma.c after Injecting media error in loop on CCVD metadata
SCGCQ00829214 - (Closed) - MR firmware exposes more than 240 VD's to the host, even when the host driver doesn't support more than 64VD's.
SCGCQ00770120 - (Closed) - MCTP_Firmware: Exception core 0 and MonTask: line 243 in file ../../raid/1078int.c on formating a non existing physical disk
SCGCQ00774000 - (Closed) - PRL11 CCVD import fails with event in FW logs"C0:createMegaraidCfg-Offline VD pinned-this VD may not be fully inserted"
SCGCQ00780472 - (Closed) - Dev defect : To include Code Review comments
SCGCQ00780477 - (Closed) - Dev defect : Support for STP passthrough
SCGCQ00788270 - (Closed) - Dev defect : Move all the mctp pcie related changes to pciemctp.c
SCGCQ00791316 - (Closed) - MSM does not show VD info under logical tab when reconstruction operation running in 240VD mode
SCGCQ00793264 - (Closed) - After recon IO reqeuest to LBA in LDBBM list is not getting driverted to FW.
SCGCQ00794609 - (Closed) - SSD caching set to OFF throws success even when VDs are in Blocked state, through storcli.
SCGCQ00795263 - (Closed) - 3008 iMR - VPD failure with PCI SIG validation tools
SCGCQ00802118 - (Closed) - MR6.7:FW hits to MonTask: line 1272 in file ../../raid/1078dma.c after Injecting media error in loop on cachecade VD metadata
SCGCQ00802640 - (Closed) - Kill adapter during I/Os on VD associated with CCVD and with policy change script
SCGCQ00807136 - (Closed) - MR6.7:Wrong Queue Depth showing for (MR Controller)
SCGCQ00809773 - (Closed) - iMR compilation with PLDEBUG enabled fails in 6.7 codebase
SCGCQ00811274 - (Closed) - 6.7 Alpha : VDs are going to foreign config after issing OCR
SCGCQ00811296 - (Closed) - MR6.7: SVD's are getting 'Access Blocked' after OCR followed by System Reboot
SCGCQ00822385 - (Closed) - iMR compilation with PLDEBUG enabled fails in 6.7 codebase
SCGCQ00827605 - (Closed) - 6.7: Windows BSOD observed when upgrading from 6.6 to 6.7 through OFU when the OS is behind the controller
SCGCQ00769474 - (Closed) - MCTP_PCIE: Can not create more than 3 vds at the same 
SCGCQ00778601 - (Closed) - MCTP over PCI-E : On performing set/get operation through BMC while installing os , system rebooted automatically.
SCGCQ00783761 - (Closed) - Dev defect: Eventing is not working
SCGCQ00785004 - (Closed) - MCTP over PCI-E : BMC chip reset happens, when fw prints the message Got MRAPI more than 1 time for same application msgTag
SCGCQ00785950 - (Closed) - MR6.7: FW breaks into montask while making VDs offline when rebuild is going on with IOs
SCGCQ00792454 - (Closed) - System hang observed when writing to controller eeprom
SCGCQ00794698 - (Closed) - MR6.7:Montask at line 1272 in file../raid/1078dma.c after degrading the Spanned DG SVD's
SCGCQ00795483 - (Closed) - "Adapter at Baseport not responding" message seen in POST, after performing Cache Offload Scenario
SCGCQ00798645 - (Closed) - 6.7 : Order of Freeing Limd and Chain frames is not proper.
SCGCQ00798758 - (Closed) - Applications such as Ctrl R, HII, MSM etc shows "Maximum Allowed Unconfigured Good Drives" as 256
SCGCQ00804029 - (Closed) - Continuous "TASK_ABORT_INTERNAL" prints observed in FW, after running heavy IO's on JBOD configured using 12Gig SAS SSD
SCGCQ00804775 - (Closed) - CacheCade needs to check 32 MB non-aligned sizes for CCVD
SCGCQ00812842 - (Closed) - Firmware will POST bios message when there is a romId mismatch and no features present on the controller
SCGCQ00816234 - (Closed) - iMR hits Kill Adapter on running IO's on secure JBOD's
SCGCQ00831050 - (Closed) - FW faults with 4 RAID6 VDs with 12Gb/s SSDs
SCGCQ00716928 - (Closed) - CC2.5:Cahecade VD gets deleted on powercycling enclosure
SCGCQ00769756 - (Closed) - MCTP Over PCIE:Assertion failure MonTask: line 656 in file ../../i2c/i2COobMgmt.c
SCGCQ00795477 - (Closed) - FW should not allow "makeSystem" when "DriveErase" is going on
SCGCQ00799517 - (Closed) - MR6.7:CC2.5- Found DATA TLB ERROR(SRR0/1,ESR) after drives pull out
SCGCQ00805129 - (Duplicate) - MR & iMR FW Work-around is required for 3x08 chip Errata ID - 2012-RC714 for PCIE 3.0 compliance
SCGCQ00812136 - (Closed) - DEV defect to check in the SCGCQ00795477 code changes
SCGCQ00828709 - (Closed) - Write perf drop in 24R0 WB 256KB large QD
SCGCQ00830918 - (Closed) - EFI driver health fails when more than 64VDs configured
SCGCQ00638918 - (Closed) - Invader based controllers may be in config retry mode for more than 1 second
SCGCQ00825725 - (Closed) - FW upgrade from non 240VD FW to 240VD FW when OS is behind the controller results in BSOD
SCGCQ00812658 - (Closed) - Offload timed out for single image configurat
SCGCQ00227735 - (Closed) - MPI 2.6 Add Atomic Request Descriptor capability
SCGCQ00700829 - (Closed) - MPI 2.5: BIOS Page 1 additions
SCGCQ00685820 - (Closed) - MPI 2.5: distribute Target Command Buffers Received across multiple reply queues
SCGCQ00680527 - (Closed) - MPI v2.6: Added Intruder / Cutlass device IDs for manufacturing pages
SCGCQ00623271 - (Closed) - MPI 2.6: Added an additional signature value for the firmware image header
SCGCQ00619371 - (Closed) - MPI 2.6: Add new FLASH region types
SCGCQ00259613 - (Closed) - MPI v2.6: Additional request and reply descriptor formats
SCGCQ00264755 - (Closed) - MPI 2.6: SOP Encapsulated request
SCGCQ00264759 - (Closed) - MPI 2.6: NVMe Encapsulated request
SCGCQ00294055 - (Closed) - MPI 2.6: add Escape Passthrough bit to IO Flags of SCSI IO Request & Target Assist Request
SCGCQ00294131 - (Closed) - MPI 2.6: update SGL chapter to include PCIe
SCGCQ00336383 - (Closed) - MPI 2.6: PCIe IO Unit Page 0 & 1 definitions
SCGCQ00345258 - (Closed) - MPI 2.6: add IO Unit Control Request
SCGCQ00345260 - (Closed) - MPI 2.6: add PCIe Event Data (Generic), PCIe Device Status Change Event, and PCIe Enumeration Event
SCGCQ00345266 - (Closed) - MPI 2.6: PCIe Topology Change List Event
SCGCQ00345270 - (Closed) - MPI 2.6: PCIe Switch Config Pages
SCGCQ00345271 - (Closed) - MPI 2.6: add PCIe Device Config Pages
SCGCQ00353339 - (Closed) - Device Info field for PCIe devices
SCGCQ00357551 - (Closed) - MPI 2.6: add host page size to IOCInit Request and IOCFacts Reply
SCGCQ00360843 - (Closed) - MPI 2.6: add Port Request bit to IoFlags field of SCSI IO Request
SCGCQ00363600 - (Closed) - MPI 2.6: move all SAS IO Unit Page 4 functionality to IO Unit Page 11
SCGCQ00397136 - (Closed) - Modified address space bits
SCGCQ00397563 - (Closed) - MPI 2.6: Add PCIe IO Unit Page 4
SCGCQ00397568 - (Closed) - MPI 2.6: PCIe Device Page 2 reporting MDTS for NVMe devs
SCGCQ00397572 - (Closed) - MPI 2.6: Add board power fields to IO Unit Page 7
SCGCQ00397577 - (Closed) - MPI 2.6: Add support for SAS Persistent Connections
SCGCQ00398256 - (Closed) - MPI 2.6: Add NVMe SGL support
SCGCQ00432541 - (Closed) - MPI 2.6: Add NVMe SGL support to IEEE SGL
SCGCQ00480292 - (Closed) - Remove _SATA_TRANSMIT_PORT_SELECT_SIGNAL in IO Unit Control Request
SCGCQ00523879 - (Closed) - Identify physical location of a target device
SCGCQ00566306 - (Closed) - Add type BIOS for HashImageType.
SCGCQ00569175 - (Closed) - MPI 2.0: Add product-specific Flag bit to Clean Tool
SCGCQ00574070 - (Closed) - MPI 2.6: Add additional NVMe AccessStatus codes
SCGCQ00574358 - (Closed) - MPI2: Allow UEFI and BIOS to be Enabled/Disabled individually
SCGCQ00601869 - (Closed) - MPI 2.6: Add BootFlags field to Firmware Image Header
SCGCQ00732904 - (Closed) - Changes to enable controller receive\send PCIe generic message
SCGCQ00787920 - (Closed) - vSAN iMR Queue Depth change to 256 (Short term)
SCGCQ00789467 - (Closed) - Enable L3 auto flush with ON
SCGCQ00792731 - (Closed) - Increase maximum cache size for Cachecade to 2048GB.
SCGCQ00797237 - (Closed) - Change command block framework to avoid sentinel lock
SCGCQ00799438 - (Closed) - Block OFU for Firmware Updates Which Do not support Extended Commands
SCGCQ00812722 - (Closed) - Single write COL with FBU03
SCGCQ00820593 - (Closed) - Program CVFM(Cache Vault Flash Module) VPD without Supercap connected.
SCGCQ00613375 - (Closed) - Reconstruction from R0 to R1 in the presence of Media error deos not show ldbbm entries
SCGCQ00785739 - (Closed) - Antares needs LED activity for JBOD Fastpath.
SCGCQ00791114 - (Closed) - Avoid L3 flush in I/O path
SCGCQ00802656 - (Closed) - Change to allow configuration of I2C control registers for 100KHz vs 400 KHz bus
SCGCQ00820067 - (Closed) - Request to remove the repeated ROC temperature warnings in ttylog when above 104 deg C.
SCGCQ00735061 - (Closed) - MCTP over PCIE : Handling of packet
SCGCQ00787939 - (Closed) - MR FW- Update Attribution Language - Copyright, Trademark, Confidentiality to Avago
SCGCQ00789373 - (Closed) - Don’t wait for flush when unnecessary during a command block
SCGCQ00791450 - (Closed) - MR, iMR + MegaSR Support for 16 Byte CDB for ATA Microcode Download Pass-Thro
SCGCQ00764376 - (Port_Complete) - To fix S3 wakeup issue when boot mode is set to ignore errors(HCOE/HSM).
SCGCQ00766242 - (Port_Complete) - Delay OOB init untill fw is operational
SCGCQ00775673 - (Port_Complete) - TFM FAULT assertion does not change the VDs to Write-Through(WT) mode if no flag in Safety Status is set.
SCGCQ00789444 - (Port_Complete) - GG update to include concatenated GG/VPD data for Invader product generation.
SCGCQ00791476 - (Port_Not_Required) - Add prints in the FW that would be helpful while debugging
SCGCQ00791478 - (Ready) - Snapshot and CacheCade section offsets in DDF workspace
SCGCQ00791479 - (Port_Not_Required) - Supercap FAULT does not get asserted until temperature reaches 75 degrees celsius
SCGCQ00793009 - (Port_Complete) - Include learn cycle failure debug command in FW.
SCGCQ00794411 - (Port_Complete) - MCTPoverPCIE: MonTask: line 243 in file ../../raid/10 DATA TLB error on importing foreign config in Hermosa canyon(IMR) card.
SCGCQ00799380 - (Port_Complete) - Supercap FAULT does not get asserted until temperature reaches 75 degrees celsius
SCGCQ00799744 - (Port_Complete) - MCTPoverPCIE(IMR) Fatal firmware error: Line 152 in ../../raid/2108vDma.c on firing show configuration command
SCGCQ00801979 - (Port_Complete) - Firmware breaks into megamon with DATA TLB
SCGCQ00804586 - (Port_Complete) - MCTP_PCIE: Dev defect to check-in the changes for the defect SCGCQ00793277
SCGCQ00808206 - (Port_Complete) - Raid failure alerts are coming for the Card 9341 - 8i which doesn't support BBU
SCGCQ00814987 - (Port_Complete) - GG update to include concatenated GG/VPD data for Invader product generation.
SCGCQ00814997 - (Port_Complete) - Correctable ECC errors are not getting detected.
SCGCQ00815610 - (Port_Complete) - FW pkg 23.22.0-0017 and later initialize drives ~50% slower
SCGCQ00825773 - (Port_Complete) - OS (CentOS 7.0) crash observed while doing online FW update on IMR Fury controller
SCGCQ00825774 - (Port_Complete) - Background IO's on 235 R0 VD's and abrupt enclosure power cable pull resulting into Fatal FW error
SCGCQ00829759 - (Port_Complete) - MR firmware exposes more than 240 VD's to the host, even when the host driver doesn't support more than 64VD's.
SCGCQ00831408 - (Port_Complete) - EFI driver health fails when more than 64VDs configured
SCGCQ00789426 - (Port_Complete) - MegaRAID CPLD update improvements
SCGCQ00794414 - (Port_Complete) - MCTPoverPCIE:FW prints messageGot MRAPI more than 1 time for same application msgTag on performing get/set through BMC.
SCGCQ00798518 - (Port_Complete) - Break mirrored VD starts rebuilding with original PD after doing clear config
SCGCQ00799379 - (Port_Complete) - Add prints in the FW that would be helpful while debugging
SCGCQ00800782 - (Port_Complete) - Calculation for minimum blocks required to offload is wrong for single image configuration.
SCGCQ00810855 - (Port_Complete) - Remove Lock/Unlock of NOR flash by iMR and MR firmware function
SCGCQ00810860 - (Port_Complete) - Flash Improvement
SCGCQ00813062 - (Port_Complete) - Offload timed out for single image configuration
SCGCQ00821693 - (Port_Complete) - Controller commands are getting failed resulting in application hang when Logical Drive (LD) is deleted during reconstruction
SCGCQ00794413 - (Port_Complete) - Dev defect: commands fail with timeout even after firmware moves to ready state
SCGCQ00795822 - (Port_Complete) - Increase size of FCT table to 64 for MR and 32 for iMR
SCGCQ00799745 - (Port_Complete) - MCTPoverPCIE: SL fails to detect controller on uninitializing and initializing library while installing OS.
SCGCQ00810153 - (Port_Complete) - Patrol Read Properties window does not pop up on MSM
SCGCQ00810844 - (Port_Complete) - Read flash timeout from CFI instead of hardcoding
SCGCQ00810848 - (Port_Complete) - Error Handling for Flash parts using Intel SCS command set
SCGCQ00814991 - (Port_Complete) - Include learn cycle failure debug command in FW.
SCGCQ00814998 - (Port_Complete) - Correctable ECC errors are not getting detected.
SCGCQ00825775 - (Port_Complete) - MR6.7: FW breaks into montask while making VDs offline when rebuild is going on with IOs
SCGCQ00769827 - (Port_Complete) - Monitor the Safety Status Register flags when fault is asserted and take appropriate actions whenever necessary.
SCGCQ00799746 - (Port_Complete) - MCTPoverPCIE: DATA TLB Error MonTask: line 243 in file ../../raid/1078int.c on trying to clear foreignconfig in large config.
SCGCQ00772350 - (Port_Complete) - Drive activity can toggled by the user
SCGCQ00814989 - (Port_Complete) - MegaRAID CPLD update improvement
SCGCQ00827738 - (Port_Complete) - FW upgrade from non 240VD FW to 240VD FW when OS is behind the controller results in

BIOS:
SCGCQ00808086 - (Closed) - LegacyBIOS - Exposes "SecureJBOD" to system BIOS when 'Ask password at boot' entered wrongly
SCGCQ00809682 - (Closed) - BIOS - Shows expander as JBOD in POST
SCGCQ00808137 - (Closed) - BIOS - Line between "VDs handling" prints to be removed to match with "JBODs handling" prints
SCGCQ00798656 - (Closed) - Legacy BIOS: Handle new changes of BBU doc related to Battery Status
SCGCQ00799339 - (Closed) - Legacy OpROM : Legacy OpROM doesn't show proper PCI slot number on Intel WCP system.
SCGCQ00826174 - (Closed) - Legacy OpROM: 64VDs found on Host adapter eventhough more than 64 VDs are pre
SCGCQ00787941 - (Closed) - Update Attribution Language - Copyright, Trademark, Confidentiality to Avago
SCGCQ00795550 - (Closed) - Legacy BIOS: Address BBU/Supercap inconsistent Behavior across HSW a
SCGCQ00819752 - (Port_Complete) - Legacy OpROM : Legacy OpROM doesn't show proper PCI slot number on Intel WCP system.
SCGCQ00819755 - (Port_Complete) - LegacyBIOS - Exposes "SecureJBOD" to system BIOS when 'Ask password at boot' entered wrongly
SCGCQ00804825 - (Port_Complete) - Legacy OpROM : SSHA boot support
SCGCQ00819756 - (Port_Complete) - BIOS - Shows expander as JBOD in POST
SCGCQ00803146 - (Port_Complete) - Boot Device Selection in multi boot configur

NVDATA:
Numerous changes for specific customers

UEFI Driver:
SCGCQ00819632 - (Closed) - Rebranding effort for OEM
SCGCQ00813456 - (Closed) - UEFI Driver: Rebranding effort for OEM
SCGCQ00787943 - (Closed) - Update Attribution Language - Copyright, Trademark, Confidentiality to Av
SCGCQ00804835 - (Port_Complete) - UEFI Driver : SSHA boot support
SCGCQ00804837 - (Por_Complete) - Syncro 2.1 SSHA: Direction bit is not set for READ CAPACITY comm

HII:
SCGCQ00783374 - (Closed) - HII reports CCVD deleted even though its still under deletion process by FW
SCGCQ00795338 - (Closed) - HII: SSD caching enabled on a Recon VD .
SCGCQ00797318 - (Closed) - Change UCM form set title from AVAGO to LSI
SCGCQ00810827 - (Closed) - HII : 3 times wrong password at boot time – Handle the 'Manage Foreign Configuration' page options properly with Secure JBOD present
SCGCQ00798739 - (Closed) - HII Server profile shows "SILENCE ALARM" instead of "SERVER" subtitle as per design
SCGCQ00799642 - (Closed) - In copyback window the Associated Virtual Drive shows free space only for replacing drive
SCGCQ00804281 - (Closed) - MR6.7:FW hangs during SVD and CCVD migration based on DDR Size
SCGCQ00806514 - (Closed) - After entering security key it goes back to Manage Foreign config page
SCGCQ00816666 - (Closed) - HII: Handle CCVD Changes Based on new MR.h bit supportExtendedSSCSize
SCGCQ00803946 - (Closed) - HII does not show HDD /SSD information for the PDs in HII Drive management and Advanced drive properties page
SCGCQ00798824 - (Closed) - HII - NVRAM size shown as 32MB instead of 32KB
SCGCQ00783558 - (Closed) - HII Dashboard very sluggish when you have a 240 VD foreign config
SCGCQ00798579 - (Closed) - Schedule consitecny check gives invalid time when change from diable to hour, daily, weekly and monthly.
SCGCQ00798820 - (Closed) - Does not show RAID level for CCVD in 'VD management' and 'View DG properties' pages
SCGCQ00811359 - (Closed) - Change the Media type before the protocol.
SCGCQ00798684 - (Closed) - HII -> Drive management does not show "Secure" when JBOD created from a SED drive
SCGCQ00798806 - (Closed) - HII - Schedule CC right side info pane to be corrected (Add Monthly and Change Disabled to Disable as per drop down box)
SCGCQ00798962 - (Closed) - When Bootable JBOD is present under controller management ''Question value mismatch with option value'' window is displayed.
SCGCQ00808162 - (Closed) - HII allows to set 4Kn VD or 4Kn JBOD as bootable device even though legacyBIOS does not handle it
SCGCQ00810866 - (Closed) - Advanced Properties of VD are not displayed when it is Selected under Virtual Drive Management.
SCGCQ00811295 - (Reworked) - MR6.7Alpha HII: Generic RAID1 Profile based VD creation option is not grayed out after creating 64VD's.
SCGCQ00791138 - (Closed) - HII: Handle the maximum cache size value based on the max supported by FW, in the warning message shown during CCVD creation.
SCGCQ00798657 - (Closed) - HII: Handle new changes of BBU doc related to Battery Stat
SCGCQ00765822 - (Implemented) - Display the expander firmware version under Controller properties in HII when there is an expander on the controller
SCGCQ00819734 - (Closed) - HII : Rebranding effort for OEM
SCGCQ00789495 - (Closed) - RRB 87 - Suppress UEFI HII Clear Configuration setting
SCGCQ00787943 - (Closed) - Update Attribution Language - Copyright, Trademark, Confidentiality to Avago
SCGCQ00789505 - (Closed) - HII: Replace the word enclosure with expander for 720ix
SCGCQ00797917 - (Implemented) - HII: MegaRAID CPLD update improvements
SCGCQ00804082 - (Closed) - HII reports 'Security key entered is incorrect' even though it sent this request to FW and FW report as success.
SCGCQ00787942 - (Implemented) - Update Attribution Language - Copyright, Trademark, Confidentiality to Avago
SCGCQ00789504 - (Closed) - Consistency check date entry fix issue and Start Immediatley option required in SCC form
SCGCQ00787964 - (Closed) - HII: Address BBU/Supercap inconsistent Behavior across HSW a
SCGCQ00804190 - (Port_Complete) - CS2.0: HII : Domain ID should be displayed under High Availability properties
SCGCQ00804835 - (Port_Complete) - UEFI Driver : SSHA boot support
SCGCQ00805041 - (Port_Complete) - HII Create VD: Show error message when user clicks on Apply Change wihout choosing drive group
SCGCQ00820020 - (Port_Complete) - HII -> Drive management does not show "Secure" when JBOD created from a SED drive
SCGCQ00795791 - (Port_Complete) - HII Dashboard very sluggish when you have a 240 VD foreign config
SCGCQ00804183 - (Port_Complete) - HEFU HII : SSHA boot support
SCGCQ00816998 - (Port_Complete) - HII drive menu does not show 0MB drives
SCGCQ00819694 - (Port_Complete) - HII : 3 times wrong password at boot time – Handle the 'Manage Foreign Configuration' page options properly with Secure JBOD present
SCGCQ00791312 - (Port_Complete) - In HII, Not able to create Spaned Virtual Disk R50,R60 Back to 
SCGCQ00804193 - (Port_Complete) - Syncro 2.1 SSHA :Remove Provide Shared Access option of virtual drive property in HII since this option is not apply for SSHA
SCGCQ00804837 - (Port_Complete) - Syncro 2.1 SSHA: Direction bit is not set for READ CAPACITY commands
SCGCQ00820021 - (Port_Complete) - HII Create VD: Show error message when user clicks on Apply Change wihout choosing drive group
SCGCQ00820023 - (Port_Complete) - HII: SSD caching enabled on a Recon VD .
SCGCQ00820025 - (Port_Complete) - HII Server profile shows "SILENCE ALARM" instead of "SERVER" subtitle as per design
SCGCQ00769769 - (Port_Complete) - Implement password EFI_IFR_FLAG_CALLBACK bit requirement from UEFI spec 2.4 Errata B
SCGCQ00804182 - (Port_Complete) - Handling code review defects
SCGCQ00804188 - (Port_Complete) - Syncro 2.0: Support for SED.
SCGCQ00819701 - (Port_Complete) - After entering security key it goes back to Manage Foreign config page
SCGCQ00769225 - (Port_Complete) - Syncro 2.1 SSHA: Direction bit is not set for READ CAPACITY commands
SCGCQ00791320 - (Port_Complete) - HII reports CCVD deleted even though its still under deletion process by FW
SCGCQ00804176 - (Port_Complete) - Incompatibility details are not displayed under HII properties
SCGCQ00820018 - (Port_Complete) - HII allows to set 4Kn VD or 4Kn JBOD as bootable device even though legacyBIOS does not handle it
SCGCQ00820024 - (Port_Complete) - HII - NVRAM size shown as 32MB instead of 32KB
SCGCQ00803516 - (Port_Complete) - HA-DAS: Add HA support to HII
SCGCQ00804175 - (Port_Complete) - HAMR: HII Create VD- advance sees default as no share
SCGCQ00804181 - (Port_Complete) - HII - Provide support for toggling the controller to and from MAINTENANCE mode.
SCGCQ00804184 - (Port_Complete) - Syncro 2.0 HII: Support for SSC & SSHA configuration.
SCGCQ00820019 - (Port_Complete) - When Bootable JBOD is present under controller management ''Question value mismatch with option value'' window is displayed.
SCGCQ00804191 - (Port_Complete) - Display operation mode only if supportMaintenanceMode is set
SCGCQ00817018 - (Port_Complete) - Enclosure properties are not accurate in HII
SCGCQ00804185 - (Port_Complete) - Syncro 2.0 HII: Remove the option to create non-shared VD in the SSHA configuration
SCGCQ00804189 - (Port_Complete) - Syncro: VD Proprties-Advanced-GUID Value left blank and add customiztion for the string STR_FORM_HF115_PHNA_HELP
SCGCQ00810873 - (Port_Complete) - Deallocate the memory that was allocated for pPdList in SH_HF034_To_HF044()
SCGCQ00826109 - (Port_Complete) - Create Cache Cade VD option still available even after MaxConfgiureSSCSize is cro


Installation:
=============
Use StorCLI to flash the SAS controllers.  These tools can be downloaded from the support and download
section of www.lsi.com.

Command syntax:  
StorCLI /c0 download file=mr3108fw.rom






Component:
=========
SAS MegaRAID Firmware Release for MegaRAID Controllers
Release date: 03/27/15


Version Numbers:	
===============
Current Package Details:
Firmware Package:24.7.0-0042 (MR 6.6 P1)
Firmware 4.270.00-4183
ROMENV 1.09
BootBlock 3.06.00.00-0001
NVDATA  3.1411.00-0016
UEFI_Driver 0x060B0201 (SIGNED)
Hii v03.11.08.01(SIGNED)
FCODE 4.16.08.00
BIOS 6.22.03.1
Ctrl-R 5.08-0006
PCLI 1.07.05

Previous Package Details:
Firmware Package:24.7.0-0026 (MR 6.6)
Firmware 4.270.00-3972
ROMENV 1.09
BootBlock 3.06.00.00-0001
NVDATA  3.1411.00-0009
UEFI_Driver 0x060B0200 (SIGNED)
Hii v03.11.08.00(SIGNED)
FCODE 4.16.08.00
BIOS 6.22.03.0
Ctrl-R 5.08-0006
PCLI 1.07.05


Bug Fixes and Enhancements:
===========================
Firmware:
SCGCQ00812842 - (Closed) - Firmware will POST bios message when there is a romId mismatch and no features present on the controller
SCGCQ00830918 - (Closed) - EFI driver health fails when more than 64VDs configured
SCGCQ00829214 - (Closed) - MR firmware exposes more than 240 VD's to the host, even when the host driver doesn't support more than 64VD's.
SCGCQ00825725 - (Closed) - FW upgrade from non 240VD FW to 240VD FW when OS is behind the controller results in BSOD
SCGCQ00227735 - (Closed) - MPI 2.6 Add Atomic Request Descriptor capability
SCGCQ00259613 - (Closed) - MPI v2.6: Additional request and reply descriptor formats
SCGCQ00264755 - (Closed) - MPI 2.6: SOP Encapsulated request
SCGCQ00264759 - (Closed) - MPI 2.6: NVMe Encapsulated request
SCGCQ00294055 - (Closed) - MPI 2.6: add Escape Passthrough bit to IO Flags of SCSI IO Request & Target Assist Request
SCGCQ00294131 - (Closed) - MPI 2.6: update SGL chapter to include PCIe
SCGCQ00336383 - (Closed) - MPI 2.6: PCIe IO Unit Page 0 & 1 definitions
SCGCQ00345258 - (Closed) - MPI 2.6: add IO Unit Control Request
SCGCQ00345260 - (Closed) - MPI 2.6: add PCIe Event Data (Generic), PCIe Device Status Change Event, and PCIe Enumeration Event
SCGCQ00345266 - (Closed) - MPI 2.6: PCIe Topology Change List Event
SCGCQ00345270 - (Closed) - MPI 2.6: PCIe Switch Config Pages
SCGCQ00345271 - (Closed) - MPI 2.6: add PCIe Device Config Pages
SCGCQ00353339 - (Closed) - Device Info field for PCIe devices
SCGCQ00357551 - (Closed) - MPI 2.6: add host page size to IOCInit Request and IOCFacts Reply
SCGCQ00360843 - (Closed) - MPI 2.6: add Port Request bit to IoFlags field of SCSI IO Request
SCGCQ00363600 - (Closed) - MPI 2.6: move all SAS IO Unit Page 4 functionality to IO Unit Page 11
SCGCQ00397136 - (Closed) - Modified address space bits
SCGCQ00397563 - (Closed) - MPI 2.6: Add PCIe IO Unit Page 4
SCGCQ00397568 - (Closed) - MPI 2.6: PCIe Device Page 2 reporting MDTS for NVMe devs
SCGCQ00397572 - (Closed) - MPI 2.6: Add board power fields to IO Unit Page 7
SCGCQ00397577 - (Closed) - MPI 2.6: Add support for SAS Persistent Connections
SCGCQ00398256 - (Closed) - MPI 2.6: Add NVMe SGL support
SCGCQ00432541 - (Closed) - MPI 2.6: Add NVMe SGL support to IEEE SGL
SCGCQ00480292 - (Closed) - Remove _SATA_TRANSMIT_PORT_SELECT_SIGNAL in IO Unit Control Request
SCGCQ00523879 - (Closed) - Identify physical location of a target device
SCGCQ00566306 - (Closed) - Add type BIOS for HashImageType.
SCGCQ00569175 - (Closed) - MPI 2.0: Add product-specific Flag bit to Clean Tool
SCGCQ00574070 - (Closed) - MPI 2.6: Add additional NVMe AccessStatus codes
SCGCQ00574358 - (Closed) - MPI2: Allow UEFI and BIOS to be Enabled/Disabled individually
SCGCQ00601869 - (Closed) - MPI 2.6: Add BootFlags field to Firmware Image Header
SCGCQ00619371 - (Closed) - MPI 2.6: Add new FLASH region types
SCGCQ00623271 - (Closed) - MPI 2.6: Added an additional signature value for the firmware image header
SCGCQ00680527 - (Closed) - MPI v2.6: Added device IDs for manufacturing pages
SCGCQ00685820 - (Closed) - MPI 2.5: distribute Target Command Buffers Received across multiple reply queues
SCGCQ00700829 - (Closed) - MPI 2.5: BIOS Page 1 additions
SCGCQ00820593 - (Closed) - Program CVFM(Cache Vault Flash Module) VPD without Supercap connected.
SCGCQ00820067 - (Closed) - Request to remove the repeated ROC temperature warnings in ttylog when above 104 deg C.
SCGCQ00812722 - (Closed) - Single write COL with FBU03 OEM
SCGCQ00655162 - (Port_Not_Required) - Failed LED on 10HD BP does not light correctly for a bad drive
SCGCQ00783159 - (Port_Complete) - GPIO 24-31 is should be low when activity is going on drive
SCGCQ00783171 - (Port_Complete) - If diagnostic test fails on the copyback drive the FW does not allow a Recon, Copyback and CC on the same VD.
SCGCQ00783180 - (Port_Complete) - The field "expanderFwVersion=" is not populated under "ctrl info" in megamon
SCGCQ00783186 - (Port_Complete) - Behavior change when FW hit fault code 0x81 (uncorrectable ECC error)
SCGCQ00788250 - (Port_Complete) - Identify FDE drive compliant to spec and mark them as non-FDE drive
SCGCQ00788252 - (Port_Complete) - Need MR 6.3 iMR Firmware Capable of Updating the SBR on a Customer Board in the Field
SCGCQ00788283 - (Port_Complete) - Expander reports wrong active firmware version
SCGCQ00789243 - (Port_Complete) - Expander reporting temperature sensor error
SCGCQ00814987 - (Port_Complete) - GG update to include concatenated GG/VPD data for Invader product generation.
SCGCQ00814997 - (Port_Complete) - Correctable ECC errors are not getting detected.
SCGCQ00825773 - (Port_Complete) - OS (CentOS 7.0) crash observed while doing online FW update on IMR Fury controller
SCGCQ00825774 - (Port_Complete) - Background IO's on 235 R0 VD's and abrupt enclosure power cable pull resulting into Fatal FW error
SCGCQ00813062 - (Port_Complete) - Offload timed out for single image configuration
SCGCQ00821693 - (Port_Complete) - Controller commands are getting failed resulting in application hang when Logical Drive (LD) is deleted during reconstruction
SCGCQ00814991 - (Port_Complete) - Include learn cycle failure debug command in FW.
SCGCQ00825775 - (Port_Complete) - MR6.7: FW breaks into montask while making VDs offline when rebuild is going on with IOs
SCGCQ00814989 - (Port_Complete) - MegaRAID CPLD update improvements

BIOS:
SCGCQ00819752 (CSET) - Legacy OpROM : Legacy OpROM doesn't show proper PCI slot number on OEM system.
SCGCQ00819755 (CSET) - LegacyBIOS - Exposes "SecureJBOD" to system BIOS when 'Ask password at boot' entered wrongly
SCGCQ00819756 (CSET) - BIOS - Shows expander as JBOD in POST

NVDATA:
Numerous changes for specific customers

UEFI Driver:
SCGCQ00813456 (ENHREQ) - UEFI Driver: Rebranding effort for OEM
SCGCQ00819632 (ENHREQ) - Rebranding effort for OEM

HII:
SCGCQ00819694 (CSET) - HII : 3 times wrong password at boot time – Handle the 'Manage Foreign Configuration' page options properly with Secure JBOD present
SCGCQ00819701 (CSET) - After entering security key it goes back to Manage Foreign config page
SCGCQ00820018 (CSET) - HII allows to set 4Kn VD or 4Kn JBOD as bootable device even though legacyBIOS does not handle it
SCGCQ00820019 (CSET) - When Bootable JBOD is present under controller management ''Question value mismatch with option value'' window is displayed.
SCGCQ00820020 (CSET) - HII -> Drive management does not show "Secure" when JBOD created from a SED drive
SCGCQ00820021 (CSET) - HII Create VD: Show error message when user clicks on Apply Change wihout choosing drive group
SCGCQ00820023 (CSET) - HII: SSD caching enabled on a Recon VD .
SCGCQ00820024 (CSET) - HII - NVRAM size shown as 32MB instead of 32KB
SCGCQ00820025 (CSET) - HII Server profile shows "SILENCE ALARM" instead of "SERVER" subtitle as per design
SCGCQ00819734 (ENHREQ) - HII : Rebranding effort for OEM


Installation:
=============
Use StorCLI to flash the SAS controllers.  These tools can be downloaded from the support and download
section of www.lsi.com.

Command syntax:  
StorCLI /c0 download file=mr3108fw.rom





Component:
=========
SAS MegaRAID Firmware Release for MegaRAID Controllers
Release date: 01/14/15


Version Numbers:	
===============
Current Package Details:
Firmware Package:24.7.0-0026 (MR 6.6)
Firmware 4.270.00-3972
ROMENV 1.09
BootBlock 3.06.00.00-0001
NVDATA  3.1411.00-0009
UEFI_Driver 0x060B0200 (SIGNED)
Hii v03.11.08.00(SIGNED)
FCODE 4.16.08.00
BIOS 6.22.03.0
Ctrl-R 5.08-0006
PCLI 1.07.05

Previous Package Details:
Firmware Package:24.6.0-0023 (MR 6.5)
Firmware 4.260.00-3735
ROMENV 1.09
BootBlock 3.02.00.00-0001
NVDATA  3.1408.00-00
UEFI_Driver 0x06090700 (SIGNED)
Hii v03.10.09.00(SIGNED)
FCODE 4.16.08.00
BIOS 6.20.04
Ctrl-R 5.07-0006
PCLI 1.07.05


Bug Fixes and Enhancements:
===========================
Firmware:
SCGCQ00573118 - (Closed) - Change the comments to reflect updated offsets of struct fields due to increase in VD bitmap size, wherever applicable
SCGCQ00596373 - (Closed) - MR: foreign import does not happen on doing pull push of enclosure.
SCGCQ00596403 - (Closed) - MR: fw is allowing to set cachecade for more than 64th VD.
SCGCQ00596410 - (Closed) - MR: fw is allowing to set bootdrive for VD's after first 64
SCGCQ00598804 - (Closed) - MR: fw is allowing to create more than 64 raid 5 VD's
SCGCQ00598823 - (Closed) - MR: Firmware breaks into montask on creating virtual drive on spundown drive.
SCGCQ00624906 - (Closed) - MR6.3_240VD: When trying to import Virtual Drives to a JBOD enabled firmware that does not support 240 Virtual Drives, physical drives with configuration come as JBOD
SCGCQ00634632 - (Closed) - MR_240VD_ctrl-R: Cannot delete 64th VD from ctrl-R
SCGCQ00637521 - (Closed) - VD policy is not proper when auto Configuration direct command is fired.
SCGCQ00650083 - (Closed) - Fixed merge issues
SCGCQ00669493 - (Closed) - Code Cleanup and porting code review defects from auto Configuration ER of Tbolt.
SCGCQ00673189 - (Closed) - Fixing code compilation in 240 ld stream
SCGCQ00695591 - (Closed) - Firmware times out when removing cable from enclosure #2 causing a adapter kill.
SCGCQ00711787 - (Closed) - Enable DIS feature for 240VD Support
SCGCQ00716430 - (Closed) - MR6.5_FW: Firmware breaks while FW Upgrade and Downgrade followed by Dirty Shutdown of System
SCGCQ00735503 - (Closed) - To remove ignore64ldRestriction check
SCGCQ00738986 - (Closed) - Thermal Throttle – add controller shutdown logic if the ROC temperature is greater than Junction temperature(>115).
SCGCQ00755031 - (Closed) - MR6.6_FW: FW Breaks while doing target drive offline-online through apps when reconstruction is in progress.
SCGCQ00758821 - (Closed) - Firmware displaying device ID for only one of the expanders connected in multipath
SCGCQ00758866 - (Closed) - Invader 6.6 : OFU with Ios results in exception core 0
SCGCQ00758942 - (Closed) - Correctable Errors seen in Link disable/enable C-script test
SCGCQ00759837 - (Closed) - identifty secured JBOD state appropriately on Drive hotplug
SCGCQ00759926 - (Closed) - MR 6.6 : Firmware breaks into montask at line line 1992 in file ../../raid/cache.c
SCGCQ00761018 - (Closed) - Resolving compilation warning
SCGCQ00762277 - (Closed) - Seginus 240 drive test failed
SCGCQ00762588 - (Closed) - Firmware breaks while creating virtual drives in iMR controller
SCGCQ00764584 - (Closed) - MR FW 6.6 : Montask at line 1272 in file ../../raid/1078dma.c when trying to do recon on vd 0 when 64 vd is present.
SCGCQ00765750 - (Closed) - Disallow disabling security key on controller if there are any secure JBODs.
SCGCQ00767050 - (Closed) - MR 6.6 : Montask at line 1272 in file ../../raid/1078dma.c
SCGCQ00773743 - (Closed) - Handle secure erase operation on SATA SSD
SCGCQ00774042 - (Closed) - MR6.6_FW: Access policy remain as HD even after unhidding the VDs after restoring the configuration
SCGCQ00775075 - (Closed) - Disable OOB debug message during I2C initializaion
SCGCQ00775121 - (Closed) - MR6.6_FW: Excluded Virtual Drives from CC get automatically included after checking CC properties through MSM
SCGCQ00775267 - (Closed) - 3008 iMR - DPA extended capabilities bits structure is invalid
SCGCQ00779343 - (Closed) - All apps showing "Battery Learn in Progress" after 5th timeout with a supercapacitor flashed with Bad gas gauge.
SCGCQ00783613 - (Closed) - Firmware logs are not dumped to flash during device discovery phase
SCGCQ00784722 - (Closed) - Changing FW between 240 VD and non 240 VD versions will cause drives to go Unconfigured good if CCVDs are created.
SCGCQ00790104 - (Closed) - Devdefect: Reverting changes of MCTP from 6.6
SCGCQ00791909 - (Closed) - BSOD observed when tried to install OS with inbox driver using 240VD firmware
SCGCQ00793021 - (Closed) - PL fault iopiFault:FaultCode = 0000d10e observed, when removed drives were inserted back to the configuration
SCGCQ00793037 - (Closed) - MR_6.6: OCR is not triggered in OEL 5.11 UEK kernal with MRdiag running in background.
SCGCQ00800534 - (Resolved) - Performance with large block IOs (typically 64K and greater) have a large drop in performance while scaling QD with HDDs with R10 raid level
SCGCQ00575707 - (Closed) - DCMD cleanup
SCGCQ00625672 - (Closed) - fixed merge issues
SCGCQ00627932 - (Closed) - MR_6.4_FW: On creating a 2 drive R0 WT CC VD and a 2 drive R1 WB CC VD, FW hits 6916 in file ../../ssd/ssd_cache_fw.c
SCGCQ00637078 - (Closed) - Changed the logic of acquiring and releasing command block for hot plug case during auto Configuration (as part of 240 VD implementation) of physical drives.
SCGCQ00702586 - (Closed) - Added check to use old FW_RAID_MAP for iMR controllers as 240VD feature is not supported for iMR.
SCGCQ00705660 - (Closed) - Source VD's are getting lost after continuous back to back OCR with background IO's
SCGCQ00718552 - (Closed) - Hit Montask while creating R0 CC VD using 4 1TB SSD drives
SCGCQ00753530 - (Closed) - Post an event when Dirty data is discarded for LD under deletion
SCGCQ00759158 - (Closed) - MR 6.6 Coverity Defects
SCGCQ00759189 - (Closed) - Do not enable fast path on security enabled JBODs.
SCGCQ00760713 - (Closed) - Not able to set autobgi=on/off through storcli for a hidden VD
SCGCQ00760785 - (Closed) - Fix Coverity Defects
SCGCQ00762388 - (Closed) - Drives are coming as Full size 1 Drive R0 upon same drive Hot Plug
SCGCQ00765254 - (Closed) - Unable to change policies of auto configured VDs
SCGCQ00767393 - (Closed) - DDF_WORKSPACE data structure is made backward compatible
SCGCQ00774702 - (Closed) - Firmware breaks after foreign configuration import
SCGCQ00777721 - (Closed) - MR_6.6: Disable of MCTP for integration release
SCGCQ00781764 - (Closed) - Gas Gauge parameters are not updated for config change
SCGCQ00595201 - (Closed) - Firmware crash is seen when reconstruction operation is started on a VD
SCGCQ00601801 - (Closed) - MR : On trying to create RAID0 volumes on all drives, FW breaks into montask.
SCGCQ00701768 - (Closed) - Bandwidth falls as queue depth increses on R5/R6 24/40Dr SATA HDD configurations at 256KSW block size
SCGCQ00706915 - (Closed) - MR_240VD: On discarding Preserved cache, Consistency Check gets initiated on VD
SCGCQ00758012 - (Closed) - coverity defect 15429
SCGCQ00759131 - (Closed) - A particular bad TFM(CV) can cause FW OCR at boot time due to Montask
SCGCQ00759973 - (Closed) - MR FW 6.6: AWB option support should be removed with CCVD.
SCGCQ00763930 - (Closed) - JBOD feature got disabled upon foreign import
SCGCQ00765466 - (Closed) - Drives are detected as UG after migrating 240VD config from MR to IMR controller
SCGCQ00767157 - (Closed) - MR6.6:Montask at line 203 in file ../../raid/timer.c after PR is triggered from HII
SCGCQ00767346 - (Closed) - CacheCade: Delete/ modify the unnecessary debug prints
SCGCQ00768394 - (Closed) - fwDownload memory was freed in check_for_flush_over() before the fw upgrade process is initiated
SCGCQ00772348 - (Closed) - CCVD policy fails to change the policy from WB to WT from MSM/Storcli
SCGCQ00783354 - (Closed) - MR_6.6_ALPHA: Kill adapter found while deleting ld with discardcache
SCGCQ00792440 - (Closed) - Montask observed at line 1026 in file ../../dm/src/dm.c with Enclosure Cable Pull/Push Scenario
SCGCQ00573110 - (Closed) - Optimize host command dispatch code in set_state()
SCGCQ00715154 - (Closed) - Event logging for incoming controller property value is done incorrectly.
SCGCQ00755042 - (Closed) - Consistency check starts even on excluded virtual drives
SCGCQ00763683 - (Closed) - Delay OOB init untill fw is operational
SCGCQ00765165 - (Closed) - 6.6 Coverity : For 15356, 15353, 15351, 15349 and 15345 defects
SCGCQ00767348 - (Closed) - Firmware indicating that PD can be spun down even in online state
SCGCQ00772255 - (Closed) - CRC calculated wrongly after NVRAM layout migration from legacy to new format
SCGCQ00777096 - (Closed) - Instruction TLB error seen during reboot after all 240 VD's policy being changed
SCGCQ00800530 - (Resolved) - 6.6 Beta code has a regression from 6.5 GCA in 64K RW workloads with 40x SAS HDDs
SCGCQ00739663 - (Closed) - MegaRAID CacheCade Pro 2.0 Feature will deactivate on restart
SCGCQ00755332 - (Closed) - Fail to import foreign drives in iMR controller
SCGCQ00759941 - (Closed) - nomChgVoltage displaying wrong value.
SCGCQ00760182 - (Closed) - 6.6 Coverity : CID 13587 and 10827
SCGCQ00764459 - (Closed) - FW Breaks into MonTask: line 1968 in file ../../bbu/onfi.c on doing OCR with Pinned cache and setting termolog ON
SCGCQ00780134 - (Closed) - Disable sgpioSmpPresenceDetect for specific customer
SCGCQ00787285 - (Closed) - StorCLI crashed when tried to enquire LD information
SCGCQ00761748 - (Closed) - drives were identified as JBOD by default; add condition to verify enableJBOD is set to 1
SCGCQ00762592 - (Closed) - Workaround for Hardware Issue - SCGCQ00632364
SCGCQ00757456 - (Closed) - Handle the deadlock scenario which could occur during ld deletion with Discarding the dirty data.
SCGCQ00765315 - (Closed) - MR6.6_FW_240: Virtual Drive deleted after OCR during reconstruction
SCGCQ00765738 - (Closed) - Controller crashes on running dual core capable writes on dual core capable volumes whose VD # is greater then 64
SCGCQ00779326 - (Closed) - Displaying wrong CCVD size in all applications
SCGCQ00227735 - (Closed) - MPI 2.6 Add Atomic Request Descriptor capability
SCGCQ00680527 - (Closed) - MPI v2.6: Added Intruder / Cutlass device IDs for manufacturing pages
SCGCQ00623271 - (Closed) - MPI 2.6: Added an additional signature value for the firmware image header
SCGCQ00619371 - (Closed) - MPI 2.6: Add new FLASH region types
SCGCQ00601869 - (Closed) - MPI 2.6: Add BootFlags field to Firmware Image Header
SCGCQ00574070 - (Closed) - MPI 2.6: Add additional NVMe AccessStatus codes
SCGCQ00259613 - (Closed) - MPI v2.6: Additional request and reply descriptor formats
SCGCQ00264755 - (Closed) - MPI 2.6: SOP Encapsulated request
SCGCQ00264759 - (Closed) - MPI 2.6: NVMe Encapsulated request
SCGCQ00294055 - (Closed) - MPI 2.6: add Escape Passthrough bit to IO Flags of SCSI IO Request & Target Assist Request
SCGCQ00294131 - (Closed) - MPI 2.6: update SGL chapter to include PCIe
SCGCQ00336383 - (Closed) - MPI 2.6: PCIe IO Unit Page 0 & 1 definitions
SCGCQ00345258 - (Closed) - MPI 2.6: add IO Unit Control Request
SCGCQ00345260 - (Closed) - MPI 2.6: add PCIe Event Data (Generic), PCIe Device Status Change Event, and PCIe Enumeration Event
SCGCQ00345266 - (Closed) - MPI 2.6: PCIe Topology Change List Event
SCGCQ00345270 - (Closed) - MPI 2.6: PCIe Switch Config Pages
SCGCQ00345271 - (Closed) - MPI 2.6: add PCIe Device Config Pages
SCGCQ00353339 - (Closed) - Device Info field for PCIe devices
SCGCQ00357551 - (Closed) - MPI 2.6: add host page size to IOCInit Request and IOCFacts Reply
SCGCQ00360843 - (Closed) - MPI 2.6: add Port Request bit to IoFlags field of SCSI IO Request
SCGCQ00363600 - (Closed) - MPI 2.6: move all SAS IO Unit Page 4 functionality to IO Unit Page 11
SCGCQ00397136 - (Closed) - Modified address space bits
SCGCQ00397563 - (Closed) - MPI 2.6: Add PCIe IO Unit Page 4
SCGCQ00397568 - (Closed) - MPI 2.6: PCIe Device Page 2 reporting MDTS for NVMe devs
SCGCQ00397572 - (Closed) - MPI 2.6: Add board power fields to IO Unit Page 7
SCGCQ00397577 - (Closed) - MPI 2.6: Add support for SAS Persistent Connections
SCGCQ00398256 - (Closed) - MPI 2.6: Add NVMe SGL support
SCGCQ00432541 - (Closed) - MPI 2.6: Add NVMe SGL support to IEEE SGL
SCGCQ00480292 - (Closed) - Remove _SATA_TRANSMIT_PORT_SELECT_SIGNAL in IO Unit Control Request
SCGCQ00552730 - (Closed) - Auto Configuration of Raid 0 volumes for 240 VD requirement.
SCGCQ00563479 - (Closed) - Convert all 64-bit LD bitmaps to a generic bitmap mechanism, and RAID_MAP API changes
SCGCQ00574463 - (Closed) - Integrating MR APIs for 240LD support into firmware
SCGCQ00600962 - (Closed) - NVRAM migration from LEGACY to EXT format and NVRAM EXT struct reformatting (cleanup)
SCGCQ00601214 - (Closed) - Write new extended DDF format on the physical drives.
SCGCQ00710437 - (Closed) - Long term API solution, ability to change disableImmediate from MFI API
SCGCQ00712485 - (Closed) - Expanders with diffrent SAS address but same ELI shown as single device
SCGCQ00774902 - (Closed) - Match the FW configuration with our latest Gas Gauge settings for an OEM
SCGCQ00732904 - (Implemented) - Changes to enable controller receive\send PCIe generic message
SCGCQ00751803 - (Closed) - Enable 16k SS for custom business
SCGCQ00573772 - (Closed) - DDF module changes to support 240 Virtual Drives.
SCGCQ00625447 - (Closed) - Enabled R5/R6 240 VD support
SCGCQ00741705 - (Closed) - Support 128K bypass threshold
SCGCQ00571124 - (Closed) - implement IO path and NVRAM changes
SCGCQ00712501 - (Closed) - LD Deletion stalling all IOs on HBA 12.12.0-0178
SCGCQ00735061 - (Closed) - MCTP over PCIE : Handling of packet
SCGCQ00711560 - (Closed) - Enable security on JBOD
SCGCQ00751088 - (Closed) - Command block optimizations to avoid IO stalls


BIOS:
SCGCQ00769239 - (Closed) - Don't issue REAID I/O on the 4K JBOD
SCGCQ00783579 - (Closed) - Auto Select Boot device (alias multiboot): INT13 drive type is not set correctly for physical disk
SCGCQ00769269 - (Closed) - Before calling Translate_LdTargetIdList_To_LdList set int13 drive type
SCGCQ00550426 - (Closed) - Increase OpROM code size from 40k to 48k


NVDATA:
Numerous changes for specific customers

UEFI Driver:
SCGCQ00638308 - (Closed) - FMP GetImageInfo could result in stack corruption - Code Review Defect ID D26304
SCGCQ00335617 - (Closed) - Drives are reporting timeout on Write Buffer cmd on H310 and Nautilus.efi
SCGCQ00378953 - (Closed) - HII not showing up + other enhancement for driver health formset
SCGCQ00413986 - (Closed) - HII app doesnt appear when there is critical message and when platform uses SetOptions
SCGCQ00479003 - (Closed) - Disable Debug print in UEFI Driver
SCGCQ00618669 - (Closed) - UEFI Driver: StartHiiBackEnd() has Print statement with %g
SCGCQ00320619 - (Closed) - UEFI: Build Device Path and Get Next Target function of SCSI Pass Thru is not returning correct EFI status for certain cases
SCGCQ00339371 - (Closed) - UEFI Driver fails SCT Test
SCGCQ00408333 - (Closed) - UEFI: Critical boot message formatting issue
SCGCQ00691044 - (Closed) - Code refactor effort: Hii Image buffer clean-up
SCGCQ00347171 - (Closed) - MR: on having pinned cache on oem -2GB controller, the option to invoke storage dosent come.
SCGCQ00384884 - (Closed) - Customize health formset + few other issues
SCGCQ00395190 - (Closed) - HII - 03.02.03.00/When trying to create an R6/R5, I am unable to create though there are 3 SAS unconfigured good avail
SCGCQ00396051 - (Closed) - UEFI Driver (MR 5.7) should not display finite boot messages
SCGCQ00435384 - (Closed) - UEFI System hang if controller FW is in fault state
SCGCQ00732773 - (Closed) - UEFI Driver: If the platform contains UEFI Spec Rev < than 2.3.0, then don't HII
SCGCQ00688789 - (Closed) - DHP: Remove default value from numeric primitive that is present under suppressif
SCGCQ00343869 - (Closed) - Enhance critical boot message handling
SCGCQ00369636 - (Closed) - UEFI: Settime only when FW time is not set; DHP: Return appropriate health status when there is no critical boot message
SCGCQ00408094 - (Closed) - Supermicro system with a critical message does not enter EFI preboot config utility
SCGCQ00498925 - (Closed) - Not able to boot into BIOS boot menu in oem server
SCGCQ00756810 - (Closed) - PKG 9 HII form/When you have a a critical message such as missing VDs, after select "C" <ENTER>, it will show an assert
SCGCQ00312683 - (Closed) - UEFI Driver not timing out in 3 mins when FW is in undefined state
SCGCQ00726723 - (Closed) - Ext/SCSI PassThru: UEFI Driver not filling direction flag correctly for Read
SCGCQ00518791 - (Closed) - DriverDiagnostics2.c: In IsValidHandle() - Free the buffer if status is not EFI success for LocateHandle
SCGCQ00493654 - (Closed) - Memory Leak issue in UEFI driver when reconnect happens
SCGCQ00308870 - (Closed) - EFI Driver 518\When disconnecting the driver in EFI, I am still able to exectue the EFI utility menu.
SCGCQ00696656 - (Closed) - Update Mbox value for 240VD Support
SCGCQ00601851 - (Closed) - System hang when we press F1 on second time when we are in HII form
SCGCQ00578194 - (Closed) - UEFI Driver should calculate checksum before setting bios data (MR_BIOS_DATA)
SCGCQ00262858 - (Closed) - Debug message is shown from EFI app choice prompt on a Yilan system
SCGCQ00589148 - (Closed) - Diskpart EFI utility can't create partition on a JBOD
SCGCQ00483847 - (Closed) - EKMS: Remove private GUID and use EFI_KMS_PROTOCOL_GUID defined in UEFI 2.3.1 spec
SCGCQ00628310 - (Closed) - Install FMP on Controller Handle at Start() and the exception
SCGCQ00340581 - (Implemented) - UEFI Driver should check pMRCtrlInfo ->maxHANodes with > 1 to determine HAMR
SCGCQ00365374 - (Implemented) - Add 3108 device ID for oem
SCGCQ00385365 - (Closed) - UEFI Driver (FoD): 
SCGCQ00285974 - (Implemented) - Add 4k secotor boot support in UEFI Driver
SCGCQ00404216 - (Closed) - Add 3008 device ID for iMR product.
SCGCQ00318101 - (Closed) - Timed critical boot message under UEFI mode
SCGCQ00347492 - (Closed) - UEFI: Retry read capacity if scsi status is not success
SCGCQ00395996 - (Closed) - UEFI Driver: Parse Boot message and remove \r\n at the beginning and replace \n with \r in other parts
SCGCQ00526851 - (Closed) - Support EFI_FIRMWARE_MANAGEMENT_PROTOCOL for controller firmware upgrade.
SCGCQ00292963 - (Implemented) - UEFI Driver: LSIP200198414/LSIP200229508/LSIP200231613: Disables all requirement for human input at boot time
SCGCQ00331573 - (Closed) - MR_UEFI_Driver: Remove dependency on deprecated Driver Configuration2 protocol from UEFI Driver
SCGCQ00392836 - (Closed) - LSI to Support Remote Key Management
SCGCQ00278257 - (Implemented) - Add FoD support for 3108 for oem
SCGCQ00436609 - (Closed) - oem add PnPID's for 3004 and 3108
SCGCQ00338782 - (Implemented) - If SetOptions is called for Invader dont show EFI WebBIOS and EFI CLI option
SCGCQ00338066 - (Implemented) - UEFI - HAMR: Fire LD list query based on maxHANodes
SCGCQ00550389 - (Closed) - WebCloud Group - Write Caching HBA, JBOD/R0 supported TB controller with 240 SystemPD/LD support
SCGCQ00626601 - (Implemented) - VT-d/IOMMU support for iMR - Implement mechanism to allow system BIOS to put entries for iMR mem allocation into proper table
SCGCQ00310476 - (Implemented) - Load HII when user responds to critical boot message by pressing C
SCGCQ00650086 - (Implemented) - UEFI Driver UDK2010 complaince
SCGCQ00635878 - (Port_Complete) - UEFI Driver- has debug print statements during POST
SCGCQ00688987 - (Port_Complete) - Don't let user boot to OS until user discards dirty cache
SCGCQ00484086 - (Port_Complete) - platfrom has UEFI hang when SATA is connected (the issue discovered in pre-dev 13G platform)
SCGCQ00677776 - (Port_Complete) - Initilize the buffer that we allocate to load HII and return EFI_OUT_OF_RESOURCES if allocation fails
SCGCQ00678154 - (Port_Not_Required) - For oemdont free the host memory during disconnect/unload process
SCGCQ00736761 - (Port_Complete) - Return health status failed if we have returned device error from Start()
SCGCQ00756861 - (Port_Complete) - ControllerInfo[CtrlIndex].ControllerHandle got initialized incorrectly or too early
SCGCQ00468948 - (Port_Complete) - Uninstall HII CAP and Driver Health formset if platform calls Start again without calling GetHealthStatus
SCGCQ00477828 - (Port_Complete) - 9240/9260/9270 UEFI driver issue with RD640/RD440 platforms when user having 2TB or 4TB VD
SCGCQ00679073 - (Port_Complete) - Do not go to WebBIOS due to a bad health status when WebBIOS is disabled in NVDATA.
SCGCQ00695249 - (Port_Complete) - Safe guard: Return health status failed if platform calls GetHealthStatus w/ NULL handle after we return intermediate status
SCGCQ00716623 - (Port_Complete) - For oem change memory type from EfiRuntimeServicesData to EfiMemoryMappedIO
SCGCQ00606367 - (Port_Complete) - UEFI Driver returns EFI_NOT_FOUND when platform passes valid Target for ExtSPT.BuildDevicePath()
SCGCQ00644508 - (Port_Complete) - CPU EXCEPTION ERROR During CSIOR Stage- After Updating idrac X38 to X39 (Dont double free the memory)
SCGCQ00478692 - (Port_Complete) - Block IO tests from SCT IHV test suite failed
SCGCQ00484114 - (Port_Complete) - ATA PT: Follow UEFI Spec on interpreting In and Out Transfer Length that upper layer sends
SCGCQ00580313 - (Port_Complete) - User can't access RAID HII in UEFI mode after removing a HDD
SCGCQ00658168 - (Port_Complete) - ATA Pass thru: Timeout is not passed correctly to FW
SCGCQ00716622 - (Port_Complete) - For oem dont free the host memory during disconnect/unload process


HII:
SCGCQ00740787 - (Closed) - Cloning (alias Save/Restore) : HII issues Add Config when there is no config
SCGCQ00764936 - (Closed) - Schd CC page/Consistency Check mode does not explain the difference between sequential & concurrent
SCGCQ00768459 - (Closed) - HII 5.13 PKG 01/Enclosure Management screen and Drive managment screen do not match
SCGCQ00771730 - (Closed) - HII: Locked PD is shown in Preview Foreign Configuration form.
SCGCQ00758589 - (Closed) - Dashboard View Help Content: Reuse the string where possible and incoporate following changes suggested by tech pub
SCGCQ00762860 - (Closed) - HII Dashboard/3.11.02.00/View server profile is showing two periods after the word "them" under Hardware Components
SCGCQ00767605 - (Closed) - When you have a locked PD/FDE in a foreign state, it is not showing up on the dashboard only under configure
SCGCQ00783556 - (Closed) - Question value mismatch when Fan3 and 4 is selected
SCGCQ00756533 - (Closed) - Remove FRU from Enclosure Management
SCGCQ00762856 - (Closed) - HII Dashboard/3.11.02.00/When preview foreign config from Dashboard, it is coming up as HF034 at the top
SCGCQ00783558 - (Closed) - HII Dashboard very sluggish when you have a 240 VD foreign config
SCGCQ00784597 - (Closed) - HII Configuration Management Enable Security On JBOD OK button is grayed out
SCGCQ00783374 - (Closed) - HII reports CCVD deleted even though its still under deletion process by FW
SCGCQ00714530 - (Closed) - HII: Firmware Update - On selecting empty folder, hang is seen.
SCGCQ00755277 - (Closed) - Change "Consistency Check" to "Make Data Consistent" for CC Rate and Stop CC on error is not changed
SCGCQ00770227 - (Closed) - HII displays supercap module version as "Firmware Version"
SCGCQ00771193 - (Closed) - HII: Entering security key in HII to unlock PD fails to import afterwards
SCGCQ00765519 - (Closed) - HII: R5/R6 creation fails in HII from Profilebased creation
SCGCQ00755021 - (Closed) - HII 6.6: Operation's are not refreshed in Dashboard
SCGCQ00760501 - (Closed) - DashBoard HII showing 1 enclosure connected even though there are 0 connected.
SCGCQ00766787 - (Closed) - HII- DHS assgining fails in presence of 240 Vds
SCGCQ00765523 - (Closed) - Invader 6.6: HII : BGops fails to start when VD erase is already runnign on the other VD
SCGCQ00760435 - (Closed) - Date getting corrupted when selecting different Check Consistency Frequencie
SCGCQ00768437 - (Closed) - Entering the wrong security key in HII & go back to enter the correct one the security key form should be cleared
SCGCQ00684992 - (Closed) - Question about "Connected Port" in PD advance menue
SCGCQ00779364 - (Closed) - Wrong drivegroup count shown with foreign config in safe mode
SCGCQ00767138 - (Closed) - HII: Controller in Safe Mode - ASSERTs seen on console during the Preview of Foreign Configuration
SCGCQ00765244 - (Closed) - Dashboard: comment out the referesh interval for all other fields except conroller status.
SCGCQ00756640 - (Closed) - MR_6.6_HII: In configuration Management creation of JBOD not possible as option to set JBOD is grey out.
SCGCQ00761105 - (Closed) - Dashboard/HII 03.11.02.00/Using generic oem Controller or oem controller yields spaces in HII Dash
SCGCQ00764215 - (Closed) - HII 5.13 PKG 01/3.11.02.00/Preview foreign configuration screen missing words
SCGCQ00776052 - (Closed) - 5.13 HII PKG 02/When creating a VD that is more than 1TB in size in HII, you will loose the extra space after saving the VD
SCGCQ00778462 - (Closed) - HII Boot time Asserts
SCGCQ00760450 - (Closed) - HII: Need to remove Force Write Back option with CCVD creation
SCGCQ00742103 - (Closed) - Remove Head Of Queue rebuild feature
SCGCQ00750118 - (Closed) - Remove Head Of Queue rebuild feature
SCGCQ00756784 - (Closed) - Chk the err status for HL_Get_PD_List() and HL_Get_PD_Info in UF002_PrepareData() + check Driver handle if index is valid
SCGCQ00760432 - (Closed) - Getting question value mismatch when changing the Consistency check Frequency settings
SCGCQ00768009 - (Closed) - HII : Locked PD on controller with security disabled does not show properly when viewing under Foreign config
SCGCQ00730596 - (Closed) - UEFI: Refreshing individual field (in this case progress field)
SCGCQ00711563 - (Closed) - RRB 71 - enable SED support for iMR JBOD
SCGCQ00721161 - (Closed) - SAS3: HII Create Virtual Drive advanced option defaults Protect Virtual Drive to enabled
SCGCQ00712484 - (Closed) - HII. Create dashboard view as a landing form in HII
SCGCQ00756855 - (Port_Complete) - Chk the err status for HL_Get_PD_List() and HL_Get_PD_Info in UF002_PrepareData() + check Driver handle if index is valid
SCGCQ00765468 - (Port_Complete) - Hardware Component Details are not being displayed under Hardware Components
SCGCQ00780729 - (Port_Complete) - Enclosure properties are not accurate in HII
SCGCQ00757730 - (Port_Complete) - Help string corrections + Suppress subtitle CACHECADE + Change Safe mode to Safe mode on errors
SCGCQ00768167 - (Port_Complete) - H730p battery's manufacture date can be set to any date in the controllers HII environment
SCGCQ00790204 - (Port_Complete) - 2TB and 4TB HDD show 1TB and 3TB in HII

Ctrl-R:
SCGCQ00759987 - (Closed) - CTRL+R: AWB option support with CCVD should not be there.
SCGCQ00725192 - (Closed) - Firmware Crash is hit while creating the Raid1 vd without drives selected
SCGCQ00756647 - (Closed) - 6.6_StorCli: StorCli lists all cascaded enclosures at position 0.
SCGCQ00757358 - (Closed) - Add adapterOperation support details in /c0 show all for cachebypassMode.
SCGCQ00758770 - (Closed) - FW breaks in iMR when excluding VD's from CC
SCGCQ00759187 - (Closed) - Boot Volume details is shown in Megacli but not with storcli.
SCGCQ00759290 - (Closed) - SSM-FLASh drives property is displayed for regular drives.
SCGCQ00759862 - (Closed) - OEMID is coming as "Unknown" for /c0 show all
SCGCQ00761937 - (Closed) - MR 6.6 Prealpha2 Storcli:Similar PCI address(BDF number) is displayed for multiple controllers connected to FreeBSD 9.3.
SCGCQ00771626 - (Closed) - Storcli errors are printing in a different line.
SCGCQ00772243 - (Closed) - StorCLI shows CacheBypass Size and CacheBypass Mode feature enabled against a VD which is associated with a CacheCade VD
SCGCQ00772302 - (Closed) - Storcli has option to set PR maxconcurrentpd but show is not present
SCGCQ00772332 - (Closed) - vpdpage should be read from 4 bytes to get serial number of drive
SCGCQ00779789 - (Closed) - Active operation(s) is coming as none when virtual drive erase is in progress.
SCGCQ00779800 - (Closed) - MR6.6_CLI_FreeBSD: Displaying incorrect Driver name
SCGCQ00783357 - (Closed) - CTRL-R:2 iMR Card in same System hitting Montask
SCGCQ00790050 - (Closed) - "./storcli64 /c0 show all page" shows "cachevault flash size = 8.0 ZB
SCGCQ00764750 - (Closed) - MR6.6_Ctrl+R: Not able to see Advanced Software Option (ASO) in Virtual Drive Management
SCGCQ00759181 - (Closed) - Add adapterOperation support details in /c0 show all for Emulationtype.
SCGCQ00759969 - (Closed) - Adapters are not listed in sorted order.
SCGCQ00765759 - (Closed) - StorCLI shows wrong "Number of blocks" for a 65.5TB VD size
SCGCQ00765762 - (Closed) - StorCLI VMware Binary not displaying detailed description for phyerrorcounters of enclosures
SCGCQ00767347 - (Closed) - Patrol read delay is showing wrong value when set to continuous
SCGCQ00778577 - (Closed) - GB scale to be added while showing CacheCade size in CLI
SCGCQ00779806 - (Closed) - ASO count mismatch in show ASO w.r.t ASO in storcli show all cmd
SCGCQ00782882 - (Closed) - MR6.6:StorCLI shows incorrect information about "Cache Vault Flash Size"
SCGCQ00785679 - (Closed) - MR 6.6 Apha: Controllers are not sorted according to BDF(bus device funtion) in CTRL-R.
SCGCQ00777828 - (Closed) - CTRL-R reports CCVD deleted even though its still under deletion process by FW
SCGCQ00760989 - (Closed) - CTRL-R: FW hits MonTask, When CTRL-R is launched immediately after the MR Controller initialization is complete and before the iMR card initialization starts in the BIOS POST.
SCGCQ00752000 - (Closed) - In Windows and Linux only controller grouping is working but not sorting
SCGCQ00758101 - (Closed) - MR_6.6_Storcli: Storcli reports supercap state 'unknown' while learn is happening on the controller.
SCGCQ00759183 - (Closed) - SED adapterOperation detailed is not shown in detailed show controller properties
SCGCQ00759959 - (Closed) - Support details are not shown in /c0 show all for discard cache (stalling LD deletion)
SCGCQ00760385 - (Closed) - MR_6.6: StorCLI showing incorrect value for next Schedule time for consistency check after disabling the CC
SCGCQ00762663 - (Closed) - Storclio : Different error code is coming for 'set pcilinkspeed' in VMware 4.1U3
SCGCQ00764658 - (Closed) - StorCLI /c0 show all command does not reflect the discard vd delete filed
SCGCQ00765714 - (Closed) - StorCLI shows CacheBypass Size and CacheBypass Mode feature enabled against a CacheCade VD
SCGCQ00767363 - (Closed) - Showing wrong creation date for Autoconfigured virtual drives
SCGCQ00785400 - (Closed) - VD level hide/unhide is not possible through storcli in PPC
SCGCQ00790062 - (Closed) - "./storcli64 /c0 show cc" fails in RHEL 6.6 PPC64 with more than 64 VDs present
SCGCQ00756487 - (Closed) - Incorrectness in the popupmenu generated for the controller info when controller is in Safe Mode
SCGCQ00765643 - (Closed) - Ctrl+R not handling VD policy change error case for Autoconfigured Virtual Drives
SCGCQ00730505 - (Closed) - After Rebuilding, DHS and Expand VD operations failed to update as per VD properties
SCGCQ00758924 - (Closed) - Exception with command /co show badblocks or "storcli /cx flasherase"
SCGCQ00759178 - (Closed) - SupportMaxRate SATA is not listed in PD allowed operations.
SCGCQ00760398 - (Closed) - MR6.6: Segmentation fault (Core Dumped) in CLI when setting any invalid value for PR start time
SCGCQ00760752 - (Closed) - /c0 show all does not list hwCfg information as compared to MegaCLI.
SCGCQ00790022 - (Closed) - ./storcli64 /c0 show pr gives segmentation fault on PPC with more than 64 VDs
SCGCQ00755063 - (Closed) - Add support bits for uneven-span and SSHA support
SCGCQ00765712 - (Closed) - StorCLI is not updated with the error Message for all new MFI_STAT added in mfistat.h
SCGCQ00786895 - (Closed) - MR 6.6 CTRL-R: The warning message is not shown when user tries to create CCVD greater than max configurable SSC size.
SCGCQ00786830 - (Closed) - In 2 iMR controller environment switching between iMR cards hits MonTask
SCGCQ00758768 - (Closed) - Incorrectness in the confirmation popupmenu while creation of VD from available size.
SCGCQ00760689 - (Closed) - CTRL+R: not able to set cacheflushint value to 255 for MR card.
SCGCQ00760972 - (Closed) - Error code coming as "Unknown" while importing Foreign Configuration, when controller is in Safe Mode
SCGCQ00696872 - (Closed) - Consistent Sorting of Controllers for End Users in Customer Facing Tools
SCGCQ00735171 - (Closed) - Implemented the storcli command to print SATA drive's phy error counters and reset them.
SCGCQ00755527 - (Closed) - Enable SED on JBOD
SCGCQ00711564 - (Implemented) - RRB 71 - enable SED support for iMR JBOD
SCGCQ00750164 - (Closed) - RRB 71 - enable SED support for iMR JBOD
SCGCQ00757473 - (Closed) - LD Deletion stalling all IOs on oem HBA 12.12.0-0178
SCGCQ00696872 - (Closed) - Consistent Sorting of Controllers for End Users in Customer Facing Tools
SCGCQ00735171 - (Closed) - Implemented the storcli command to print SATA drive's phy error counters and reset them.
SCGCQ00755527 - (Closed) - Enable SED on JBOD
SCGCQ00711564 - (Implemented) - RRB 71 - enable SED support for iMR JBOD
SCGCQ00750164 - (Closed) - RRB 71 - enable SED support for iMR JBOD
SCGCQ00757473 - (Closed) - LD Deletion stalling all IOs on oem HBA 12.12.0-0178


Installation:
=============
Use StorCLI to flash the SAS controllers.  These tools can be downloaded from the support and download
section of www.lsi.com.

Command syntax:  
StorCLI /c0 download file=mr3108fw.rom




Component:
=========
SAS MegaRAID Firmware Release for MegaRAID Controllers
Release date: 10/01/14


Version Numbers:	
===============
Current Package Details:
Firmware Package:24.6.0-0023 (MR 6.5)
Firmware 4.260.00-3735
ROMENV 1.09
BootBlock 3.02.00.00-0001
NVDATA  3.1408.00-00
UEFI_Driver 0x06090700 (SIGNED)
Hii v03.10.09.00(SIGNED)
FCODE 4.16.08.00
BIOS 6.20.04
Ctrl-R 5.07-0006
PCLI 1.07.05

Previous Package Details:
Firmware Package: 24.5.0-0015 (MR 6.4)
Firmware 4.250.00-3569
ROMENV 1.09
BootBlock 3.02.00.00-0001
NVDATA 3.1406.00-0075
UEFI_Driver 0x06080500 (SIGNED)
Hii v03.09.06.00 (SIGNED)
FCODE 4.16.08.00
BIOS 6.19.05.0
Ctrl-R 5.06-0003
PCLI 1.07.05



Firmware:
SCGCQ00584299 - (Closed) - R5/R6 SSD 4K Random Write IOps lower than expected (at a QD fo 256)
SCGCQ00609808 - (Closed) - R0, R5, R6 read bandwidth drops abruptly at 256K block size with 24Dr SATA SSD configuration
SCGCQ00630717 - (Closed) - SED: Montask fdeSM.c seen when using previously locked FDE drives.
SCGCQ00649088 - (Closed) - Continuous Message in log "logGet: Found invalid event at fc570abc"
SCGCQ00692488 - (Closed) - Assertion failure while running sequential reads on read ahead volume
SCGCQ00693153 - (Closed) - The VDs when migrated from 6.4 to 6.5 will no longer be hidden from OS
SCGCQ00699179 - (Closed) - Head of Queue Functionality is not getting executed
SCGCQ00701317 - (Closed) - Change deviceExposure value from MegaMon for better debugging
SCGCQ00704603 - (Closed) - OEM firmware will crash or hang on unsupport cmd
SCGCQ00705240 - (Closed) - Not able to set OEM value apart from 6
SCGCQ00705302 - (Closed) - MR 6.5 FW:returning status failure while associating raid arrays to cachcade array.
SCGCQ00710588 - (Closed) - MR6.5:Caching not happening after rebuild completed on R1 CCVD with BGIO's running on SVD
SCGCQ00715282 - (Closed) - initialize the tempsensor to default full mode on restart
SCGCQ00715395 - (Closed) - Virtual drive missing after online controller reset
SCGCQ00715413 - (Closed) - Controller resets to its earlier time after OCR
SCGCQ00719591 - (Closed) - Cannot change drive state while removing & inserting drive during recon and cannot start manual rebuild after recon.
SCGCQ00724968 - (Closed) - Rebuild not starting on SSD, when Enclosure PD’s[used for SVD] and SSD's[used for CCVD] are foreign imported together
SCGCQ00725070 - (Closed) - I/Os continue to run after hiding the VD for second time
SCGCQ00726288 - (Closed) - New CMD_BLOCK added to initialize temperature sensor
SCGCQ00732059 - (Closed) - Battery Learn Cycle is not getting initiated after CLBAD set for more than 3 mins.
SCGCQ00734705 - (Closed) - Data TLB error seen on switching from FPM to HPM with OCR
SCGCQ00643509 - (Closed) - Incorrect Max number of disks shown by LSA for Spanned Raid levels in IMR controller during Volume creation.
SCGCQ00685640 - (Closed) - 3108 MR solution reports supercap is 254 C when actual ambient temp is -2 C
SCGCQ00695428 - (Closed) - FW crashes during OS installation
SCGCQ00696619 - (Closed) - MR 6.5 : Firmware breaks to Montask on line ../../raid/cache.c
SCGCQ00696625 - (Closed) - PSOD observed while changing controller property 'enableJBOD' to 1.
SCGCQ00701744 - (Closed) - FW got hung up during error handling of sence 0B/47/xx
SCGCQ00704600 - (Closed) - OEM firmware will crash when get to the end of "next devhandle"
SCGCQ00705255 - (Closed) - Average Read response time for RAID 1 configuration is never calculated
SCGCQ00712125 - (Closed) - iMR:6.5-Exception in core 0 is seen when drives are spun down and an ocr is triggered
SCGCQ00716517 - (Closed) - MR6.5_FW: Pinned cache is not Flushing after second Foriegn Import while PD is removed in First Foriegn Import
SCGCQ00725087 - (Closed) - Head Of Queue leads to negative delays between rebuild cycles
SCGCQ00731286 - (Closed) - Core 0 exception in line 243 in file ../raid.c encountered when GG update fails with Stress IOs on all WB VDs
SCGCQ00736509 - (Closed) - "Restore done successfully" prints available in firmware logs even after cache data is lost.
SCGCQ00736863 - (Closed) - Inconsistent values reported for Write response times for RAID 1 VD's with HOQ and no IO
SCGCQ00742024 - (Closed) - Disabling Control of HOQ Rebuild through applications
SCGCQ00649094 - (Closed) - SSD VD association to CC VD through storcli shows success but actually it is not associated
SCGCQ00692393 - (Closed) - LmidFifo Isr observed during drive pull with IO's on R5 VD
SCGCQ00696256 - (Closed) - FW hit the Montask while running the TASIO
SCGCQ00724961 - (Closed) - improper setting of targetSpeed in PCI link control 2 register to change pci link rate resulted in adapter reset.
SCGCQ00713615 - (Closed) - MR6.4 random write throughput on 24SATA SSD R5/R6 configuration regressed compared to MR6.3
SCGCQ00664261 - (Closed) - Port CQ Defect 421011 IOP: Asynchronous reset may cause system reset and PCIe Link Down
SCGCQ00688064 - (Closed) - Foreign configuration import is successful but drive state still remains unconbad foreign during copyback
SCGCQ00704310 - (Closed) - Disable DCR ERR LOG interrupt to fix DIS issue
SCGCQ00712480 - (Closed) - Bypass cache for sequential writes which are greater than or equal to 128 KB
SCGCQ00703189 - (Closed) - "Prepare For Removal" does not work on a PD when drive erase is in progress
SCGCQ00700829 - (Closed) - MPI 2.5: BIOS Page 1 additions
SCGCQ00685820 - (Closed) - MPI 2.5: distribute Target Command Buffers Received across multiple reply queues
SCGCQ00683317 - (Closed) - Dirty Lba sorting is removed for fully SSD RAID Arrays.
SCGCQ00682656 - (Closed) - Use region lock engine's capability to release local message identifier along with releasing region locks
SCGCQ00634798 - (Closed) - Enable FastPath for all LSI Controllers
SCGCQ00642226 - (Implemented)   - Implement HEAD OF QUEUE to improve Rebuild performance over MR controllers
SCGCQ00696862 - (Closed) 	- Ability to Support VPD Information in MR 6.3
SCGCQ00652300 - (Closed) 	- MegaRAID power throttling implementation
SCGCQ00650087 - (Closed) 	- Implemention to report HDD Temperature for Drives which does not support exceptional log page
SCGCQ00656611 - (Implemented)   - Add ability to take a VD offline, bring back VD online
SCGCQ00667140 - (Port_Complete) - OEM Additional update required ontop of CritCom 66:PCIe SERDES parameter setting updates
SCGCQ00675820 - (Port_Complete) - Updated long term WA for PPC errata #46
SCGCQ00680739 - (Port_Complete) - Custom KeyGen Solution
SCGCQ00682665 - (Port_Complete) - Cache offload failure with pinned cache on R5 VD
SCGCQ00685986 - (Port_Complete) - Add better debugging functionality for Alarm related field issues
SCGCQ00687878 - (Port_Complete) - Ctrl+R is not enabled after downgrade and upgrade FW
SCGCQ00695333 - (Port_Complete) - Serial prints getting jumbled up due to print message inside spourious interrupt handler.
SCGCQ00695385 - (Port_Complete) - 4K VDs missing after server reboot
SCGCQ00695393 - (Port_Complete) - Postpone CC on boot for 5 minutes
SCGCQ00702593 - (Port_Complete) - Issue a complete Gas Gauge reset on every boot
SCGCQ00703177 - (Port_Complete) - Update Gas Guage Safety Status register bit positions
SCGCQ00704303 - (Port_Complete) - Implemented Gas gauge FW update functionality .
SCGCQ00710111 - (Port_Complete) - Reduce the monitoring time of CL (Capacitor Learning) flag in BQ33100 Operation Status register to 5Sec when a learn command is issued.
SCGCQ00711812 - (Port_Complete) - Change SuperCap auto learn cycle period to 27 days and 22 hours.
SCGCQ00712593 - (Port_Complete) - Prowl x24 not spinning up all disks (1.8 SSDs)
SCGCQ00713099 - (Port_Complete) - OEM Data Corruption is taking place on Windows OS installed on top of ESX 5.5 U1 OS.
SCGCQ00714527 - (Port_Complete) - Internal development defect to correct Module version validation logic for Gas Gauge firmware update
SCGCQ00719724 - (Port_Complete) - FW doesn't do an Online Firmware Update (OFU) after a successful Gas Gauge firmware update .
SCGCQ00722959 - (Ready) - Higher Jetstress average database writes latency
SCGCQ00734987 - (Port_Complete) - The cache policy of Virtual Drives(VDs) do not change to Write-Through(WT) if FAULT is asserted and there is no indication in BQ33100 Safety Status register.
SCGCQ00671448 - (Port_Complete) - ONFI: To properly handle the OCR case with RESET Status Register.
SCGCQ00673627 - (Port_Complete) - Supercap properties reports wrong in storcli
SCGCQ00687692 - (Port_Complete) - Foreign configuration import failure for spanned array with pinned cache
SCGCQ00688780 - (Port_Complete) - Enable FastPath for all LSI Controllers
SCGCQ00692233 - (Port_Complete) - Make sure numbers show up in Ctrl_R for drive Ids when drives connected through passive backplane
SCGCQ00693961 - (Port_Complete) - [R630] Failed LED on 10HD BP does not light correctly
SCGCQ00706922 - (Port_Complete) - Cache offload not triggered on few servers rarely
SCGCQ00714523 - (Port_Complete) - Performing reboot immediately after updating the Gas Gauge (before learn completes) results in the FW reporting an update error on every subsequent boot.
SCGCQ00723647 - (Port_Complete) - Flashing wrong Gas Gauge image (or any bad image) will force VDs to WT(Write Through) and fail and there is no path back to WB other than rebooting
SCGCQ00757273 - (Port_Complete) - Performance degrade up to 35% in Write Back enabled 100% Random Writes as compared to MR 6.3 FW
SCGCQ00679766 - (Port_Complete) - MR 6.4 : MonTask: line 4699 in file ../../raid/ld.c seen on iMR FW during boot to OS with R0 and PRL11 VD
SCGCQ00695622 - (Port_Complete) - PPC exception seen during reboot test case on a VD
SCGCQ00696014 - (Port_Complete) - OEM Data Corruption is taking place on Windows OS installed on top of ESX 5.5 U1 OS.
SCGCQ00711847 - (Port_Complete) - Cache offload not triggered on few servers rarely
SCGCQ00719701 - (Port_Complete) - When supercap learn is pending (overdue) at boot, exposure time in WB mode is seen for up to 1 minute 5 seconds.
SCGCQ00730750 - (Port_Complete) - Flashing wrong Gas Gauge FW will succeed if flashed after good Gas Gauge FW is flashed and before the learn starts
SCGCQ00695390 - (Port_Complete) - Serial prints getting jumbled up due to print message inside spourious interrupt handler.
SCGCQ00703187 - (Port_Complete) - When we attempt to retrieve iMR Thunderbolt controller firmware logs using an application, we see some lines that are wrapped without starting on a new line.
SCGCQ00704221 - (Port_Complete) - CSET: Continuous Message in log "logGet: Found invalid event at fc570abc" - (SCGCQ00649088)
SCGCQ00716842 - (Port_Complete) - Preventing a specific supercap error message being printed in term log
SCGCQ00734876 - (Port_Complete) - Few un-acceptable prints in serial log.
SCGCQ00678585 - (Port_Complete) - Controller in JBOD mode is allowing a PD designated as a Hot Spare to be a configured via OOB as the boot drive
SCGCQ00693962 - (Port_Complete) - RAID 5 Random Writes on SSDs
SCGCQ00695613 - (Port_Complete) - 4K VDs missing after server reboot
SCGCQ00700868 - (Port_Complete) - When we attempt to retrieve iMR Thunderbolt controller firmware logs using an application, we see some lines that are wrappedwithout starting on a new line.


BIOS:
SCGCQ00720411 - (Closed) - OpROM 240VD: Not able to boot to OS from the VD whose target ID is greater than 128
SCGCQ00455591 - (Closed) - Memory access issue for Mercury when loading Ctrl R
SCGCQ00693494 - (Closed) - setting deviceExposure greater than or eaual to 128 will show wrong VD handled by bios
SCGCQ00455597 - (Closed) - Memory allocation: Allocate only two 64k
SCGCQ00736737 - (Port_Complete) - xprintf display issue when FW reports percentage for device scan
SCGCQ00709995 - (Port_Complete) - OEM wants the battery status text in BIOS to change from "missing" to "N/A" for iMR solutions.



NVDATA:
Numerous changes for specific customers

UEFI Driver:
SCGCQ00691044 - (Closed) - Code refactor effort: Hii Image buffer clean-up
SCGCQ00688789 - (Closed) - DHP: Remove default value from numeric primitive that is present under suppressif
SCGCQ00732773 - (Closed) - UEFI Driver: If the platform contains UEFI Spec Rev < than 2.3.0, then don't HII
SCGCQ00756810 - (Closed) - PKG 9 HII form/When you have a a critical message such as missing VDs, after select "C" <ENTER>, it will show an assert
SCGCQ00726723 - (Closed) - Ext/SCSI PassThru: UEFI Driver not filling direction flag correctly for Read
SCGCQ00696656 - (Closed) - Update Mbox value for 240VD Support
SCGCQ00650086 - (Implemented) - UEFI Driver UDK2010 complaince
SCGCQ00688987 - (Port_Complete) - Don't let user boot to OS until user discards dirty cache
SCGCQ00736761 - (Port_Complete) - Return health status failed if we have returned device error from Start()
SCGCQ00756861 - (Port_Complete) - ControllerInfo[CtrlIndex].ControllerHandle got initialized incorrectly or too early
SCGCQ00695249 - (Port_Complete) - Safe guard: Return health status failed if platform calls GetHealthStatus w/ NULL handle after we return intermediate status
SCGCQ00716623 - (Port_Complete) - For OEM change memory type from EfiRuntimeServicesData to EfiMemoryMappedIO
SCGCQ00716622 - (Port_Complete) - For OEM dont free the host memory during disconnect/unload process


HII:
SCGCQ00689437 - (Closed) - Schedule consistency check gives an error message on Apply changes
SCGCQ00692849 - (Closed) - When Controller is in Safe Mode don't remove UCM formset
SCGCQ00696506 - (Closed) - Grammaical errors in HII warning message during FW Flash.
SCGCQ00691938 - (Closed) - HII: Return device error when MR_DCMD_CTRL_PROPERTIES_SET fails.
SCGCQ00700304 - (Closed) - MR_240VD:System fails to boot into SETUP[F2] and displays blank screen with 160 and 240 VDs
SCGCQ00716628 - (Closed) - To Handle Code collab review Defect for SCGCQ00700199
SCGCQ00700199 - (Closed) - After selcting Discard pinned Cache from Controller Management, Form will be taken to Cache and Memory after success.
SCGCQ00702200 - (Closed) - Firmware Update feature fails to update firmware in HII
SCGCQ00709543 - (Closed) - gHiiDriver.ExtLDSupport should be Filled with appropriate value before it's used
SCGCQ00702196 - (Closed) - Asserts seen before loading HII
SCGCQ00704309 - (Closed) - HII: Question value mismatch message seen in Enclosure Management screen.
SCGCQ00714530 - (Closed) - HII: Firmware Update - On selecting empty folder, hang is seen.
SCGCQ00731567 - (Closed) - use hwPresent.memory to determine iMR
SCGCQ00706817 - (Closed) - MR_240VD: Virtual Drive properties[Read/Write/IO Policy] gets changed after VD creation from HII
SCGCQ00710064 - (Closed) - Handline code collaborator Defect for SCGCQ00709543
SCGCQ00716636 - (Closed) - Incomplete SAS Address
SCGCQ00705577 - (Closed) - Unable to select the second enlcosure when multiple enclosures are connected to a controller .
SCGCQ00723184 - (Closed) - Capacity Allocation in drive group properties is inappropriate
SCGCQ00730496 - (Closed) - MR: HII gives the option to set -head of queue for raid 0
SCGCQ00742103 - (Closed) - Remove Head Of Queue rebuild feature
SCGCQ00704216 - (Closed) - HII hangs on selecting "View Drive Group Properties"
SCGCQ00734447 - (Closed) - Patrol read prop page gives an error message on Apply changes
SCGCQ00642228 - (Implemented) - Implement Head of Queue drive rebuild for MegaRAID controllers
SCGCQ00650085 - (Implemented) - HEFU HII UDK2010 complaince
SCGCQ00689070 - (Closed) - MR 6.2- Negative test HII browser- Mixing unsupported drives message needs update
SCGCQ00664753 - (Closed) - Ability to enable/disable JBOD mode in HII & CTRL-R
SCGCQ00656614 - (Closed) - Add ability to take a VD offline, bring back VD online
SCGCQ00688454 - (Implemented) - HEFU HII UDK2010 complaince
SCGCQ00695063 - (Port_Complete) - Call UninstallStoreLib when we call StopControllerHiiImpl function
SCGCQ00695068 - (Port_Complete) - In HII Create VD option is enabled when resconstruction is in progress (on partial VD)
SCGCQ00695072 - (Port_Complete) - H730P- Not showing PD to assign as DHS to R50/ R60 VD if PD is of lesser size than largest PD in V
SCGCQ00695223 - (Port_Complete) - OEM 9.1.2 - HII: Contents of few help messages are improper
SCGCQ00728678 - (Port_Complete) - UEFI creating a new VD in a "hole" in the drive group free space, hangs when viewing drive group properties
SCGCQ00756855 - (Port_Complete) - Chk the err status for HL_Get_PD_List() and HL_Get_PD_Info in UF002_PrepareData() + check Driver handle if index is valid


Ctrl-R:
SCGCQ00720815 - (Closed) - Ctrl+R: <prev> and <next> links in Properties Page both redirects to next page and vice versa.
SCGCQ00716584 - (Closed) - /c0 show all page are having some incorrectness in controller information
SCGCQ00704259 - (Closed) - Firmware Hangs/breaks while creation of RAID1 with GHS
SCGCQ00738006 - (Closed) - Incorrectness in the popup for Virtual drive Expansion
SCGCQ00712982 - (Closed) - Verify StorCLI warns on destructive operations - R0 with 2 x SED drives Deleted with no warning.
SCGCQ00729691 - (Closed) - fault(coredump) observed on executing ./storcli /c1/v63 show all for 64th cachecade VD in ubuntu14.04
SCGCQ00707450 - (Closed) - While creating cachecade vd with one SAS-SSD;Raid 1 option is also enabled
SCGCQ00710520 - (Closed) - Ctrl+R_6.5: Incorrectness in Help file generated by pressing F1
SCGCQ00712171 - (Closed) - While creating cachecade vd with one SAS-SSD;Raid 1 option is also enabled
SCGCQ00730497 - (Closed) - MR: ctrl-r gives the option to set -head of queue for raid 0
SCGCQ00727409 - (Closed) - CTRL-R:Incorrectness in CTRL Management while launching Manage Link Speed
SCGCQ00706013 - (Closed) - VD I/O policy changes from cached to direct when VDs are created from Ctrl-R
SCGCQ00725545 - (Closed) - In foreign Config Preview VD Size is coming as NA instead of actual size,when VD state is foreign.
SCGCQ00735369 - (Closed) - not able to navigate through "join mirror -choose option" window
SCGCQ00730412 - (Closed) - Incorrectness in the popup generated during deletion of Cachecade associated Virtual Drive
SCGCQ00742106 - (Closed) - Remove Head Of Queue rebuild feature
SCGCQ00731292 - (Closed) - Unable to see PD(s) Count in Cachecade RAID1 w.r.t to Cachecade RAID0
SCGCQ00709969 - (Closed) - Ctrl+R_6.5: Showing incorrectness in Memory Size in Properties Page2
SCGCQ00719102 - (Port_Complete) - Date Created field in storCLI display is incorrect after creating a VD in MSM using SWR versio 1.34 on ALM2-16
SCGCQ00732019 - (Active) - CLI command to access/modify Immediate IO
SCGCQ00694663 - (Port_Complete) - Simulator files check-in with changes in new API.
SCGCQ00732058 - (Port_Complete) - CLI command to access/modify Drive Activity LED
SCGCQ00699269 - (Port_Complete) - storcli is displaying only information of one enclosure when all option is given for phyerrorcounters, on multiple enclosures


Installation:
=============
Use StorCLI to flash the SAS controllers.  These tools can be downloaded from the support and download
section of www.lsi.com.

Command syntax:  
StorCLI /c0 download file=mr3108fw.rom



Component:
=========
SAS MegaRAID Firmware Release for MegaRAID Controllers
Release date: 08/08/14


Version Numbers:	
===============
Current Package Details:
Firmware Package: 24.5.0-0015 (MR 6.4)
Firmware 4.250.00-3569
ROMENV 1.09
BootBlock 3.02.00.00-0001
NVDATA 3.1406.00-0075
UEFI_Driver 0x06080500 (SIGNED)
Hii v03.09.06.00 (SIGNED)
FCODE 4.16.08.00
BIOS 6.19.05.0
Ctrl-R 5.06-0003
PCLI 1.07.05

Previous Package Details:
Firmware Package: 24.3.0-0050 (MR 6.3)
Firmware 4.230.20-3532
ROMENV 1.09
BootBlock 3.02.00.00-0001
NVDATA 3.1403.00-0079
UEFI_Driver 0x06060A01
Hii 03.07.12.01
FCODE 4.16.08.00
BIOS 6.17.04.0
Ctrl-R 5.04-0002
PCLI 1.07.05


Bug Fixes and Enhancements:
===========================
Firmware:
SCGCQ00651356 - (Closed) - Cache offload not triggered on few servers rarely
SCGCQ00663028 - (Closed) - Patrol read is in progress even after issuing stop patrol read command through App
SCGCQ00669540 - (Closed) - PPC exception seen during reboot test case on a VD
SCGCQ00672868 - (Closed) - Firmware crash @line 1266 in file ../../raid/1078dma.c while Clearing the configuration when reconstruction going on.
SCGCQ00677415 - (Closed) - Patrol read suspended message continues to appear even after it is stopped
SCGCQ00678651 - (Closed) - Firmware breaks into montask at line : 931 in file ../../raid/bladeDMA.c
SCGCQ00685276 - (Closed) - Configuration lost on Controller while importing the configuration just as the drives start to show in discovery.
SCGCQ00687265 - (Closed) - Exception in Core 0 on rebooting the System while reconstruction is in progress
SCGCQ00695573 - (Closed) - Performance degrade up to 35% in Write Back enabled 100% Random Writes as compared to MR 6.3 FW
SCGCQ00637612 - (Closed) - eccBucketSize set to threshold value 15 upon changing its value to 0 or 1
SCGCQ00638190 - (Closed) - PD is reported as a 'HSP by storcl64 which is neither DHSP nor GHSP.
SCGCQ00644645 - (Closed) - FW Breaks while importing Foreign Config(BS Assertion Failure while flushing the pinned cache)
SCGCQ00652759 - (Closed) - set the BBUEnable flag as per the cacheoffload requirement
SCGCQ00685001 - (Closed) - patrolread suspended message appears even after resuming it and while progress in PR
SCGCQ00604480 - (Closed) - locate behavior will incorrect light some drive LED not located after some loop locate test on 3108 MR+PMC Expander
SCGCQ00613357 - (Closed) - Able to perform PD format and PD secure erase operations simultaniously
SCGCQ00620701 - (Closed) - All the menu items in MSM such as create VD are highlighted when the controller is in safe mode.
SCGCQ00624038 - (Closed) - Changed the order of evaluation to compiler independent
SCGCQ00633906 - (Closed) - Disable the HW assisted L3 cache flush prior to offload in case of powerloss.
SCGCQ00634405 - (Closed) - Data Misscompare found on Raid 60 when pinned cache is created on Raid 50.
SCGCQ00636277 - (Closed) - Battery Retention Test not reporting test result.
SCGCQ00642679 - (Closed) - Assertion failure in ../../raid/cache.c at line 2772
SCGCQ00653832 - (Closed) - Delay in OCR with IO timeouts is seen when Security is enabled
SCGCQ00658494 - (Closed) - FW issuing false event saying VD policy change from WT to WB even the memory module is bad
SCGCQ00664511 - (Closed) - Enable DIS feature in FW
SCGCQ00672040 - (Closed) - MonTask: line 7204 in file ../../bbu/onfi.c with power cycle script
SCGCQ00673991 - (Closed) - ocr does not trigger after deleting nvram
SCGCQ00677803 - (Closed) - Cache offload failure with pinned cache on R5 VD
SCGCQ00679787 - (Reworked) - Foreign configuration import is successful but drive state still remains unconbad foreign during copyback - SingleNode
SCGCQ00681033 - (Closed) - Assertion in ../../raid/raidscsi.c at line 904 with controller reset while CacheCade toggling for mix of VDs.
SCGCQ00630344 - (Closed) - Coverity Integrity Manager tool defect
SCGCQ00645801 - (Closed) - Getting Question Value mismatch when entering Controller management screen in HII
SCGCQ00655979 - (Closed) - Drive failures observed while issuing a pass through link reset to all phys in a loop
SCGCQ00669055 - (Closed) - Hit a MonTask while running overnight learn cycles with OCR every 10mins
SCGCQ00669713 - (Closed) - Solid amber LED does not reset on a failed SGPIO slot upon device recovery if locate is on before the drive fails
SCGCQ00679180 - (Closed) - Foreign Config fails to import max config
SCGCQ00642473 - (Closed) - Jetstress test fails after completion of rebuild
SCGCQ00661244 - (Closed) - Mismatch in emulation properties observed on importing VD from foreign configuration
SCGCQ00665670 - (Closed) - Join Mirror command with option 2 imports foreign configurations which are not part of broken mirror.
SCGCQ00674868 - (Closed) - observed when OS was formatting the VD in which cluster double medium error injected
SCGCQ00680326 - (Closed) - Failed import VDs with pinned cache after ONFI tranport
SCGCQ00661190 - (Closed) - cache is not getting bypassed for 64 VD;s
SCGCQ00671194 - (Closed) - Failed import a R5 VD with pinned cache after ONFI tranport
SCGCQ00677411 - (Closed) - MonTask: line 6556 in file ../../bbu/onfiBBM.c is seen when you delete NVRAM
SCGCQ00678566 - (Closed) - Automatically VD gets created for mirror arm of 1st VD on joining the mirror arm of 2nd VD as new virtual drive.
SCGCQ00665475 - (Closed) - To properly handle the OCR case with RESET Status Register.
SCGCQ00574358 - (Closed) - Allow UEFI and BIOS to be Enabled/Disabled individually
SCGCQ00523879 - (Closed) - Identify physical location of a target device
SCGCQ00566306 - (Closed) - Add type BIOS for HashImageType.
SCGCQ00569175 - (Closed) - Add product-specific Flag bit to Clean Tool
SCGCQ00621554 - (Closed) - Refactor Buffer Manager to avoid overheads with various lists
SCGCQ00648403 - (Closed) - Roll back latency improvements from MR6.4
SCGCQ00660441 - (Closed) - Short term fix for PPC476 Errata
SCGCQ00674506 - (Closed) - Long term work around for PPC 476 Errata #46
SCGCQ00692938 - (Closed) - Remove unwanted prints in sysDMA path
SCGCQ00602088 - (Closed) - Command timeouts with cdb=ff ff ff ff
SCGCQ00669013 - (Closed) - Disable cache bypass in least latency mode
SCGCQ00674233 - (Closed) - F/w changes to set deviceExposure default from NVDATA
SCGCQ00524743 - (Opened) - Enable support L3 auto-flush on power fail when BBU is connected
SCGCQ00586309 - (Closed) - Enable cache bypass for better performance with large writes on WB volumes
SCGCQ00599993 - (Closed) - Remove EBBU code as it is no longer needed
SCGCQ00634750 - (Closed) - Requirement for 512e implementation changes
SCGCQ00654566 - (Closed) - Work Around for PPC 476 Errata #46 in MR Firmware
SCGCQ00626667 - (Closed) - Add Mirror Join functionality
SCGCQ00654568 - (Closed) - Work Around for PPC476 Errata #46 in iMR Firmware
SCGCQ00599829 - (Closed) - Refactor DM for modularity
SCGCQ00634792 - (Closed) - Need to support both SAS and SATA disks in the same dual path/expander jbod/backplane
SCGCQ00642323 - (Closed) - Driver support for read IO load balance on more a >2 drive R1 volume
SCGCQ00589296 - (Closed) - Misc code cleanup for performance improvement
SCGCQ00556387 - (Port_Complete) - VPD (Vital Product Data) needs to identify PCB hardware level
SCGCQ00564594 - (Port_Complete) - Output async event message to upper layer when it detected "Write Timeout" in between on-board flash
SCGCQ00574402 - (Port_Complete) - Display the NCQ enabled/disabled status of every SATA disk drive in the output of StorCLI and MegaCLI
SCGCQ00605439 - (Port_Complete) - FW debugger scrolls continuous message and eventually resets after deleting Source VD during a Cachecade disassocation
SCGCQ00609779 - (Port_Complete) - Add Fastpath Support by Default for a particular OEM.
SCGCQ00619496 - (Port_Complete) - Storecli reporting incorrect values for tfm and supercap date of manufacture
SCGCQ00630129 - (Port_Complete) - Bad battery warning message that comes up during POST isn't aligned properly.
SCGCQ00630133 - (Port_Complete) - Static analysis tool defects
SCGCQ00642804 - (Port_Complete) - Wrong behavior of Break Mirror operation on starts rebuild
SCGCQ00643486 - (Port_Not_Required) - Getting Question Value mismatch when entering Controller management screen
SCGCQ00651193 - (Port_Not_Required) - Battery learn cycle continues to more than one cycle even FW has marked it as bad in previous reboot
SCGCQ00651381 - (Port_Not_Required) - DC observed upon performing OCR on a degraded R1 (AWB).
SCGCQ00656141 - (Port_Complete) - CacheCade data loss after reboot
SCGCQ00662365 - (Port_Complete) - Write buffer flash programming support
SCGCQ00663056 - (Port_Complete) - CC doesn't correct medium error in P drive
SCGCQ00666941 - (Port_Complete) - Start a learn even if the SuperCap is not completely charged.
SCGCQ00666982 - (Port_Complete) - Change the cache policy of Virtual Drives(VDs) to Write Through(WT) if SuperCap temperature goes above 60 degree Celsius.
SCGCQ00667965 - (Port_Complete) - CS2.0: Coverity defects (11619, 14267, 14334)
SCGCQ00675271 - (Port_Complete) - Updated long term WA for PPC errata #46
SCGCQ00675820 - (Port_Complete) - Updated long term WA for PPC errata #46
SCGCQ00678184 - (Port_Complete) - MonTask: line 4699 in file ../../raid/ld.c seen on iMR FW during boot to OS with R0 and PRL11 VD
SCGCQ00681040 - (Port_Complete) - PD is reported as a 'HSP by storcl64 which is neither DHSP nor GHSP.
SCGCQ00682665 - (Port_Complete) - Cache offload failure with pinned cache on R5 VD
SCGCQ00690088 - (Port_Complete) - DIS mismatch while running system reboot script with dirty data in DDR
SCGCQ00692999 - (Port_Complete) - Data Corruption is taking place on Windows OS installed on top of ESX 5.5 U1 OS.
SCGCQ00695994 - (Port_Complete) - Serial prints getting jumbled up due to print message inside spourious interrupt handler.
SCGCQ00706936 - (Port_Complete) - Cache offload not triggered on few servers rarely
SCGCQ00714274 - (Port_Complete) - Serial prints getting jumbled up due to print message inside spourious interrupt handler.
SCGCQ00614988 - (Port_Not_Required) - not enough bs found during double Dip power cycle Test
SCGCQ00630137 - (Port_Complete) - Unable to suspend the Patrol Read operation in iMR mode from the HII application
SCGCQ00639588 - (Port_Complete) - Hitting montask line 1930 in file ../../bbu/onfi.c while running FP IO's on degraded VD's
SCGCQ00642810 - (Port_Complete) - Copyback is not start immediately after reconstruction is completed in OS.
SCGCQ00642816 - (Port_Complete) - Send Inquiry after expander responds with Unit Attention Microcode Change
SCGCQ00650280 - (Port_Complete) - FW Breaks while importing Foreign Config(BS Assertion Failure while flushing the pinned cache)
SCGCQ00654731 - (Port_Not_Required) - Fw hit montask with machinecheck exception on PD pushpull with IO on R5
SCGCQ00662326 - (Port_Complete) - Prevent data correction in pagefil.sys to happen during Check Consistency after heavy I/O test.
SCGCQ00662532 - (Port_Complete) - locate behavior will incorrect light some drive LED not located after some loop locate test on 3108 MR+PMC Expander
SCGCQ00663057 - (Port_Complete) - Check and resume rebuild after a stipulated time 
SCGCQ00671448 - (Port_Complete) - To properly handle the OCR case with RESET Status Register.
SCGCQ00676945 - (Port_Complete) - For OEM do cache offload for when cache is is dirty (WB and ForceWB modes) and when there is a battery present (WT mode).
SCGCQ00676950 - (Port_Complete) - DHS that becomes GHS does not start rebuilding automatically with an already degraded VD
SCGCQ00679174 - (Port_Complete) - MonTask: line 4699 in file ../../raid/ld.c seen on iMR FW during boot to OS with R0 and PRL11 VD
SCGCQ00682959 - (Port_Complete) - Enter Montask during rebuild after reboot
SCGCQ00714465 - (Port_Complete) - When we attempt to retrieve iMR Thunderbolt controller firmware logs using an application, we see some lines that are wrapped without starting on a new line.
SCGCQ00601065 - (Port_Not_Required) - Getting Question Value mismatch when entering Controller management screen
SCGCQ00619497 - (Port_Complete) - Pinned cache gets flushed to incorrect VD for mirrored RAID levels
SCGCQ00625016 - (Port_Complete) - montask seen with "Assertion failure in line 4168" on running IO on 4K VD.
SCGCQ00628213 - (Port_Complete) - correct when copyback (replace) for R11 can be done.
SCGCQ00630147 - (Port_Complete) - Unable to discard pinned cache in Headless Safe Mode.
SCGCQ00650926 - (Port_Complete) - JetStress average database write latency is above previous generation controller
SCGCQ00651383 - (Port_Not_Required) - Hitting montask line 1930 in file ../../bbu/onfi.c while running FP IO's on degraded VD's
SCGCQ00662330 - (Port_Complete) - (SATA) Failed temperature Capture on when link up/down experienced
SCGCQ00665693 - (Port_Complete) - TFM/BBU error seen with latest TFM FW/VPD
SCGCQ00669083 - (Port_Complete) - Cannot import foreign configuration.
SCGCQ00674858 - (Port_Complete) - Updated long term WA for PPC errata #46
SCGCQ00677304 - (Port_Complete) - Estimated Time Left" shows confusing values
SCGCQ00679755 - (Port_Complete) - Cell Disk With Status not Present Was Found to be Showing a Green Status Light
SCGCQ00679766 - (Port_Complete) -  MonTask: line 4699 in file ../../raid/ld.c seen on iMR FW during boot to OS with R0 and PRL11 VD
SCGCQ00696015 - (Port_Complete) - Data Corruption is taking place on Windows OS installed on top of ESX 5.5 U1 OS.
SCGCQ00623210 - (Port_Complete) - expander not spinning up all disks (1.8 SSDs)
SCGCQ00625642 - (Port_Complete) - Fault LED is not set when drive is bad
SCGCQ00668344 - (Port_Complete) - Coverity defects (11619, 14267, 14334)
SCGCQ00669082 - (Port_Complete) - Limit the number of retries when learn fails to start after firmware issues the learn command.
SCGCQ00601559 - (Port_Complete) - Write buffer flash programming support
SCGCQ00620171 - (Port_Complete) - RAID configured on PD been erased with Normal or Thorough will lost after system reboot/reset
SCGCQ00664887 - (Port_Complete) - converting MR to IMR fails
SCGCQ00670778 - (Port_Complete) - SecureVD erase is not resumed on reboot in ronaldo server.
SCGCQ00673077 - (Port_Complete) - Data corruption after media error correction
SCGCQ00570181 - (Port_Complete) - Deep learn will not start immediately when Relative State of Charge (RSOC) of battery is equal to 95%.
SCGCQ00666938 - (Port_Complete) - If cache offload happens during a relearn, then the Firmware will halt at next boot for the learn completion.
SCGCQ00676948 - (Port_Complete) - I2C Issue - Unintended failures following response timeout
SCGCQ00646713 - (Port_Complete) - Cannot recover data from a recoverable media error after Patrol Read encounters recovery failure for RAID-1
SCGCQ00651316 - (Port_Complete) - Change when checking if copyback can be done on a PD in a PRL11

BIOS:
SCGCQ00626821 - (Closed) - 240VD Support: In Post Restrict to 64 VD only
SCGCQ00629987 - (Closed) - With more than 64 VD's in the configuration, number of Virtual Drives handled by BIOS message is not shown in the POST.
SCGCQ00659974 - (Closed) - OpROM - If there is boot message, BIOS won't detect > 64 VDs
SCGCQ00653048 - (Closed) - AutoSelectBootLd is not working if user has OS in VD > 64
SCGCQ00632011 - (Closed) - Firmware enters faults state after a reboot on flashing firmware with IO in progress.
SCGCQ00682646 - (Closed) - Display the first 64 VDs in the POST (in the same sequence we get it from FW)
SCGCQ00626602 - (Implemented) - VT-d/IOMMU support for iMR - Implement mechanism to allow system BIOS to put entries for iMR mem allocation into proper table
SCGCQ00621895 - (Closed) - WebBIOS of MR card hangs due to bios control mis-direct 
SCGCQ00550388 - (Closed) - Write Caching HBA, JBOD/R0 supported TB controller with 240 SystemPD/LD support
SCGCQ00679070 - (Port_Complete) - Display Warning Message when Preboot Configuration Utility are Disabled and User tries to lunch it

NVDATA:
Numerous changes for specific customers

UEFI Driver:
SCGCQ00638308 - (Closed) - FMP GetImageInfo could result in stack corruption - Code Review Defect ID D26304
SCGCQ00628627 - (Closed) - UEFI Driver- has debug print statements during POST
SCGCQ00628310 - (Closed) - Install FMP on Controller Handle at Start() and the exception
SCGCQ00550389 - (Closed) - Write Caching HBA, JBOD/R0 supported TB controller with 240 SystemPD/LD support
SCGCQ00626601 - (Implemented) - VT-d/IOMMU support for iMR - Implement mechanism to allow system BIOS to put entries for iMR mem allocation into proper table
SCGCQ00635878 - (Port_Complete) - UEFI Driver- has debug print statements during POST
SCGCQ00677776 - (Port_Complete) - Initilize the buffer that we allocate to load HII and return EFI_OUT_OF_RESOURCES if allocation fails
SCGCQ00678154 - (Port_Not_Required) - For OEM dont free the host memory during disconnect/unload process
SCGCQ00679073 - (Port_Complete) - Do not go to WebBIOS due to a bad health status when WebBIOS is disabled in NVDATA.
SCGCQ00644508 - (Port_Complete) - CPU EXCEPTION ERROR (Dont double free the memory)
SCGCQ00644509 - (Port_Complete) - CPU EXCEPTION ERROR (Dont double free the memory)
SCGCQ00644856 - (Port_Complete) - Install FMP on Controller Handle at Start() and the exception
SCGCQ00661595 - (Port_Complete) - Timeout is not passed correctly to FW
SCGCQ00644859 - (Port_Complete) - FMP GetImageInfo could result in stack corruption - Code Review Defect ID D26304
SCGCQ00658168 - (Port_Complete) - ATA Pass thru: Timeout is not passed correctly to FW

HII:
SCGCQ00625438 - (Closed) - Minor Typos and consistency issues in HEFU HII help text
SCGCQ00633320 - (Closed) - Handling code collaborator Defects: SCGCQ00573222 and SCGCQ00568814
SCGCQ00602492 - (Closed) - HII fails to list the foreign configuration
SCGCQ00658674 - (Closed) - Hii - Restrict the user from creating the 65th VD.
SCGCQ00630532 - (Closed) - Consistency Check Start - remove mm/dd/yyyy from the string as the format is out of control of LSI
SCGCQ00624890 - (Closed) - Handling Code Collaborator Defect: SCGCQ00573222
SCGCQ00678695 - (Closed) - Change the Step Value to 0 for all numeric to make sure for free edit instead of Incrementing and decrementing using +/-
SCGCQ00640534 - (Closed) - HII is showing RAID6 and RAID5 levels while creating VD when we have 2 512n drives and 1 4k Drives
SCGCQ00645532 - (Closed) - Update the string for "
SCGCQ00679861 - (Closed) - Not able to create VD with 4k drives 
SCGCQ00637539 - (Closed) - Remove FMP installed on the controller handle in HII
SCGCQ00678603 - (Closed) - HII does not display power state of a PD
SCGCQ00627778 - (Closed) - Address review comments
SCGCQ00672925 - (Closed) - Unable to set spinup drive count in HII
SCGCQ00550390 - (Closed) - Write Caching HBA, JBOD/R0 supported TB controller with 240 SystemPD/LD support
SCGCQ00626605 - (Closed) - Clone SCGCQ00556243 HII-based PCI Inventory - MR) into the mainline
SCGCQ00620259 - (Closed) - Port 240VD change to Tbolt SCGCQ00441334
SCGCQ00634019 - (Closed) - Change the default Setting of Disk Cahce Policy from Unchanged to Disable.
SCGCQ00626591 - (Closed) - Add Mirror Join functionality - PR SCGCQ00521537
SCGCQ00626585 - (Closed) - Requirement for 512e implementation changes - PR SCGCQ00425778
SCGCQ00642232 - (Closed) - Ability to enable/disable JBOD mode in HII
SCGCQ00621285 - (Closed) - Change the wording in HII from Check Consistency to Make data consistent
SCGCQ00652171 - (Port_Complete) - HII is gave a option to start reconstruction from any degraded RAID level to RAID 0.
SCGCQ00677103 - (Port_Complete) - Detail Drives info shows incorrectly in BIOS - unknown characters appearing
SCGCQ00679042 - (Port_Complete) - Enhance strings for Locked foreign config import feature
SCGCQ00644857 - (Port_Complete) - Remove FMP installed on the controller handle in HII
SCGCQ00644858 - (Port_Complete) - RSOD during POST after enabling SecureBoot - HEFU.ROM should report exact size of .EFI image
SCGCQ00661685 - (Port_Complete) - HII reports wrong data under 'Eligible JBOD Drives for conversion' while converting JBOD to UG
SCGCQ00652168 - (Port_Complete) - In HII ,Full initialization is not grayed out for R6 DIF arrays.
SCGCQ00603251 - (Port_Complete) - Creation+ FW updation+ Scan foreign Configuration is disabled/grayed out in HII page
SCGCQ00652424 - (Port_Complete) - change the numeric primitive's maximum from MAX_PHYSICAL_DRIVES to 0xff
SCGCQ00644788 - (Port_Complete) - Enhance help message for PD/VD Operation field
SCGCQ00679036 - (Port_Complete) - After Rebuilding, DHS and Expand VD operations failed to update as per VD properties
SCGCQ00634684 - (Port_Complete) - RSOD during POST after enabling SecureBoot - HEFU.ROM should report exact size of .EFI image
SCGCQ00644575 - (Port_Complete) - Consistency Check Start - remove mm/dd/yyyy from the string as the format is out of control of LSI
SCGCQ00652169 - (Port_Complete) - HII reports wrong data under 'Eligible JBOD Drives for conversion' while converting JBOD to UG
SCGCQ00652170 - (Port_Complete) - HII is showing RAID levels, irrespective of drives to configure a new RAID level.
SCGCQ00679049 - (Port_Complete) - "Make Unconfigured good" option missing in HII even if JBOD's are present in the config
SCGCQ00682962 - (Port_Complete) - creation in HII is showing GB
SCGCQ00644786 - (Port_Complete) - Enhance help message for PD/VD Operation field
SCGCQ00682960 - (Port_Complete) - HII is not displaying the cachecade 512GB warning message

Ctrl-R:
SCGCQ00647392 (DFCT) - join mirror-mirror drive is not seen in join mirror-choose option in CTRL-R
SCGCQ00648182 (DFCT) - Port informations are not displayed in Connector field for the drives attached to antares card.
SCGCQ00663996 (DFCT) - Not able to change emulation properties in CTRL-R for iMR
SCGCQ00666806 (DFCT) - Set factory defaults option is blocking the "prev" button in controller properties page
SCGCQ00666807 (DFCT) - "enable jbod" help file is not opening with f1 option on it.
SCGCQ00667550 (DFCT) - Not able to Manually stop or suspend the copyback operation once started
SCGCQ00677458 (DFCT) - Under Join mirror-choose option page existing drives for second R1 VD are not listed.
SCGCQ00677460 (DFCT) - Montask on joining the mirror arm as new virtual drive when doing with the second array.
SCGCQ00678600 (DFCT) - Gramatical Error in Ctrl-R while modifying SuperCap properties
SCGCQ00625148 (DFCT) - in-appropriate drive state is seen on connecting back the drives in ctrl-r .
SCGCQ00625164 (DFCT) - not able to navigate in the warning message window for having more than 64VD.
SCGCQ00625175 (DFCT) - on having more than 64 VD's and initiating a copyback from ctrl-r will result in montask
SCGCQ00628684 (DFCT) - OEM enclosure connected in multi-path is not showing all ports
SCGCQ00642546 (DFCT) - Help is missing for break and join mirror feature in Control-H
SCGCQ00644056 (DFCT) - Join mirror is not enabled in CTRL-R 
SCGCQ00646220 (DFCT) - Getting an option in join mirror to select both "add new vd" and "existing VD" in ctrl-r
SCGCQ00647015 (DFCT) - LD emulation properties not getting set on updating VD properties
SCGCQ00606059 (DFCT) - Ctrl-R - In iMR controller we are able to set VD properties to write back and cached .
SCGCQ00614734 (DFCT) - unable to cretae VD with property "Write back with BBU"
SCGCQ00615350 (DFCT) - In multicontroller environment unable to enter in to ctrl-R after 1st controller initililization.
SCGCQ00635638 (DFCT) - spelling issue in help file of VD Size.
SCGCQ00630099 (ENHREQ) - Requirement for 512e implementation changes
SCGCQ00632051 (ENHREQ) - Added the OEM check for getting default disk-cache policy in Libmods as Disable.
SCGCQ00634020 (ENHREQ) - Added the OEM check for getting default disk-cache policy in Libmods as Disable.


Installation:
=============
Use StorCLI to flash the SAS controllers.  These tools can be downloaded from the support and download
section of www.lsi.com.

Command syntax:  
StorCLI /c0 download file=mr3108fw.rom












Component:
=========
SAS MegaRAID Firmware Release for MegaRAID Controllers
Release date: 07/09/14


Version Numbers:	
===============
Current Package Details:
Firmware Package: 24.3.0-0050 (MR 6.3)
Firmware 4.230.20-3532
ROMENV 1.09
BootBlock 3.02.00.00-0001
NVDATA 3.1403.00-0079
UEFI_Driver 0x06060A01
Hii 03.07.12.01
FCODE 4.16.08.00
BIOS 6.17.04.0
Ctrl-R 5.04-0002
PCLI 1.07.05

Previous Package Details:
Firmware Package: 24.2.1-0021 (MR 6.2)
Firmware 4.220.40-3267
ROMENV 1.09
BootBlock 3.02.00.00-0000
NVDATA 3.1310.00-0070
UEFI_Driver 0x06030501
Hii 03.05.11.03
FCODE 4.16.08.00
BIOS 6.14.05.0
Ctrl-H 5.03-0005
PCLI 1.07.05


Bug Fixes and Enhancements:
===========================
Firmware:
SCGCQ00568080 - (Closed) - Defect Fix for VPD and inquiry callback issues in DISM
SCGCQ00568134 - (Closed) - Patrolread will not start on any VD after a PR is started, suspended and VD is deleted
SCGCQ00569895 - (Closed) - Defect Fix for Command gets retried infinitely times when drive responds with 0B/47/03 always
SCGCQ00572662 - (Closed) - FW failure during read on 3PD R5 with 1000 CME with skip count 2
SCGCQ00574276 - (Closed) - FW breaks if wrong security key is entered
SCGCQ00575006 - (Closed) - Too many unexpected sense AEN raised by CC during CME recovery on R5
SCGCQ00577680 - (Closed) - spin up tracker dequeue is not handled for case in which TUR error happens even after MAX retries
SCGCQ00580162 - (Closed) - Only 1mb crash dump is getting generated of fw fault
SCGCQ00580847 - (Closed) - not enough bs found during double Dip power cycle Test
SCGCQ00586163 - (Closed) - cache restore failure message displayed though cache restore was successfull
SCGCQ00588173 - (Closed) - Routines to inject bit error in NF and ecc error in DDR for ONFI
SCGCQ00588185 - (Closed) - Mismatch in LD id and target ID during set/reset boot device
SCGCQ00589365 - (Closed) - on breaking the multipath in loop while drives are spinnning up will result in montask
SCGCQ00589728 - (Closed) - FW hangs while creating 64 VDs on the controller with SLES11 SP2 PPC64
SCGCQ00592996 - (Closed) - While running reconstruction from R1 to 4 drive PRL11 with IO,FW hits to MonTask: line 1270 in file ../../raid/1078dm
SCGCQ00593776 - (Closed) - SMART poll needs to issue log sense with page control set to current/ cummulative value
SCGCQ00602556 - (Closed) - Static analysis tool defects
SCGCQ00602665 - (Closed) - Static analysis tool defect
SCGCQ00602726 - (Closed) - Static Analysis Tool defects
SCGCQ00602855 - (Closed) - Static analysis tool defect
SCGCQ00603306 - (Closed) - static analysis tool defects resolution
SCGCQ00603564 - (Closed) - added support for debugqueue
SCGCQ00603779 - (Closed) - Not getting "Clear ldbbm badblocks" options on VD
SCGCQ00611275 - (Closed) - FW goes to kill adaptor to handle partial copy of crash_dump
SCGCQ00612927 - (Closed) - Montask in divert.c seen when injecting 64K consecutive errors on R0 VD, Patrol Read running in background.
SCGCQ00614455 - (Closed) - Static analysis tool defects
SCGCQ00625843 - (Resolved) - PR Progress event is not generated for 1TB/3TB SATA drive
SCGCQ00634578 - (Closed) - Defect fix for kenel panic with iMR Fury with Free BSD driver
SCGCQ00636748 - (Closed) - Running Storcli /C0/CV show or (show all) starts a relearn on supercap issue
SCGCQ00651356 - (Resolved) - Cache offload not triggered on few servers rarely
SCGCQ00451219 - (Closed) - Defect Fix for Online DIF drives are getting punctured after PI enabled R5 VDs are offlined with pinned cache
SCGCQ00466289 - (Cloned_EnhReq) - PDs more than 32 which has configuration, is reporting as JBODs after importing from MR to IMR
SCGCQ00574071 - (Closed) - md5sum mismatch seen on a copied file from R5 VD with CME
SCGCQ00574277 - (Closed) - Power removal of enclosure FW hits to MonTask: line 4056 in file ../../bbu/onfiBBM.c
SCGCQ00586190 - (Closed) - Fix GNU make file compilation
SCGCQ00586341 - (Closed) - Crash Dump Error Handling
SCGCQ00605227 - (Closed) - When OS on VD ,after collecting crash dump file system becomes readable
SCGCQ00606571 - (Closed) - Physical drives go to power save mode just after restarting the server
SCGCQ00610881 - (Closed) - storcli and CtrlR still show new PD information as 4K sector after replacing a 4K sector drive with a 512 sector drive
SCGCQ00630075 - (Resolved) - Unexpected power state change
SCGCQ00631492 - (Resolved) - Media error on Last sector of stripe isn't added to LDBBM list
SCGCQ00524842 - (Closed) - CME logic using overlaid fields in c->rec
SCGCQ00568655 - (Closed) - defect fix for Compilation issue
SCGCQ00593295 - (Closed) - Not able import foreign configuration immediately after breaking the mirror.
SCGCQ00602561 - (Closed) - Static Analysis Tool defects
SCGCQ00560474 - (Closed) - code review change implemented
SCGCQ00563498 - (Closed) - FW should not try to boot iMR mode without informing host if ECC error happens when OS is running.
SCGCQ00576138 - (Closed) - The restore successful and unsuccessful prints to be handled properly
SCGCQ00603086 - (Closed) - Kill adapter is seen while performing CME recovery during Write operation.
SCGCQ00546691 - (Closed) - hostCmdSortingWrites is not updated when VD policy changes(WT/WB)
SCGCQ00531118 - (Closed) - Changes to support PD IO history
SCGCQ00564339 - (Closed) - Enable break mirror support
SCGCQ00567706 - (Closed) - Extened LDBBM table to hold more bad block entires (SCGCQ00295621); with relevent increase in divert nodes.
SCGCQ00574801 - (Closed) - Implemented Fix to Problem [PDs more than 32 which has configuration, is reporting as JBODs after importing from MR to IMR]
SCGCQ00577793 - (Closed) - Moved divert code from iopath region to save memory
SCGCQ00621767 - (Closed) - Update Ptolemy VPD and GasGauge with COL settings for a OEM
SCGCQ00624326 - (Closed) - Disable sgpioSmpPresenceDetect for OEM
SCGCQ00624936 - (Opened) - Add MaintainPdFailHistory clear function
SCGCQ00625006 - (Closed) - Show valid ROC temperatuer
SCGCQ00625044 - (Closed) - Change SES Green/Amber LED behavior
SCGCQ00501179 - (Rejected) - Enable cache bypass for better performance with large writes on WB volumes
SCGCQ00562733 - (Closed) - Support for DIS feature in dual image
SCGCQ00563486 - (Closed) - Make MR to iMR migration generic on TMM fault
SCGCQ00582016 - (Opened) - For OEM, GPIO 39 should toggle low once at SOD
SCGCQ00563795 - (Closed) - Modify MR fw to eliminate four second window where drive swap is not recognized.
SCGCQ00563959 - (Opened) - enhancement of crashdump tool -6.3
SCGCQ00588208 - (Closed) - Adding test routine for the bad block loop test for PR SCGCQ00423195
SCGCQ00564166 - (Closed) - Single image support for ONFI
SCGCQ00455360 - (Closed) - Implement CME solution for "Do not allow 3 minute timer to expire forceing driver to kill fw on CME/disk timeout/etc.
SCGCQ00523966 - (Port_Complete) - Rebuild failed event is not seen when rebuild fails due to LDBBM and SBBM tables getting full (puncturing disabled)
SCGCQ00526627 - (Port_Complete) - Faulty protocol used for changing the Disk Write Cache Policy
SCGCQ00530866 - (Port_Complete) - command storclif /c1 start diag duration=0 causes controller card to montask.
SCGCQ00552415 - (Port_Complete) - Modify WCE bit for improved Linux performance
SCGCQ00560388 - (Port_Complete) - adapterOperations.alarmControl is being set to 1 even if controller doesnot have alarm on board
SCGCQ00564367 - (Port_Complete) - BGI operation still running on RAID0 VD even after PI protection disabled
SCGCQ00566951 - (Port_Complete) - LED Blink operation doesn't stop after VD deletion
SCGCQ00579929 - (Port_Complete) - SGPIO functionality is not working when only cable A is connected
SCGCQ00579931 - (Port_Complete) - Review Defect: Potential null pointer derefence
SCGCQ00614997 - (Port_Complete) - Physical drives go to power save mode just after restarting the server
SCGCQ00614998 - (Port_Complete) - Physical drives go to power save mode just after restarting the server
SCGCQ00615001 - (Port_Complete) - Montask in divert.c seen when injecting 64K consecutive errors on R0 VD, Patrol Read running in background.
SCGCQ00617621 - (Port_Complete) - cache restore failure message displayed though cache restore was successfull
SCGCQ00620166 - (Port_Complete) - RAID configured on PD been erased with Normal or Thorough will lost after system reboot/reset
SCGCQ00620168 - (Port_Complete) - RAID configured on PD been erased with Normal or Thorough will lost after system reboot/reset
SCGCQ00620169 - (Port_Complete) - RAID configured on PD been erased with Normal or Thorough will lost after system reboot/reset
SCGCQ00621785 - (Port_Complete) - CME handling of Invader
SCGCQ00622709 - (Port_Complete) - storcli and CtrlR still show new PD information as 4K sector after replacing a 4K sector drive with a 512 sector drive
SCGCQ00624531 - (Port_Complete) - Cache policy of Virtual Drives(VD) does not change to Write Through(WT) mode even after detecting a bad supercap.
SCGCQ00630382 - (Port_Complete) - Add MaintainPdFailHistory clear function
SCGCQ00631230 - (Port_Complete) - SSD causes system to hang at POST
SCGCQ00631232 - (Port_Complete) - Behavior change when FW hit fault code 0x81 (uncorrectable ECC error)
SCGCQ00631474 - (Port_Complete) - Power removal of enclosure FW hits to MonTask: line 4056 in file ../../bbu/onfiBBM.c
SCGCQ00631478 - (Port_Complete) - Adding 2GB DDR and 4GB Flash combination support for NEC Single Image Write.
SCGCQ00637535 - (Port_Complete) - FW hits MonTask: line 1143 in file ../../raid/pd.c on starting VD erase in standard mode.
SCGCQ00638312 - (Port_Not_Required) - FW crash while launching Ctrl+R
SCGCQ00640126 - (Port_Complete) - 9240-4i on OEM motherboard is not getting required memory resources on boot
SCGCQ00640469 - (Port_Complete) - Running Storcli /C0/CV show or (show all) starts a relearn on supercap issue
SCGCQ00640470 - (Port_Complete) - L2/L3 cache error on OEM controllers on reboot
SCGCQ00643455 - (Port_Complete) - Defect fix for kenel panic with iMR Fury with Free BSD driver
SCGCQ00643524 - (Port_Complete) - Defect fix for kenel panic with iMR Fury with Free BSD driver
SCGCQ00643526 - (Port_Complete) - 9240-4i on OEM motherboard is not getting required memory resources on boot
SCGCQ00658583 - (Port_Complete) - Work Around for PPC 476 Errata #46 in MR Firmware
SCGCQ00658585 - (Port_Complete) - Work Around for PPC 476 Errata #46 in iMR Firmware
SCGCQ00675820 - (Port_Complete) - Updated long term WA for PPC errata #46
SCGCQ00682665 - (Port_Complete) - Cache offload failure with pinned cache on R5 VD
SCGCQ00695994 - (Port_Complete) - Serial prints getting jumbled up due to print message inside spourious interrupt handler.
SCGCQ00495877 - (Port_Complete) - disableBatteryWarning should not be reset if changed by user
SCGCQ00498741 - (Port_Complete) - Megamon during Injecting errors to VD with 512e PDs on iMR controller
SCGCQ00552416 - (Port_Complete) - firmware 25.2.0-0013 causes the SEP to not be seen 
SCGCQ00552446 - (Port_Complete) - Implement I2C Slave Address for Sideband Management
SCGCQ00555332 - (Port_Complete) - Transparent Learn Cycle does not kick off and RSOC (Relative State Of Charge) eventually goes down to 0%.
SCGCQ00558037 - (Port_Complete) - Megamon issue when disabling the drive security on a MR controller with spun down FDE drives.
SCGCQ00559322 - (Port_Complete) - EEprom CRC error is detected when WebBIOS is running
SCGCQ00560393 - (Port_Complete) - When attempting to secure LD during RLM, receive option to secure LD, LD not secured (message incorrect/misleading.)
SCGCQ00560476 - (Port_Complete) - Unable to open "Set Patrol Read Properties" in MSM with 2008-iMR
SCGCQ00579928 - (Port_Not_Required) - AdpDiags does not fail when the SAS link is down
SCGCQ00588880 - (Port_Complete) - HDD resume failed during dimmer switch test method.
SCGCQ00631340 - (Port_Complete) - Single image support for ONFI
SCGCQ00637536 - (Port_Complete) - FW hits MonTask: line 1143 in file ../../raid/pd.c on starting VD erase in standard mode.
SCGCQ00671448 - (Port_Complete) - To properly handle the OCR case with RESET Status Register.
SCGCQ00504394 - (Port_Complete) - For a particular OEM, size of some 4TB drives is reported as zero
SCGCQ00563282 - (Port_Complete) - OEM hi-temp warning not being displayed
SCGCQ00567378 - (Port_Complete) - CLI Reporting of TMM VPD
SCGCQ00570249 - (Port_Complete) - SGPIO support not working
SCGCQ00574969 - (Port_Complete) - Retention test failure during stress test 
SCGCQ00596686 - (Port_Complete) - cntr-R fails to show correct PD sector size once PD's swapped to same slot 512B PD with 512e PD type
SCGCQ00621783 - (Port_Complete) - Assertion failure (not enough BS found) in double DIP power cycle test case
SCGCQ00646386 - (Port_Complete) - DIS mismatch while running system reboot script with dirty data in DDR
SCGCQ00679766 - (Port_Complete) - MonTask: line 4699 in file ../../raid/ld.c seen on iMR FW during boot to OS with R0 and PRL11 VD
SCGCQ00696015 - (Port_Complete) - Data Corruption is taking place on Windows OS installed on top of ESX 5.5 U1 OS.
SCGCQ00366011 - (Port_Complete) - FW goes to montask at cache offload.
SCGCQ00530868 - (Port_Complete) - "OOB:Got DCMD, but FW is not ready " meesages are flooding in tty log during OCR .
SCGCQ00553197 - (Port_Complete) - Prevent overtemp warnings while charging between 45C and 50C
SCGCQ00550612 - (Port_Complete) - Do not print VPD86 errors for BP/expander
SCGCQ00556598 - (Port_Complete) - megacli reports battery pack is missing on hot insertion

BootBlock:
SCGCQ00685115 - (Closed) - Memory/battery problems in Focused Regression

BIOS:
SCGCQ00579962 - (Closed) - Initialize deviceExposure with MAX_INT13DISKS instead of 0xFF
SCGCQ00572939 - (Closed) - Make sure all the make file adheres to the latest binary names.
SCGCQ00559095 - (Closed) - Provide an option to limit the max number of INT 13h devices presented to system BIOS

NVDATA:
Numerous changes for specific customers

UEFI Driver:
SCGCQ00618669 - (Closed) - StartHiiBackEnd() has Print statement with %g
SCGCQ00578194 - (Closed) - UEFI Driver should calculate checksum before setting bios data (MR_BIOS_DATA)
SCGCQ00601851 - (Closed) - System hang when we press F1 on second time when we are in HII form
SCGCQ00628627 - (Closed) - UEFI Driver- has debug print statements during POST
SCGCQ00589148 - (Closed) - Diskpart EFI utility can't create partition on a JBOD
SCGCQ00526851 - (Closed) - Support EFI_FIRMWARE_MANAGEMENT_PROTOCOL for controller firmware upgrade.
SCGCQ00579837 - (Port_Complete) - UEFI Driver should calculate checksum before setting bios data (MR_BIOS_DATA)
SCGCQ00606367 - (Port_Complete) - UEFI Driver returns EFI_NOT_FOUND when platform passes valid Target for ExtSPT.BuildDevicePath()
SCGCQ00644509 - (Port_Complete) - CPU EXCEPTION ERROR During CSIOR Stage- After Updating idrac X38 to X39 (Dont double free the memory)
SCGCQ00644856 - (Port_Complete) - Install FMP on Controller Handle at Start() and the exception
SCGCQ00661595 - (Port_Complete) - ATA Pass thru: Timeout is not passed correctly to FW
SCGCQ00644859 - (Port_Complete) - FMP GetImageInfo could result in stack corruption - Code Review Defect ID D26304
SCGCQ00580313 - (Port_Complete) - User can't access RAID HII in UEFI mode after removing a HDD

HII:
SCGCQ00618669 - (Closed) - StartHiiBackEnd() has Print statement with %g
SCGCQ00578194 - (Closed) - UEFI Driver should calculate checksum before setting bios data (MR_BIOS_DATA)
SCGCQ00601851 - (Closed) - System hang when we press F1 on second time when we are in HII form
SCGCQ00628627 - (Closed) - UEFI Driver- has debug print statements during POST
SCGCQ00589148 - (Closed) - Diskpart EFI utility can't create partition on a JBOD
SCGCQ00526851 - (Closed) - Support EFI_FIRMWARE_MANAGEMENT_PROTOCOL for controller firmware upgrade.
SCGCQ00579837 - (Port_Complete) - UEFI Driver should calculate checksum before setting bios data (MR_BIOS_DATA)
SCGCQ00606367 - (Port_Complete) - UEFI Driver returns EFI_NOT_FOUND when platform passes valid Target for ExtSPT.BuildDevicePath()
SCGCQ00644509 - (Port_Complete) - CPU EXCEPTION ERROR During CSIOR Stage
SCGCQ00644856 - (Port_Complete) - Install FMP on Controller Handle at Start() and the exception
SCGCQ00661595 - (Port_Complete) - ATA Pass thru: Timeout is not passed correctly to FW
SCGCQ00644859 - (Port_Complete) - FMP GetImageInfo could result in stack corruption - Code Review Defect ID D26304
SCGCQ00580313 - (Port_Complete) - User can't access RAID HII in UEFI mode after removing a HDD

Ctrl-R:
SCGCQ00644489 (ENHREQ) - Added a new Control to enable/disable JBOD on the page.
SCGCQ00648965 (ENHREQ) - Displaying the Battery status as N/A for iMR cards.
SCGCQ00584991 (DFCT) - current write policy is not getting updated until we press f5 .
SCGCQ00584993 (DFCT) - unable to diplay the reason for difference in write policy
SCGCQ00593822 (DFCT) - Both the Connector information(0-3 & 4-7) is not shown in PD properties while connected in Multipath
SCGCQ00579600 (CSET) - Write policy is not added with writeback with BBu when MFC is set
SCGCQ00579607 (CSET) - VD Erase will be disabled in Ctrl+R when Initlization on particular VD is aborted
SCGCQ00585013 (ENHREQ) - Added the code to unset the boot-device to NONE
SCGCQ00565979 (DFCT) - /c0/pall show and Linkspeed information is not in same in Ctrl-R.
SCGCQ00568182 (DFCT) - showing wrong page number in properties page
SCGCQ00568220 (DFCT) - observing wrong help for "cache flush interval"
SCGCQ00568586 (DFCT) - help file for emergency spare displays wrong
SCGCQ00568725 (DFCT) - Not showing PD to assign as DHS to R50/ R60 VD if PD is of lesser size than largest PD in VD
SCGCQ00568150 (CSET) - showing "BIOS Mode" in both the pages of ctrl mgmt
SCGCQ00568689 (CSET) - Help content is not updated with the Key stroke added
SCGCQ00564149 (CSET) - Added a shortcut Ctrl+S which saves the changes and refreshes the page. The short cut info is added at the bottom status bar.


Installation:
=============
Use MegaCLI or StorCLI to flash the SAS controllers.  These tools can be downloaded from the support and download
section of www.lsi.com.

Command syntax:  
MegaCli -adpfwflash -f mr3108fw.rom -a0
or
StorCLI /c0 download file=mr3108fw.rom







Component:
=========
SAS MegaRAID Firmware Release for MegaRAID Controllers
Release date: 04/02/14


Version Numbers:	
===============
Current Package Details:
Firmware Package: 24.2.1-0021 (MR 6.2)
Firmware 4.220.40-3267
ROMENV 1.09
BootBlock 3.02.00.00-0000
NVDATA 3.1310.00-0070
UEFI_Driver 0x06030501
Hii 03.05.11.03
FCODE 4.16.08.00
BIOS 6.14.05.0
Ctrl-H 5.03-0005
PCLI 1.07.05

Previous Package Details:
Firmware Package: 24.1.1-0006 (MR 6.1)
Firmware 4.210.50-3015
ROMENV 1.09
BootBlock 3.00.00.00-0009
NVDATA 3.1310.00-0062
UEFI_Driver 0x06010600
Hii 03.03.10.00
FCODE 4.14.05.00
BIOS 6.13.00.1
Ctrl-H 5.01-0005


Bug Fixes and Enhancements:
===========================
Firmware:
SCGCQ00651072 - (Closed) - Battery learn cycle continues to more than one cycle even FW has marked it as bad in previous reboot
SCGCQ00645802 - (Closed) - DIS mismatch while running system reboot script with dirty data in DDR
SCGCQ00644122 - (Closed) - Optiomize onfi descriptor setting for offload
SCGCQ00637239 - (Resolved) - FW crash while launching Ctrl+R
SCGCQ00612786 - (Resolved) - Assertion failure in double DIP power cycle test case
SCGCQ00604253 - (Closed) - Elapsed time of Patrol Read in tty log is incorrect
SCGCQ00602839 - (Resolved) - Elapsed time of Reconstruction is incorrect
SCGCQ00598917 - (Closed) - Firmware not taking "SMARTerEnabled" from NVDATA
SCGCQ00598825 - (Resolved) - Rebuild triggered on an incompatible blocksize PD
SCGCQ00573764 - (Closed) - Upgrade 3108 MR FW failing
SCGCQ00569093 - (Closed) - PD erase does not work with SATA SSDs
SCGCQ00558985 - (Closed) - Diagnostics failed after Drives goes to shield state
SCGCQ00549095 - (Closed) - The DQlog.bin is getting corrupted after restarting the service of MRDiag
SCGCQ00546653 - (Closed) - protect the removal of the device when the device is still under initialization
SCGCQ00527932 - (Closed) - BIOS is not getting updated with the DISM progress
SCGCQ00527416 - (Closed) - Running out of free entries in task list due to recursive addition of tasks
SCGCQ00527397 - (Closed) - Wrong information of PD erase progress is shown by the firmware.
SCGCQ00527241 - (Closed) - DM_DISM_LOG_SENSE state is not present in DISM
SCGCQ00524801 - (Closed) - PI enabled VD is importing successfully even though "prevent PI Import" option is enabled
SCGCQ00524040 - (Closed) - Change the CRC filed size
SCGCQ00518855 - (Closed) - Fix the learn issue at powerup
SCGCQ00505401 - (Closed) - LSI_MR Controllers fails to set "FACTORY SETTINGS"
SCGCQ00503341 - (Closed) - VD's switch from Write Back with BBU to Write Through when an OCR is issued and BBU gets disabled.
SCGCQ00503309 - (Closed) - Fix scheduling of hostspare correctly
SCGCQ00503257 - (Closed) - seen DC error while running io's on 6.2 in Dev pull-push setup
SCGCQ00499700 - (Closed) - chaos fails on R6 VD after importing failed R5 VD and one of R1 CacheCade drive
SCGCQ00499455 - (Closed) - Defect fix for MSM doesnot show Create cachecade option
SCGCQ00495896 - (Closed) - To fix task list overflow issue on max config setup
SCGCQ00452322 - (Closed) - FW throws "MPT_LogDiscoveryErrors: SAS_TOPOLOGY_MAX_TOPO_PHYS_EXCEED" when connect 2 in multi-path
SCGCQ00457909 - (Closed) - Assertion failure in ../../raid/raidpci.c at line 10522
SCGCQ00461907 - (Closed) - Read VPD error message on 3108
SCGCQ00464372 - (Closed) - Configurable drives count in iMR reflected wrongly to applications
SCGCQ00466545 - (Closed) - wrong error code displayed and wrong error message for copyback command
SCGCQ00466936 - (Closed) - FW hits to MonTask: while running enclosure power cycle with 4K drives
SCGCQ00469174 - (Closed) - Issue with supercap energy calculations
SCGCQ00470287 - (Closed) - modify scap energy calculation
SCGCQ00471823 - (Closed) - directly attached SATA drive is not detected by controller
SCGCQ00472614 - (Closed) - Dual Context to Single Context switching does not toggle when Cobra expanders are cascaded with EDFB enabled PHY's.
SCGCQ00473420 - (Closed) - Defect fix for Montask observed while installing OS on JBOD
SCGCQ00476945 - (Closed) - Controller Hangs during execution of Storcli command ''/c0 delete termlog''
SCGCQ00477266 - (Closed) - Battery retention test failure during contnuous loop test when there was power failure during erase
SCGCQ00477667 - (Closed) - Battery Enable (BBE) is asserted even when BBU/Supercap not present or even when all LDs are in WT mode
SCGCQ00485545 - (Closed) - TM timeout during enclosure pull while running heavy IO
SCGCQ00486810 - (Closed) - Learn is not completing at powerup
SCGCQ00487215 - (Closed) - 3TB Seagate PD size being reported as 2TB in Apps/Firmware
SCGCQ00493312 - (Closed) - Controller Reset due to Fatal Error with RAID6/60 configuration
SCGCQ00494704 - (Closed) - Elapsed Seconds displayed in firmware logs for background operations progress is improper
SCGCQ00384656 - (Closed) - Kill adapter observed while running IOs on JBODs and VDs
SCGCQ00614723 - (Closed) - CME handling of Invader
SCGCQ00599798 - (Closed) - Issue with Global Hot Spare assignment
SCGCQ00596434 - (Resolved) - Drives connected through enclosure showing wrong slot numbers.
SCGCQ00580415 - (Closed) - issue with MR 24.1.1-003 with JBOD Mode enabled
SCGCQ00557580 - (Closed) - (null) noticed while PD pull-push testing.
SCGCQ00554546 - (Closed) - SMPpassthru is not happening through storlib.
SCGCQ00551614 - (Closed) - System Reboots after issuing the OCR and kernel panic is observed
SCGCQ00524812 - (Closed) - on breaking multipath while drives are spinnning up results in montask
SCGCQ00523544 - (Closed) - Initialize invalid interrupt as part of intInitialize function
SCGCQ00518692 - (Closed) - OEM server hangs after enabling EKM and rebooting.
SCGCQ00505537 - (Closed) - Associating cachecade VD to a secured VD from Storcli does not fail.
SCGCQ00496454 - (Closed) - Offload fails after corrupting BMT1 and BBT 2 address location
SCGCQ00496422 - (Closed) - Adding the log event corresponding to ER SCGCQ00493492
SCGCQ00435204 - (Closed) - BGI kicks in on 5R5 but shows no progress at any point of time.
SCGCQ00446327 - (Closed) - Defect fix for Unable create R0 in HII with 4K drives
SCGCQ00451805 - (Closed) - FW-FW hit 'MonTask: line 243 in file ../../raid/1078in' while issuing OS reboot command on 9340 controller
SCGCQ00470310 - (Closed) - CPLD input GPIO 21 driving when supercap is present and not present
SCGCQ00472407 - (Closed) - Pinned cache gets flushed even after memory battery problem occurs.
SCGCQ00474617 - (Closed) - VD erase restars instead of resuming after reboot.
SCGCQ00477301 - (Closed) - Fix the cset issue
SCGCQ00478707 - (Closed) - Cache Memory Size of controller Information is ZERO
SCGCQ00484448 - (Closed) - Data Corruption observed while running FPIO on VDs; making-breaking multipath in overnight loop.
SCGCQ00486766 - (Closed) - Config loss after OCR during creation of config - when the drives are still spinning up
SCGCQ00486982 - (Closed) - Added an event to notify the user when command times out on PD
SCGCQ00487803 - (Closed) - FDE/SED drives does not reflect as FDE/SED drives.
SCGCQ00605077 - (Resolved) - "Corrected medium error" event is logged for uncorrectable mendium errors during PR
SCGCQ00530495 - (Closed) - To declare block bad at the earliest for the safer side the number of error correction bits shall be reduced
SCGCQ00504346 - (Closed) - Re-enable EKMS for OEM
SCGCQ00421822 - (Closed) - System reboots continuously after flashing Firmware in Solaris _11
SCGCQ00460033 - (Closed) - MonTask: line 7193 in file ../../bbu/onfi.c
SCGCQ00461733 - (Closed) - Kill adapter observed on large setup on enquiring Controller properties while drives spinning up from powersave.
SCGCQ00463368 - (Closed) - coverity tool reported issue 13545(Wrong sizeof argument)
SCGCQ00465561 - (Closed) - restore and flushing cache to PD are not reliable when 1st image of NF mem is corrupted
SCGCQ00470502 - (Closed) - Firmware is allow to create slices in cachecade drivegroup using SMIS utility.
SCGCQ00474005 - (Closed) - EKMS feature for OEM is disabled
SCGCQ00474734 - (Closed) - max temperature bytes read from VPD is should be swapped before using
SCGCQ00477996 - (Closed) - MR_6.2_DISM: FW hung due to DISM discovery failure on pulling the enclosure cable on reboot after running adpbattest.
SCGCQ00488780 - (Closed) - Controller alarm continues to beep after transitioning VD from degraded to optimal state.
SCGCQ00494084 - (Closed) - Handle OEM falut LED behavoir
SCGCQ00556570 - (Closed) - MR6.2_iMR_fury_DM_Issue_TUR
SCGCQ00524903 - (Closed) - In enclosure management page for OEM ,it shows some junk data in HII
SCGCQ00501356 - (Closed) - Controller Reset due to Fatal Error with RAID6/60 configuration
SCGCQ00402933 - (Closed) - CME logic using overlaid fields in c->rec
SCGCQ00460254 - (Closed) - Montask appears on running IO's on 64VD's while changing LD policies
SCGCQ00465672 - (Closed) - Enable OCR by default on GCA builds
SCGCQ00480503 - (Closed) - MR: on FW init, controller post adapter base port missing
SCGCQ00495361 - (Closed) - Invalid "Elapsed Seconds" value for FGI
SCGCQ00531106 - (Closed) - Rebuild and Consistency Check aren't progressed when it is executed by CTL+R
SCGCQ00518734 - (Closed) - Latest API changes in mr.h breaks FW compilation in mrdebug.c
SCGCQ00464536 - (Closed) - Build Issue using GNUmakefile for MR and iMR
SCGCQ00524913 - (Closed) - Storcli command to reset the boot ld on controller fails
SCGCQ00506335 - (Closed) - boot block compile fails because of an erroneous macro definition
SCGCQ00468366 - (Closed) - DATA TLB error faced while powercycle the enclosure during controller initialization 
SCGCQ00490696 - (Closed) - foreign import fails if degraded VD is present in import
SCGCQ00415512 - (Closed) - Toolbox Console Text Display Tool
SCGCQ00451314 - (Opened) - Porting of the PR "spin up changes to accommodate multiple power domains simultaneously" to Invader.
SCGCQ00460871 - (Closed) - Validate the requested blocks for SCSI VERIFY commands on RAID volumes
SCGCQ00466819 - (Closed) - IOCInit multiple Reply Descriptor Post Queue addresses
SCGCQ00471500 - (Opened) - Firmware Change for Pre-boot management tool & boot capability for SPARC
SCGCQ00477817 - (Closed) - add reserved fields to IO Unit Page 7 for future use
SCGCQ00481549 - (Closed) - Disable thermal throttle changes
SCGCQ00493492 - (Closed) - Identifying the DDR, ONFI flash and SCap combination
SCGCQ00518786 - (Closed) - SGPIO back plane requires ramdon slot number support.
SCGCQ00595486 - (Closed) - Increase PCIe Receiver Margin
SCGCQ00595487 - (Closed) - Increase margin in PCIe Rx Serdes
SCGCQ00438437 - (Closed) - obsolete SAS IO Unit Control _TRANSMIT_PORT_SELECT_SIGNAL
SCGCQ00471293 - (Closed) - obsolete "Limit SATA max rate to 1.5 Gbps"
SCGCQ00490725 - (Closed) - Debug Queue Implementation and Support as part of enhanced MR Diagnostic support
SCGCQ00573397 - (Closed) - Increase the support for 32 slots
SCGCQ00585068 - (Closed) - Add Critical event in FW to indicate that an INIT operation was halted due to reboot or other failure
SCGCQ00593824 - (Closed) - Update code to modify GG and VPD at powerup
SCGCQ00468085 - (Closed) - Implement throttle mechanism to prevent thermal run away
SCGCQ00472399 - (Closed) - Change hash algorithm for cache row hash from a bit mask to a modulo
SCGCQ00556564 - (Closed) - DIS feature
SCGCQ00469990 - (Closed) - Signed images for FWDownload
SCGCQ00342679 - (Port_Complete) - Don't interpret the cachecade BVD flags if the volume is created with old FW which does not support cachecade.
SCGCQ00359329 - (Port_Complete) - Code-review action item for removing and updating names for AEN dism.
SCGCQ00454419 - (Port_Complete) - Patrol Read - no progress
SCGCQ00462259 - (Port_Complete) - WB Logical disks are moving to WT after corrupting BMT1,BBT1 and reboot.
SCGCQ00462309 - (Port_Complete) - Deep Learn is not invoked in new battery, when the system is reboot before the first learn completes
SCGCQ00462327 - (Port_Complete) - Transparent Learn Cycle is rescheduled even though it is not completed
SCGCQ00469037 - (Port_Complete) - TFM error handling : Cache policy change for WB to WT if supercap is faulty
SCGCQ00469755 - (Port_Complete) - Intermittent SEP errors on iMR and MR controllers
SCGCQ00471540 - (Port_Complete) - When Cachecade LD is deleted invalid LD details is shown in the Cachecade size changed event.
SCGCQ00473330 - (Port_Complete) - Hotspare Recovery Doesn't Start after Inserting Failed Drives
SCGCQ00478032 - (Port_Complete) - FW sending wrong configuration data during boot msg pending state
SCGCQ00479443 - (Port_Complete) - Upgrading from Software RAID to 9260-8i causes Alarm to sound
SCGCQ00482660 - (Port_Complete) - ONFI_BBM Dev test build: FwTermLog does not preserve information before powerup. 
SCGCQ00483590 - (Port_Complete) - iMR TB Data loss when reconstructing from 1 drive R0 to 2 drive R1 with reboot
SCGCQ00484771 - (Port_Complete) - incorrectly uses a slot offset value to enumerate HDD.
SCGCQ00485259 - (Port_Complete) - In case of a certain OEM iMR shows R5 enabled.
SCGCQ00492432 - (Port_Complete) - MSM log warning: Controller booted in headless mode with errors
SCGCQ00495888 - (Port_Complete) - Set the Recovery mode page (WriteRetryCount and recoveryTimeLimit)
SCGCQ00498734 - (Port_Complete) - If VD is secured while reconstruction is going on does not stay secured once reconstruction is done.
SCGCQ00498742 - (Port_Complete) - SEAGATE hotspare drives remain spun up on LSI FW 12.12.0-0079
SCGCQ00498946 - (Port_Complete) - Firmware is not updating recovery timer as intended
SCGCQ00502953 - (Port_Complete) - Call DDF_discardInvalidPds only if DS3 is enabled
SCGCQ00518879 - (Port_Complete) - LSI_MR Controllers fails to set "FACTORY SETTINGS"
SCGCQ00521513 - (Port_Complete) - Controller Reset due to Fatal Error with RAID6/60 configuration
SCGCQ00521758 - (Port_Complete) - VPD output of lspci –vvxxx showing [RV] Reserved: checksum bad, 86 byte(s) reserved
SCGCQ00523958 - (Port_Complete) - Multi-stripe size in each raid level of R1,r5,r6 with SAS, DIF, 4K pinned cache offline vd import cause Montask
SCGCQ00523962 - (Port_Complete) - Remove memory module on MR controller to downgrade to iMR does not work
SCGCQ00523970 - (Port_Not_Required) - HII critical message form/Extra character "r" with configuration not supported critical message.
SCGCQ00523976 - (Port_Complete) - Fw defect in PdStateSet()
SCGCQ00524442 - (Port_Complete) - Controller Reset due to Fatal Error with RAID6/60 configuration
SCGCQ00524493 - (Port_Complete) - Correct how the SCL high and low period values are calculated for the I2C to run at 400Khz
SCGCQ00524494 - (Port_Complete) - For new spin up code get persistent devId for drives that are connected via internal back plane.
SCGCQ00526284 - (Port_Complete) - Controller Reset due to Fatal Error with RAID6/60 configuration
SCGCQ00526632 - (Port_Not_Required) - Drive security mode switching in MSM
SCGCQ00526633 - (Port_Complete) - Unable to create another Virtual Drive when pulling first drive (degrading) in partial Virtual Drive where all drives are configured
SCGCQ00549320 - (Port_Complete) - Baseboard Management Controller (BMC): STP passthru command failure
SCGCQ00552443 - (Port_Complete) - External Key management security for iMR
SCGCQ00552444 - (Port_Complete) - Re-keying a controller with External Key Management(EKM) security enabled, results in a corrupted key ID.
SCGCQ00554050 - (Port_Complete) - Performing an online firmware update or Online Controller Reset(OCR) on a controller with External Key Management(EKM) enabled, results in all secured drives marked as foreign.
SCGCQ00558051 - (Port_Complete) - MR 4K Validation : 4K VD assigned to 512K CacheCade
SCGCQ00559254 - (Port_Complete) - Re-keying in External Key Management mode followed by disabling security and enabling LKM results in a bail out while creating a Virtual Drive
SCGCQ00562800 - (Port_Complete) - VD goes offline when we start reconstruction on 32 Drive R0 VD
SCGCQ00566690 - (Port_Complete) - Raise priority of pci config trap interrupt to critical
SCGCQ00567036 - (Port_Complete) - Not seeing the correct Boot Message when the connection to the External Key Management server is down
SCGCQ00575842 - (Port_Complete) - Switching to Local Key Management Mode(LKM) after a rekey in External Key Management(EKM) rekey without rebooting results in HII saying key incorrect but Firmware says key was created.
SCGCQ00575843 - (Port_Complete) - On a controller with Local Key Management(LKM) enabled, user is asked to enter the security key to unlock and import a foreign, locked and External Key Management(EKM) enabled drive.
SCGCQ00579499 - (Port_Complete) - FwTermLog does not preserve information before powerup. 
SCGCQ00579847 - (Port_Complete) - Implement I2C Slave Address for Sideband Management
SCGCQ00580752 - (Port_Complete) - Defect Fix for VPD and inquiry callback issues in DISM
SCGCQ00580771 - (Port_Complete) - spin up tracker dequeue is not handled for case in which TUR error happens even after MAX retries
SCGCQ00588963 - (Port_Complete) - Too many unexpected sense AEN raised by CC during CME recovery on R5
SCGCQ00588964 - (Port_Complete) - Too many unexpected sense AEN raised by CC during CME recovery on R5
SCGCQ00588973 - (Port_Complete) - Fix GNU make file compilation
SCGCQ00588977 - (Port_Complete) - Routines to inject bit error in NF and ecc error in DDR for ONFI
SCGCQ00588978 - (Port_Complete) - Mismatch in LD id and target ID during set/reset boot device
SCGCQ00588979 - (Port_Complete) - Mismatch in LD id and target ID during set/reset boot device
SCGCQ00593826 - (Port_Complete) - Adding test routine for the bad block loop test for PR SCGCQ00423195
SCGCQ00595783 - (Port_Complete) - SMART poll needs to issue log sense with page control set to current/ cummulative value
SCGCQ00597425 - (Port_Complete) - FW breaks if wrong security key is entered
SCGCQ00604028 - (Port_Complete) - on breaking the multipath in loop while drives are spinnning up will result in montask
SCGCQ00604030 - (Port_Complete) - FW hangs while creating 64 VDs on the controller with SLES11 SP2 PPC64
SCGCQ00604033 - (Port_Complete) - While running reconstruction from R1 to 4 drive PRL11 with IO,FW hits to MonTask: line 1270 in file ../../raid/1078dm
SCGCQ00604041 - (Port_Complete) - Static analysis tool defect
SCGCQ00604042 - (Port_Complete) - Static Analysis Tool defects
SCGCQ00609872 - (Port_Complete) - CLI Reporting of TMM VPD
SCGCQ00610801 - (Port_Complete) - Rebuild triggered on an incompatible blocksize PD
SCGCQ00610813 - (Port_Complete) - Issue with Global Hot Spare assignment
SCGCQ00610824 - (Port_Complete) - Elapsed time of Reconstruction is incorrect
SCGCQ00610834 - (Port_Complete) - Elapsed time of Patrol Read in tty log is incorrect
SCGCQ00610846 - (Port_Complete) - "Corrected medium error" event is logged for uncorrectable mendium errors during PR
SCGCQ00612226 - (Port_Complete) - Increase margin in PCIe Rx Serdes
SCGCQ00612228 - (Port_Complete) - Increase PCIe Receiver Margin
SCGCQ00620118 - (Port_Complete) - Liberator Card loses its boot VD after many reboots
SCGCQ00635628 - (Port_Complete) - Cache policy of Virtual Drives(VD) does not change to Write Through(WT) mode even after detecting a bad supercap.
SCGCQ00638288 - (Port_Complete) - RAID configured on PD been erased with Normal or Thorough will lost after system reboot/reset
SCGCQ00646479 - (Port_Complete) - Defect fix for kenel panic with iMR Fury with Free BSD driver
SCGCQ00651117 - (Port_Complete) - Hitting montask line 1930 in file ../../bbu/onfi.c while running FP IO's on degraded VD's
SCGCQ00335860 - (Port_Complete) - Cachecade configurations could not be created.
SCGCQ00462330 - (Port_Complete) - Deep learn doesn't start when it is requested during relaxing.
SCGCQ00469041 - (Port_Complete) - Write policy changed from WT to WB when the battery/Supercap is declared as bad
SCGCQ00471509 - (Port_Not_Required) - Firmware crash seen while doing continuous sas cable pull
SCGCQ00471542 - (Port_Complete) - Invalid "mode select(Page=0a)" issued during disk initialization phase.
SCGCQ00477967 - (Port_Complete) - Defect fix for Montask observed while installing OS on JBOD
SCGCQ00478050 - (Port_Complete) - Firmware returns asc value as 0 when failing IOs with medium errors
SCGCQ00482662 - (Port_Complete) - display BMU fw version in battery design info
SCGCQ00482663 - (Port_Complete) - Break Mirror for R10 should not be allowed
SCGCQ00486553 - (Port_Complete) - Medium error correction event is not logged during CC
SCGCQ00498748 - (Port_Complete) - 9240-4i on BCM RX67Q-6S motherboard is not getting required memory resources on boot
SCGCQ00503258 - (Port_Complete) - foreign import fails if degraded VD is present in import
SCGCQ00504804 - (Port_Complete) - L2/L3 cache error on reboot
SCGCQ00514666 - (Port_Complete) - search for one wire devices prints are masked after the boot
SCGCQ00518020 - (Port_Complete) - VPD info can't be retrieved for OEM enclosure
SCGCQ00523959 - (Port_Complete) - If a BOOT Passphrase is enabled with SafeStor "MegaCli adpbios dsply a0" will display "BIOS will Stop on error" even if any other mode is set.
SCGCQ00523972 - (Port_Complete) - Profile based VD creation - [Partial RAID options blocked until system reboot]
SCGCQ00523975 - (Port_Complete) - Hard coded values should be removed in TFM module
SCGCQ00524802 - (Port_Complete) - Fix repeated prints issue
SCGCQ00559253 - (Port_Complete) - A data TLB error occurs when the External Key Management Server(EKMS) is down and drive security is changed from External Key Management(EKM) mode to Local Key Management(LKM) mode.
SCGCQ00563824 - (Port_Complete) - HII & Ctrl-R: BGI operation still running on RAID0 VD even after PI protection disabled
SCGCQ00575844 - (Port_Complete) - Getting a non informative message when trying to import a Virtual Drive after a re-key without reboot
SCGCQ00577296 - (Port_Complete) - Deep learn will not start immediately when Relative State of Charge (RSOC) of battery is equal to 95%.
SCGCQ00593485 - (Port_Complete) - Raid configuration loss after reboot - PDs in POWERSAVE
SCGCQ00600939 - (Port_Complete) - Fix the learn issue at powerup
SCGCQ00603399 - (Port_Complete) - Faulty protocol used for changing the Disk Write Cache Policy
SCGCQ00604029 - (Port_Complete) - on breaking the multipath in loop while drives are spinnning up will result in montask
SCGCQ00604031 - (Port_Complete) - FW- FW hangs while creating 64 VDs on the controller with SLES11 SP2 PPC64
SCGCQ00604038 - (Port_Complete) - Static Analysis Tool defects
SCGCQ00604039 - (Port_Complete) - Static Analysis Tool defects
SCGCQ00604074 - (Port_Complete) - Enabling DQ support bit in FW
SCGCQ00610444 - (Port_Complete) - The restore successful and unsuccessful prints to be handled properly
SCGCQ00614828 - (Port_Complete) - not enough bs found during double Dip power cycle Test
SCGCQ00615002 - (Port_Complete) - Montask in divert.c seen when injecting 64K consecutive errors on R0 VD, Patrol Read running in background.
SCGCQ00615537 - (Port_Complete) - Single image support for ONFI
SCGCQ00635323 - (Port_Complete) - Assertion failure (not enough BS found) in double DIP power cycle test case
SCGCQ00651115 - (Port_Complete) - DC observed upon performing OCR on a degraded R1 (AWB).
SCGCQ00450647 - (Port_Complete) - 9260-8i(SAS2108) hitting OOB SRAT timeout for a long time causing OOB commands to fail
SCGCQ00470568 - (Port_Complete) - modify scap energy calculation
SCGCQ00483575 - (Port_Complete) - wrong error code displayed and wrong error message for copyback command
SCGCQ00485096 - (Port_Complete) - Bad or Missing TMM boot message is changed to Critical error
SCGCQ00498752 - (Port_Complete) - 9260-16i's drive locate/fault LED header doesn't work
SCGCQ00518011 - (Port_Not_Required) - MR Controller does OCR due to Temp Buffer overflow
SCGCQ00523459 - (Port_Complete) - The Firmware does not change the Virtual Drives's from Write Through to Write Back after a battery manual learn cycle is complete
SCGCQ00554074 - (Port_Complete) - SLES 11.3 x64 Halts when Loading Kernel During Warm Reboot Stress
SCGCQ00555052 - (Port_Complete) - Initialize invalid interrupt as part of intInitialize function
SCGCQ00567037 - (Port_Complete) - Switching the security mode from External Key Management(EKM) to Local Key Management(LKM) on iMR controller will result in a corrupted controller key.
SCGCQ00595833 - (Port_Complete) - SMART poll needs to issue log sense with page control set to current/ cummulative value
SCGCQ00604043 - (Port_Complete) - Static Analysis Tool defects
SCGCQ00617625 - (Port_Complete) - Power removal of enclosure FW hits to MonTask: line 4056 in file ../../bbu/onfiBBM.c
SCGCQ00359282 - (Port_Complete) - Multiple interposer drives will not be detected by MegaRAID firmware.
SCGCQ00454415 - (Port_Complete) - Infinite retry happens on Test Unit command when HDD didn't respond to TU command during the initialization.
SCGCQ00462149 - (Port_Complete) - Secondary RAID key data page read failure 6 seen on some controllers and key vault combination
SCGCQ00478428 - (Port_Complete) - StorCLI_F showed firmware download failed but really took
SCGCQ00481856 - (Port_Complete) - Assertion failure in ../../raid/raidpci.c at line 10522
SCGCQ00484769 - (Port_Not_Required) - FW Crash when using SCSI Passthrough SCSI_READ_10(0x28) to read 512 bytes on a RAID5 Native 4K drive.
SCGCQ00492431 - (Port_Complete) - When pinned cache present VD property not changing from WB to WT.
SCGCQ00492433 - (Port_Complete) - PDs go online without VD created & App doesn't allow any VD creation on passing a wrong parameter in Spanned VD.
SCGCQ00497659 - (Port_Complete) - Customer is hitting an ECC error
SCGCQ00521514 - (Port_Complete) - Invader: Cache Memory Size of controller Information is ZERO
SCGCQ00554312 - (Port_Complete) - Incorrect variable type in MR Read/Modify/Write path
SCGCQ00598504 - (Port_Complete) - StorCLI_F showed firmware download failed but really took
SCGCQ00617620 - (Port_Complete) - cache restore failure message displayed though cache restore was successfull
SCGCQ00372236 - (Port_Complete) - System hanged after pulling out drives from a 8Raid-6 array during OCR in Debian OS
SCGCQ00454381 - (Port_Complete) - Change SES Green/Amber LED behavior for OEM ACHILLES JBOD enclosure.
SCGCQ00597426 - (Port_Complete) - FW breaks if wrong security key is entered
SCGCQ00366030 - (Port_Complete) - While executing path-failover test with an SATA-SSD drive behind an interposer, the device is marked failed.
SCGCQ00454368 - (Port_Complete) - Card Running iMR Machine Checks when Requesting Host Memory
SCGCQ00456776 - (Port_Complete) - iMR FW update caused card to FW fault state and card cannot boot to OS.
SCGCQ00479292 - (Port_Complete) - system black screen during S1 Sleep test
SCGCQ00490892 - (Port_Complete) - Firmware Crash during Controller StartUp when large number of drives are connected

BootBlock:
SCGCQ00288393 (DFCT) - iMR boot Block code intial changes
SCGCQ00322313 (DFCT) - Errbios load fails on Fury adapters
SCGCQ00337925 (DFCT) - Merged 6.0 boot block changes to 6.1
SCGCQ00313425 (CSET) - Bootblock is using NVRAM data even if NVRAM is uninitialized
SCGCQ00371801 (CSET) - Configure chip reset to link down
SCGCQ00375108 (DFCT) - Added the code to enable OCM RMW errors
SCGCQ00505902 (DFCT) - Coherency bit is disabled in SRAM TLBs

BIOS:
SCGCQ00479507 - (Closed) - Getting memory conflict during boot 
SCGCQ00455591 - (Closed) - Memory access issue when loading Ctrl R
SCGCQ00495471 - (Closed) - OOB function corrupts EBDA area used by other server function
SCGCQ00552308 - (Closed) - not allocating memory correctly when MR and iMR are in the same system
SCGCQ00493680 - (Closed) - Optimize reading IO port in INT15h path
SCGCQ00482283 - (Closed) - System reboots during IO because FW didnt receive permanent host memory from OpROM
SCGCQ00503046 - (Closed) - OpROM is displaying incorrect value for the number of INT13h device it supports
SCGCQ00559094 - (Closed) - Provide an option to limit the max number of INT 13h devices presented to system BIOS
SCGCQ00466276 - (Closed) - Check the controller status bit in the function which hooks INT15
SCGCQ00455597 - (Closed) - Allocate only two 64k
SCGCQ00454086 - (Closed) - Add boundary checking when allocating EBDA and PMM memory for BIOS post.
SCGCQ00504752 - (Port_Complete) - OpROM is displaying incorrect value for the number of INT13h device it supports
SCGCQ00460724 - (Port_Complete) - Memory access issue for Mercury when loading Ctrl R
SCGCQ00460725 - (Port_Complete) - Memory allocation: Allocate only two 64k
SCGCQ00501253 - (Port_Complete) - OOB function corrupts EBDA area used by other server function

NVDATA:
Numerous changes for specific customers

UEFI Driver:
SCGCQ00478652 - (Closed) - Block IO tests from SCT IHV test suite failed
SCGCQ00479003 - (Closed) - Disable Debug print in UEFI Driver
SCGCQ00498925 - (Closed) - Not able to boot into BIOS boot menu
SCGCQ00518791 - (Closed) - In IsValidHandle() - Free the buffer if status is not EFI success for LocateHandle
SCGCQ00493654 - (Closed) - Memory Leak issue in UEFI driver when reconnect happens
SCGCQ00483847 - (Closed) - Remove private GUID and use EFI_KMS_PROTOCOL_GUID defined in UEFI 2.3.1 spec
SCGCQ00479016 - (Port_Complete) - Disable Debug print in UEFI Driver
SCGCQ00484085 - (Port_Complete) - UEFI hang when SATA is connected
SCGCQ00484086 - (Port_Complete) - UEFI hang when SATA is connected
SCGCQ00579837 - (Port_Complete) - UEFI Driver should calculate checksum before setting bios data (MR_BIOS_DATA)
SCGCQ00468948 - (Port_Complete) - Uninstall HII CAP and Driver Health formset if platform calls Start again without calling GetHealthStatus
SCGCQ00477828 - (Port_Complete) - 9240/9260/9270 UEFI driver issue with RD640/RD440 platforms when user having 2TB or 4TB VD
SCGCQ00477705 - (Port_Complete) - 9240/9260/9270 UEFI driver issue with RD640/RD440 platforms when user having 2TB or 4TB VD
SCGCQ00484113 - (Port_Complete) - Follow UEFI Spec on interpreting In and Out Transfer Length that upper layer sends
SCGCQ00478692 - (Port_Complete) - Block IO tests from SCT IHV test suite failed
SCGCQ00484114 - (Port_Complete) - Follow UEFI Spec on interpreting In and Out Transfer Length that upper layer sends

HII:
SCGCQ00470101 - (Closed) - Allow user to edit VD size (that is free form input) as it is cumbersome to modify the size using +/-
SCGCQ00471830 - (Closed) - Save and Restore Configuration – MR
SCGCQ00556209 - (Closed) - Transition a Thunderbolt MR controller to run in iMR mode = Controller fail in HII After Memory removed
SCGCQ00556811 - (Closed) - When controller is in safe mode the PD menu displays inaccurate text and hangs when clicking a PD
SCGCQ00579816 - (Closed) - HII\EKM-LKM without reboot should show proper message
SCGCQ00452128 - (Closed) - HII cannot assign partial space less than 1 GB
SCGCQ00573871 - (Closed) - fixing code review defects (AIM version + UCM GUID + deallocation)
SCGCQ00529287 - (Closed) - Profile Based Raid1 Creation fails as invalid arguments
SCGCQ00502940 - (Closed) - Naming inconsistency in option present in Create VD and Create VD - Advanced
SCGCQ00482092 - (Closed) - condition checking is not right
SCGCQ00474402 - (Closed) - Allows user to select EKM mode when supportEKM is set to 0
SCGCQ00485401 - (Closed) - Using 84 PD encl when clicking on HW, Advanced then Enclosure Management, it completly freezes the system
SCGCQ00571353 - (Closed) - Allow user to select RAID level when controller has other VD + error handling
SCGCQ00569098 - (Closed) - Enter security key for locked drives screen, press down to get to OK, OK will show up again on right
SCGCQ00473204 - (Closed) - unable to show UF003 as well the first two forms + XML special character handling
SCGCQ00486457 - (Closed) - fixing memory leak of 128 drive enclosure implementation
SCGCQ00556839 - (Closed) - Able to select EKM even when the EKM FOD key is removed from the system.
SCGCQ00505566 - (Closed) - Drop down option to set phy linkspeed tp 12 Gbps in HII browser is not available.
SCGCQ00473186 - (Closed) - Save and Restore Configuration - MR w/ Premium Features (SED and Cachecade)
SCGCQ00501111 - (Closed) - Issues when trying to change EKM security key from change security key option.
SCGCQ00523869 - (Closed) - EKMS is down but it is still possible to select drive security in MSM and HII during creation.
SCGCQ00524969 - (Closed) - Going from LKM to EKM asks for a Current Security key Identifier and Security key.
SCGCQ00527700 - (Closed) - Update the latest API change in HEFU
SCGCQ00571359 - (Closed) - UCM Phase 1: Typo "Clear Configuaration" -> "Clear Configuration"
SCGCQ00500945 - (Closed) - EXPAND operation fails in HII for prl11
SCGCQ00494431 - (Closed) - Streamline the usage of max PD in limited configuration path (alias UCM)
SCGCQ00494214 - (Closed) - Help content for Free space in Select Drive group is inappropriate
SCGCQ00485932 - (Closed) - UCM Simple Configuration: Allow Clear Config always + Suppress Checkbox (Uf002.PDs) when VD count is >0
SCGCQ00575062 - (Closed) - added a while loop and take care of the multiple PD Groups scenario.
SCGCQ00574041 - (Closed) - AIM (Agentless Inventory Manager) Issues
SCGCQ00481284 - (Closed) - Typos in help content for profile VD for Write Policy
SCGCQ00472196 - (Closed) - Profile based VD creation path incorrectly showing protect VD/secure VD checkbox when user clicks on drive selection criteria
SCGCQ00471209 - (Closed) - config using 8PDs/16 partial VDs and all stripe sizes and HSPs does not restore
SCGCQ00487936 - (Closed) - After creating a VD with UCM tool the manual configuration PD section still shows configured PDs as UG, and duplicates
SCGCQ00495236 - (Closed) - Controller not seen in HII Browsercan after switiching from EFI WebBIOS
SCGCQ00505591 - (Closed) - Checking the Enclosure Management settings in HII causes the system to reboot.
SCGCQ00475217 - (Closed) - Request to support 128 drives wihin single enclosure
SCGCQ00468930 - (Closed) - UCM Phase 2 support
SCGCQ00571579 - (Implemented) - Create a formset with classGUID that customer has provided. 
SCGCQ00481277 - (Closed) - Request to change the help content for write policy in create VD form
SCGCQ00415456 - (Closed) - Obtain the Physical Slot number from the PCI Bridge to which the Controller is connected.
SCGCQ00557522 - (Port_Complete) - System hang observed when the "PdInfo.userDataBlockSize" is set to 0
SCGCQ00476607 - (Port_Complete) - HII cannot assign partial space less than 1 GB
SCGCQ00629813 - (Port_Complete) - RSOD during POST after enabling SecureBoot - HEFU.ROM should report exact size of .EFI image
SCGCQ00482099 - (Port_Complete) - Typos in help content for profile VD for Write Policy
SCGCQ00498521 - (Port_Complete) - HII cannot create a VD using unconfigured good drives as long as PD locate is set on the drives
SCGCQ00477863 - (Port_Complete) - Obtain the Physical Slot number from the PCI Bridge to which the Controller is connected.

Ctrl-R:
SCGCQ00485184 (DFCT) - Change Emergency Spare to NONE with enable enmergency on Smarter checked will fail with error=03
SCGCQ00487220 (DFCT) - ctrl-r dosent list all the drives to do replace drive.
SCGCQ00487602 (DFCT) - Power savings button not enabled on Ctrl-R
SCGCQ00490688 (DFCT) - ctrl-H doesn't list the drives to do replace drive while doing copyback in PD MGmt Screen
SCGCQ00490789 (DFCT) - Selecting "Manage Link Speed" in CTL+R causes Fatal Error with SAS 9343-4i
SCGCQ00493479 (ENHREQ) - Implemented the safe mode in Ctrl-R
SCGCQ00518579 (DFCT) - Unable to make R10 through Ctrl R using 4k drives
SCGCQ00593396 (DFCT) - Default (Initial) setting of VD doesn't reflect MFC's setting
SCGCQ00606717 (CSET) - /c0/pall show and Linkspeed information is not in same in Ctrl-R.
SCGCQ00601637 (DFCT) - Changes in BIOS mode (pause on error) to be in sync
SCGCQ00601691 (ENHREQ) - Need to display controller memory in Control-R
SCGCQ00568108 (DFCT) - showing "BIOS Mode" in both the pages of ctrl mgmt
SCGCQ00568688 (DFCT) - Help content is not updated with the Key stroke added
SCGCQ00573077 (DFCT) - VD Erase will be disabled in Ctrl+R when Initlization on particular VD
SCGCQ00579583 (DFCT) - Write policy is not added with writeback with BBu when MFC is set

FCode:
SCGCQ00553069 - (Closed) - PCLI(1.07.05) Sparc: Command "cli set securitykey=L
SCGCQ00471703 - (Closed) - Fcode CLI support for Invader (MR only)
SCGCQ00486355 - (Closed) - Define and use capability bit to identify the StorCLI


Installation:
=============
Use MegaCLI or StorCLI to flash the SAS controllers.  These tools can be downloaded from the support and download
section of www.lsi.com.

Command syntax:  
MegaCli -adpfwflash -f mr3108fw.rom -a0
or
StorCLI /c0 download file=mr3108fw.rom






Component:
=========
SAS MegaRAID Firmware Release for MegaRAID Controllers
Release date: 01/20/14


Version Numbers:	
===============
Current Package Details:
Firmware Package: 24.1.1-0006 (MR 6.1)
Firmware 4.210.50-3015
ROMENV 1.09
BootBlock 3.00.00.00-0009
NVDATA 3.1310.00-0062
UEFI_Driver 0x06010600
Hii 03.03.10.00
FCODE 4.14.05.00
BIOS 6.13.00.1
Ctrl-H 5.01-0005

Previous Package Details:
Firmware Package: 24.0.2-0013 (MR 6.0.1)
Firmware 4.200.20-2839
ROMENV 1.09
BootBlock 3.00.00.00-0009
NVDATA 3.1304.00-0039
UEFI_Driver 0x06000500
Hii 03.02.11.01
FCODE 4.12.05.00
BIOS 6.12.00
Ctrl-H 5.00-0007


Bug Fixes and Enhancements:
===========================
Firmware:
SCGCQ00383439 - (Closed) - fix for the defect - 4k drives display wrong value of Coerced size.
SCGCQ00573649 - (Closed) - JBOD mode drive cannot be set as Bootdrive when Only JBOD Mode drive exist in MR6.1
SCGCQ00563950 - (Closed) - Fix for Infinite retries of command for sense code 0B/47/03
SCGCQ00523831 - (Closed) - controller does not boot after Cache Offload
SCGCQ00521575 - (Resolved) - LSI BIOS POST displays F/W initialized percentage greater than 100% i.e 106%
SCGCQ00452322 - (Closed) - FW throws "MPT_LogDiscoveryErrors: SAS_TOPOLOGY_MAX_TOPO_PHYS_EXCEED" when connect 2 enclosures in multi-path
SCGCQ00448575 - (Closed) - Fix coverity defect 13424
SCGCQ00448009 - (Closed) - Defect Fix for Exception in Core 0
SCGCQ00440474 - (Closed) - MISCOMPARES FOUND DURING COPYBACK
SCGCQ00433521 - (Closed) - boards have issue in bootup after the wait time was increased in finding the ONFI flash configuration
SCGCQ00426148 - (Closed) - Fix the unhandled interrupt by minimizing the critical interrupt
SCGCQ00422673 - (Closed) - FW hit Montask with line 782, L2/L3 cache error when one drive is pulled out from enclosure
SCGCQ00421805 - (Closed) - Changes to SMARTerEnabled and SSDSMARTerEnabled are not reflected in controller properties
SCGCQ00420102 - (Closed) - fw breaks into montask on transporting ONFI module from 4i contoller
SCGCQ00419935 - (Closed) - Change IO time out value to 20 seconds for FW initiated IOs
SCGCQ00415989 - (Closed) - Modify the code to support tty dump in interrupt context
SCGCQ00413690 - (Closed) - MSM freezes until full initialization completes when configuration created
SCGCQ00349837 - (Closed) - Sequential Read performance is less on CacheCade associated LD's.
SCGCQ00567996 - (Closed) - ECC Errors in tty logs
SCGCQ00550456 - (Closed) - removing the cset SCGCQ00550153: Identifying the DDR, ONFI flash and SCap combination
SCGCQ00456094 - (Closed) - Data Corruption seen upon OCR after injecting Medium Error on Metadata of one Drive of R0 WB CCVD
SCGCQ00455015 - (Closed) - Unblock 4G DDR support for OEM controllers
SCGCQ00454330 - (Closed) - Capacitance value as 0% for Supercap FBU03 even though capacitor is fully charged
SCGCQ00451378 - (Closed) - Data corruption on Raid 6 volume while running smash raw io on 63 volume
SCGCQ00448581 - (Closed) - Coverity Defect Fix
SCGCQ00442609 - (Closed) - NVCache fails on sCapMaxESRThreshold exceeds after a battery relearn
SCGCQ00435532 - (Closed) - CC SRAM optimization using overlapped sections in SRAM
SCGCQ00433463 - (Closed) - Insertion of the boot messages and the evets for montoring the ONFI backup capacity.
SCGCQ00427452 - (Closed) - Indifference between MR.H and FW implementation for lockKeyLength
SCGCQ00427326 - (Closed) - Boot block Version is not displayed in CTRL+R
SCGCQ00421908 - (Closed) - Remove NO_RETENTION flag as it is not used
SCGCQ00418459 - (Closed) - Assertion failure observed after reconstruction over from R0 to R5
SCGCQ00408827 - (Closed) - Raise priority of pci config trap interrupt to critical
SCGCQ00396609 - (Closed) - Remove 4K toggle code to enable 4K support PR in 6.1.
SCGCQ00558428 - (Closed) - Rebuild and Consistency Check aren't processed when it is executed by CTL+R
SCGCQ00455583 - (Closed) - Memory battery problem seen while corrupting both the banks at alternative address in 8G Ptolemy.
SCGCQ00452094 - (Closed) - Small Sequential Reads and Writes are lower than TB
SCGCQ00450489 - (Closed) - replacePack bit is set to 1, still FW gives the battery(FBU03) status as optimal when apps queries the status
SCGCQ00446931 - (Closed) - Firmware Version incorrectly displayed
SCGCQ00446104 - (Closed) - MR: on doing cache offload and restore, the data loss is seen
SCGCQ00427451 - (Closed) - bootMsgPending.needsEKM bit is not set when FW needs a key
SCGCQ00423468 - (Closed) - ONFI: Reducing the onfi initialize time from 7sec to 2sec
SCGCQ00422566 - (Closed) - Foreign config import fails with pinned cache when VD is migrated from one controller to another controller
SCGCQ00415034 - (Closed) - Watchdog timer excetpion in core 1
SCGCQ00413263 - (Closed) - Online R6 VD became offline after another R5 VD was removed during IO with a CC2.0 VD
SCGCQ00412599 - (Closed) - Configuring SBR for operating DDR at 800MHz does not work
SCGCQ00412591 - (Closed) - Removal of CacheCade VD causes Hang during foreign import reports Command block Data structure issue
SCGCQ00408922 - (Closed) - Enable watchdog timer
SCGCQ00396711 - (Closed) - FirmWare hitting Montask with PL fault(0000d115) while trying to create R5 vd on 3drives powersavemode
SCGCQ00396324 - (Closed) - Defect fix for Montask ../../raid/mem.c at line 280
SCGCQ00442641 - (Closed) - Defect fix for VD rebuild doesnot kickin and goes to foreign state after reboot
SCGCQ00435715 - (Closed) - Loss or corruption of meta data information declares nvcache as bad and move from WB to WT
SCGCQ00417354 - (Closed) - Firmware broke @ 639 in file ../../raid/routines for reading the puctured LBAs due to Reference Tag in PI enabled LDs.
SCGCQ00415844 - (Closed) - Defect Fix for Montask Observed during cable pull/push
SCGCQ00414361 - (Closed) - Inverted check for flush completion in L3CacheFlushAll
SCGCQ00451974 - (Closed) - Unit attention for a FP IO is not handled
SCGCQ00447956 - (Closed) - Recon progress shows improper estimated time left .
SCGCQ00436260 - (Closed) - To resolve Failure of skinny compilation
SCGCQ00415677 - (Closed) - Two different VDs getting same target IDs on MR controller and FW hangs
SCGCQ00391804 - (Closed) - Firmware crash (MonTask: line 416 in file ../../dm/mpt2/mptrec.c) on reboot after installing ESX4.1U3 on VD
SCGCQ00390068 - (Closed) - ONFI error hit when 4K sector PDs were used in CacheCade testing.
SCGCQ00411644 - (Closed) - PD state changes from JBOD to Unconfigured Good across reboots for certain PDs
SCGCQ00392627 - (Closed) - verification of error cases handling issues
SCGCQ00434812 - (Closed) - Rebuild starts automatically on drive with foreign config after reboot
SCGCQ00436221 - (Closed) - For certain OS versions, returning ASCQ=0 for TUR for an offline VD casues the storage stack to keep issuing SSU and TUR commands
SCGCQ00441021 - (Closed) - Term log capture to include the RAID-Key phase of the boot
SCGCQ00567340 - (Closed) - Add event in FW to indicate that an INIT operation was halted due to reboot or other failure 
SCGCQ00394433 - (Closed) - Invader Boot Volumes
SCGCQ00447612 - (Closed) - Cobra EDFB write performance not scaling to 6400MB/s for IOs > 32k
SCGCQ00434810 - (Closed) - Enable OCR by default in all pre-GCA builds for OEM 
SCGCQ00395865 - (Port_Complete) - Transition of defect id SCGCQ00393644 from MR_FW_SAS3_6.0 to MR_FW_SAS3_6.1
SCGCQ00413395 - (Port_Complete) - Sequential Read performance is less on CacheCade associated LD's.
SCGCQ00420689 - (Port_Complete) - BBU Charging gets disabled when Transparent Relearn fails to start due to low capacity
SCGCQ00420710 - (Port_Complete) - Implementing code review comments
SCGCQ00420713 - (Port_Complete) - Ability to power off and on individual HDD
SCGCQ00420732 - (Port_Complete) - Implementing code review comments for code collaborator review #14994
SCGCQ00420739 - (Port_Complete) - Firmware is sending totalElapsedSecs value as 0 for LD and PD progresses
SCGCQ00420745 - (Port_Complete) - 5.7 ‘Static Code Analysis Tool’ changes
SCGCQ00420749 - (Port_Complete) - MonTask: line 281 in file ../../raid/mem.c if running megacli AdpDiag
SCGCQ00420767 - (Port_Complete) - ‘Static Code Analysis Tool’ warnings 10071, 10100, 10162, 10174, 10288, 10332, 10361, 10363, 10503
SCGCQ00433405 - (Port_Complete) - Auto Foreign import fails when controller is booted with pinned cache.
SCGCQ00434144 - (Port_Complete) - Alarm continues to sound after copy-back is done, across reboot, from an unconfigured good drive that is used as an emergency spare.
SCGCQ00434149 - (Port_Complete) - Change RAID controller FW bad battery warning message that comes up during POST.
SCGCQ00434151 - (Port_Complete) - Setting the ASO key with storcli 1.02.08 (MegaCli 8.07.06) fails with an error code 3 on Windows or Linux if the MB BIOS PCI
SCGCQ00434185 - (Port_Complete) - Application could not make a JBOD bootable without a VD present
SCGCQ00435943 - (Port_Complete) - user is able to associate a DIF enabled VD to Cachecade
SCGCQ00449870 - (Port_Complete) - static variable used in PD Progress and LD Progress function which may affect multiple progresses running at the same time.
SCGCQ00549466 - (Port_Complete) - Cache Memory Size of controller Information is ZERO
SCGCQ00549468 - (Port_Complete) - Controller Reset due to Fatal Error with RAID6/60 configuration
SCGCQ00550153 - (Port_Complete) - Identifying the DDR, ONFI flash and SCap combination
SCGCQ00550337 - (Port_Complete) - Baseboard Management Controller (BMC): STP passthru command failure
SCGCQ00556151 - (Port_Complete) - SLES 11.3 x64 Halts when Loading Kernel During Warm Reboot Stress
SCGCQ00558049 - (Port_Complete) - MR 4K Validation : 4K VD assigned to 512K CacheCade
SCGCQ00562722 - (Port_Not_Required) - MR_6.2 Storlib : SMPpassthru is not happening through storlib.
SCGCQ00562793 - (Port_Complete) - Unable to create another Virtual Drive when pulling first drive (degrading) in partial Virtual Drive where all drives are configured
SCGCQ00571048 - (Port_Complete) - Elapsed Seconds displayed in firmware logs for background operations progress is improper
SCGCQ00384606 - (Port_Complete) - Assertion failure in ../../raid/raidpci.c at line 10011 , while running IO with medium errors on arrays.
SCGCQ00420692 - (Port_Complete) - The reliability and error recovery of the SuperCap firmware was improved.
SCGCQ00420747 - (Port_Complete) - ‘Static Code Analysis Tool’ code changes
SCGCQ00420750 - (Port_Complete) - ‘Static Code Analysis Tool’ Fixes: 10463, 10513, 10591, 10592
SCGCQ00420760 - (Port_Complete) - Delete VD while PR still in progress cause debugger to loop. Reboot the system, debugger still loops
SCGCQ00423453 - (Port_Complete) - Adding check to prevent WT->WB property update for SSC VD when enableSSCWB is 0
SCGCQ00434184 - (Port_Not_Required) - Skinny firmware does not progress background operations with certain systems when using WebBIOS in legacy mode
SCGCQ00454467 - (Port_Complete) - Stressing test on degrade raid with UNC drives or rebuilding on UNC drives will cause firmware hang
SCGCQ00498743 - (Port_Complete) - Don't interpret the cachecade BVD flags if the volume is created with old FW which does not support cachecade.
SCGCQ00518877 - (Port_Complete) - LSI_MR Controllers fails to set "FACTORY SETTINGS"
SCGCQ00562792 - (Port_Complete) - Incorrect variable type in MR Read/Modify/Write path
SCGCQ00394788 - (Port_Complete) - Firmware blocked firmware download to interposer
SCGCQ00420686 - (Port_Complete) - Firmware returns invalid data in OOB packet
SCGCQ00420716 - (Port_Complete) - T-bolt firmware : ECC memory error boot message and event log enhancement.
SCGCQ00420757 - (Port_Not_Required) - "Question value mismatch with Option Value" message in HII's Controller Management when in Safe Mode with pin cache
SCGCQ00420764 - (Port_Complete) - Grammatical spacing error in bios message at POST
SCGCQ00420771 - (Port_Complete) - HII /When user has a critical message and the conrtoller is in Safe Mode, going into CTRL mang will result an error msg
SCGCQ00433450 - (Port_Complete) - FW halts when you have pinned cahce and remove VD form the configuration.
SCGCQ00452019 - (Port_Complete) - Virtual drive configurations go missing during firmware upgrade from 5.3 to 5.7
SCGCQ00454364 - (Port_Complete) - OEM facing with incorrect SAS HDD's indication, MSM shows 2X drives connected
SCGCQ00458466 - (Port_Complete) - ONFI Coverity defects : 13414,13415,13416,13417,13418,13419,13420,13421,13422
SCGCQ00558941 - (Port_Complete) - Running out of free entries in task list due to recursive addition of tasks
SCGCQ00420725 - (Port_Complete) - 4K sector support - iMR, analyze all remaining hard-coded instances of "512"
SCGCQ00434153 - (Port_Complete) - Disable Band Gap feature for select customers
SCGCQ00441739 - (Port_Complete) - Allow Type2 DIF drive as JBOD drives
SCGCQ00450979 - (Port_Complete) - Incase of HW failure move to WT mode and also error case handling of flash tables
SCGCQ00420724 - (Port_Complete) - Port latency outlier fixes to FW (from legacy PR137246)
SCGCQ00420753 - (Port_Complete) - Fix code collaborator coding standard related comments for Review #18196.
SCGCQ00432857 - (Port_Complete) - Saved Release Note DataSLIB returning bad data as good data after host reboots
SCGCQ00417871 - (Port_Complete) - montask hit at the line "Fatal firmware error: Line 1057 in ../../dm/src/dm.c while running copyback
SCGCQ00420744 - (Port_Complete) - Provide Fastpath as a standard offering for TB based controllers
SCGCQ00434156 - (Port_Not_Required) - OEM- StorCli should not allow turning on JBOD in MR mode
SCGCQ00436903 - (Port_Complete) - Minimum Capacity needed for relearn is incorrect in 2208 MR FW

BIOS:
SCGCQ00455591 - (Closed) - Memory access issue for OEM when loading Ctrl R
SCGCQ00559094 - (Closed) - Provide an option to limit the max number of INT 13h devices presented to system BIOS
SCGCQ00455597 - (Closed) - Memory allocation: Allocate only two 64k
SCGCQ00504752 - (Port_Complete) - OpROM is displaying incorrect value for the number of INT13h device it supports
SCGCQ00501253 - (Port_Complete) - OOB function corrupts EBDA area used by other server function

NVDATA:
Numerous changes for specific customers

UEFI Driver:
SCGCQ00478652 - (Closed) - Block IO tests from SCT IHV test suite failed
SCGCQ00435384 - (Closed) - UEFI System hang if controller FW is in fault state
SCGCQ00404216 - (Closed) - Add 3008 device ID for iMR product.
SCGCQ00392836 - (Closed) - LSI to Support Remote Key Management
SCGCQ00436609 - (Closed) - add PnPID's for 3004 and 3108
SCGCQ00479016 - (Port_Complete) - Disable Debug print in UEFI Driver
SCGCQ00484085 - (Port_Complete) - platfrom has UEFI hang when SATA is connected
SCGCQ00477705 - (Port_Complete) - 9240/9260/9270 UEFI driver issue with platforms when user having 2TB or 4TB VD
SCGCQ00484113 - (Port_Complete) - Follow UEFI Spec on interpreting In and Out Transfer Length that upper layer sends

HII:
SCGCQ00415826 (DFCT) - UCM Driver - unable to create an 8PD R5
SCGCQ00420950 (DFCT) - empty warning prompt is given when creating a CacheCade VD with forced writeback option
SCGCQ00421615 (CSET) - BBU information and propererties are not displayed in HII browser 
SCGCQ00421618 (CSET) - HII Manage Foreign Configuration menu is not available when a foreign lockeddrive is present in the configuration.
SCGCQ00423622 (DFCT) - Tool to generate VFR
SCGCQ00423659 (DFCT) - UCM - Virtual Drive Configuration summary does not report the "Interface Type"
SCGCQ00431622 (DFCT) - Navigation issue from Enable Drive Security form
SCGCQ00422725 (CSET) - HII doesn not allow user to use the remain free capacity to configure additional VD for R50/R10.
SCGCQ00427518 (CSET) - HII failed to allow user to use the remains free capacity for R1 VD with 2 plus TB capacity.
SCGCQ00431231 (CSET) - Hii enter black screen/timeout when user switching between fields/form sub_form to create R10 VD
SCGCQ00432915 (CSET) - Hii failed to report warning that inappropriate drives are picked to config R10 VD.
SCGCQ00419159 (ENHREQ) - New Field "package version" in Controller Management
SCGCQ00441850 (DFCT) - Profile based configuration help issues
SCGCQ00443864 (DFCT) - When creating an invalid argument in HII during VD creation and after correction, save is grayed out
SCGCQ00437500 (CSET) - Hii failed to report error warning when config 2pds R10 with different drive capacity.
SCGCQ00452128 (DFCT) - HII cannot assign partial space less than 1 GB
SCGCQ00472196 (DFCT) - Profile based VD creation path incorrectly showing protect VD/secure VD checkbox when user clicks on drive selection criteria
SCGCQ00452128 (DFCT) - HII cannot assign partial space less than 1 GB
SCGCQ00477863 (CSET) - Obtain the Physical Slot number from the PCI Bridge to which the Controller is connected.
SCGCQ00482099 (CSET) - Typos in help content for profile VD for Write Policy

Ctrl-H:
SCGCQ00413334 (DFCT) - Ctrl+R- Shows 'Power Save Mode for Configured drives' as 'Enabled' for iMR Fury controller
SCGCQ00419980 (DFCT) - CtrlR shows option to create VDs even after configuring 16VDs in one DG.
SCGCQ00436692 (ENHREQ) - Implemented the old PR LSIP200082262 with this ER in Ctrl-H
SCGCQ00442610 (DFCT) - Firmware crashed @Line 244 in ../../raid/1078int.c for entering into CTRL-R with Pinned cache in R60 and R6.
SCGCQ00461680 (DFCT) - ctrlR display "cache offload" as a premium feature at the place of "safe secure" feature.
SCGCQ00461965 (DFCT) - Unable to silence the alarm
SCGCQ00468676 (DFCT) - Aligning with FW for strip calculation for 4K drives
SCGCQ00461544 (CSET) - Unable to Activate the Premium feature with PFK in Ctrl+R
SCGCQ00472563 (DFCT) - not able to create r0 WB cachecade VD in ctrl-R
SCGCQ00497771 (CSET) - Selecting "Manage Link Speed" in CTL+R causes Fatal Error with SAS 9343-4i
SCGCQ00497772 (CSET) - Power savings button not enabled on Ctrl-R
SCGCQ00558344 (DFCT) - Boot error handling settings are not consistent for HII and CTL-R
SCGCQ00558359 (ENHREQ) - Added a shortcut Ctrl+S which saves the changes and refreshes the page.  
SCGCQ00565105 (ENHREQ) - Implemented to list all 4 BIOS modes


Installation:
=============
Use MegaCLI or StorCLI to flash the SAS controllers.  These tools can be downloaded from the support and download
section of www.lsi.com.

Command syntax:  
MegaCli -adpfwflash -f mr3108fw.rom -a0
or
StorCLI /c0 download file=mr3108fw.rom





Component:
=========
SAS MegaRAID Firmware Release for MegaRAID Controllers
Release date: 11/20/13


Version Numbers:	
===============
Current Package Details:
Firmware Package: 24.0.2-0013 (MR 6.0.1)
Firmware 4.200.20-2839
ROMENV 1.09
BootBlock 3.00.00.00-0009
NVDATA 3.1304.00-0039
UEFI_Driver 0x06000500
Hii 03.02.11.01
FCODE 4.12.05.00
BIOS 6.12.00
Ctrl-H 5.00-0007


Bug Fixes and Enhancements:
===========================
Initial release for 9361-8i and 9361-4i controllers


Installation:
=============
Use MegaCLI or StorCLI to flash the SAS controllers.  These tools can be downloaded from the support and download
section of www.lsi.com.

Command syntax:  
MegaCli -adpfwflash -f mr3108fw.rom -a0
or
StorCLI /c0 download file=mr3108fw.rom